<map id="StdDriver/inc/i2s.h" name="StdDriver/inc/i2s.h">
<area shape="rect" id="node1" title=" " alt="" coords="3701,5,3828,32"/>
<area shape="rect" id="node2" href="$da/d08/_n_u_c472__442_8h.html" title="NUC472/NUC442 peripheral access layer header file. This file contains all the peripheral register&#39;s d..." alt="" coords="3671,80,3858,121"/>
<area shape="rect" id="node3" href="$d6/d83/system___n_u_c472__442_8c.html" title="NUC472/NUC442 system clock init code and assert handler." alt="" coords="5,169,241,211"/>
<area shape="rect" id="node4" href="$d8/de4/sclib_8h.html" title="Smartcard library header file." alt="" coords="266,169,410,211"/>
<area shape="rect" id="node5" href="$d8/d29/ps2_8h.html" title="NUC472/NUC442 PS2 Driver Header File." alt="" coords="434,177,565,203"/>
<area shape="rect" id="node6" href="$d8/db0/ps2_8c.html" title=" " alt="" coords="484,259,616,285"/>
<area shape="rect" id="node7" href="$d3/df1/acmp_8c.html" title="NUC472/NUC442 Analog Comparator(ACMP) driver source file." alt="" coords="640,177,783,203"/>
<area shape="rect" id="node8" href="$de/d01/adc_8c.html" title="NUC472/NUC442 ADC driver source file." alt="" coords="807,177,939,203"/>
<area shape="rect" id="node9" href="$d0/dd7/can_8c.html" title="NUC472/NUC442 CAN driver source file." alt="" coords="963,177,1095,203"/>
<area shape="rect" id="node10" href="$da/d9b/cap_8c.html" title="NUC472/NUC442 CAP driver source file." alt="" coords="1119,177,1251,203"/>
<area shape="rect" id="node11" href="$de/da0/clk_8c.html" title="NUC472/NUC442 CLK driver source file." alt="" coords="1275,177,1403,203"/>
<area shape="rect" id="node12" href="$d8/d13/crc_8c.html" title="NUC472/NUC442 CRC driver source file." alt="" coords="1428,177,1557,203"/>
<area shape="rect" id="node13" href="$df/dee/crypto_8c.html" title="Cryptographic Accelerator driver source file." alt="" coords="1582,177,1729,203"/>
<area shape="rect" id="node14" href="$d2/d01/eadc_8c.html" title="NUC472/NUC442 EADC driver source file." alt="" coords="1753,177,1891,203"/>
<area shape="rect" id="node15" href="$d1/d7e/ebi_8c.html" title="NUC472/NUC442 EBI driver source file." alt="" coords="1915,177,2043,203"/>
<area shape="rect" id="node16" href="$dc/def/emac_8c.html" title="NUC472/NUC442 EMAC driver source file." alt="" coords="2068,177,2211,203"/>
<area shape="rect" id="node17" href="$de/d46/epwm_8c.html" title="NUC472/NUC442 EPWM driver source file." alt="" coords="2235,177,2380,203"/>
<area shape="rect" id="node18" href="$d0/dbc/fmc_8c.html" title="NUC472/NUC442 FMC driver source file." alt="" coords="2404,177,2536,203"/>
<area shape="rect" id="node19" href="$d8/da0/gpio_8c.html" title="NUC472/NUC442 GPIO driver source file." alt="" coords="2560,177,2695,203"/>
<area shape="rect" id="node20" href="$d9/dcb/i2c_8c.html" title="NUC472/NUC442 I2C driver source file." alt="" coords="2719,177,2847,203"/>
<area shape="rect" id="node21" href="$d8/d6d/i2s_8c.html" title=" " alt="" coords="2871,177,2999,203"/>
<area shape="rect" id="node22" href="$d2/d14/pdma_8c.html" title="NUC472/NUC442 PDMA driver source file." alt="" coords="3024,177,3167,203"/>
<area shape="rect" id="node23" href="$de/d5c/pwm_8c.html" title="NUC472/NUC442 PWM driver source file." alt="" coords="3191,177,3330,203"/>
<area shape="rect" id="node24" href="$d3/d3d/retarget_8c.html" title="NUC472 Series Debug Port and Semihost Setting Source File." alt="" coords="3354,177,3509,203"/>
<area shape="rect" id="node25" href="$dd/d5b/retarget__isp_8c.html" title=" " alt="" coords="3533,169,3677,211"/>
<area shape="rect" id="node26" href="$d4/dcc/rtc_8c.html" title="NUC472/NUC442 RTC driver source file." alt="" coords="3701,177,3828,203"/>
<area shape="rect" id="node27" href="$df/d60/sc_8c.html" title="NUC472/NUC442 Smartcard(SC) driver source file." alt="" coords="3853,177,3978,203"/>
<area shape="rect" id="node28" href="$df/d4a/scuart_8c.html" title="NUC472/NUC442 Smartcard UART mode (SCUART) driver source file." alt="" coords="4002,177,4149,203"/>
<area shape="rect" id="node29" href="$df/d7c/sd_8c.html" title="NUC472/NUC442 SD driver source file." alt="" coords="4173,177,4298,203"/>
<area shape="rect" id="node30" href="$da/d00/spi_8c.html" title="NUC472/NUC442 SPI driver source file." alt="" coords="4322,177,4450,203"/>
<area shape="rect" id="node31" href="$d8/d91/sys_8c.html" title="NUC472/NUC442 SYS driver source file." alt="" coords="4475,177,4607,203"/>
<area shape="rect" id="node32" href="$df/d41/timer_8c.html" title="NUC472/NUC442 TIMER driver source file." alt="" coords="4631,177,4771,203"/>
<area shape="rect" id="node33" href="$d1/d87/uart_8c.html" title="NUC472/NUC442 UART driver source file." alt="" coords="4795,177,4929,203"/>
<area shape="rect" id="node34" href="$dc/dd9/usbd_8c.html" title="NUC472/NUC442 USBD driver source file." alt="" coords="4953,177,5091,203"/>
<area shape="rect" id="node35" href="$db/d1a/wdt_8c.html" title="NUC472/NUC442 WDT driver source file." alt="" coords="5115,177,5246,203"/>
<area shape="rect" id="node36" href="$d9/d90/wwdt_8c.html" title="NUC472/NUC442 WWDT driver source file." alt="" coords="5271,177,5411,203"/>
<area shape="rect" id="node37" href="$da/dca/uac__core_8c.html" title=" " alt="" coords="5435,169,5670,211"/>
<area shape="rect" id="node38" href="$da/dd9/uac__driver_8c.html" title="NUC472/NUC442 MCU USB Host Audio Class driver." alt="" coords="5694,169,5929,211"/>
<area shape="rect" id="node39" href="$dc/dea/uac__parser_8c.html" title="NUC472/NUC442 MCU USB Host Audio Class driver." alt="" coords="5953,169,6187,211"/>
<area shape="rect" id="node40" href="$de/d48/usbh__core_8c.html" title="NUC472/NUC442 MCU USB Host Library core." alt="" coords="6211,169,6390,211"/>
<area shape="rect" id="node41" href="$da/df8/usbh__debug_8c.html" title="NUC472/NUC442 MCU USB Host library." alt="" coords="6414,169,6593,211"/>
<area shape="rect" id="node42" href="$db/dee/usbh__hub_8c.html" title="NUC472/NUC442 MCU USB Host Library Hub class driver." alt="" coords="6617,169,6795,211"/>
<area shape="rect" id="node43" href="$d2/d1c/usbh__ohci_8c.html" title="NUC472/NUC442 MCU USB Host OHCI driver." alt="" coords="6819,169,6998,211"/>
<area shape="rect" id="node44" href="$d5/d7e/usbh__support_8c.html" title=" " alt="" coords="7022,169,7201,211"/>
<area shape="rect" id="node45" href="$d0/d8a/hid__core_8c.html" title="NUC472/NUC442 MCU USB Host HID library core." alt="" coords="7225,169,7395,211"/>
<area shape="rect" id="node46" href="$d3/d98/hid__driver_8c.html" title="NUC472/NUC442 MCU USB Host HID driver." alt="" coords="7419,169,7590,211"/>
<area shape="rect" id="node47" href="$d8/d4b/lw__umass_8c.html" title="Light&#45;weight USB mass storage class driver." alt="" coords="7615,169,7787,211"/>
<area shape="rect" id="node48" href="$d8/d25/lw__usbh_8c.html" title="Light&#45;Weight USB Host driver." alt="" coords="7811,169,7983,211"/>
<area shape="rect" id="node49" href="$d0/d4c/_umas_debug_8c.html" title="NUC472/NUC442 MCU USB Host Mass Storage Library." alt="" coords="8007,169,8215,211"/>
<area shape="rect" id="node50" href="$d8/d9e/_umas_driver_8c.html" title="NUC472/NUC442 MCU USB Host Mass Storage Library." alt="" coords="8239,169,8447,211"/>
</map>
