| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Modules | Macros
ADC Exported Constants
NUC472/NUC442 Device Driver » ADC Driver
Collaboration diagram for ADC Exported Constants:

## Modules
| ADC Exported Functions

## Macros
#define | ADC_CH_0_MASK
#define | ADC_CH_1_MASK
#define | ADC_CH_2_MASK
#define | ADC_CH_3_MASK
#define | ADC_CH_4_MASK
#define | ADC_CH_5_MASK
#define | ADC_CH_6_MASK
#define | ADC_CH_7_MASK
#define | ADC_CH_8_MASK
#define | ADC_CH_9_MASK
#define | ADC_CH_10_MASK
#define | ADC_CH_11_MASK
#define | ADC_CH_BG_MASK
#define | ADC_CH_TS_MASK
#define | ADC_CMP_LESS_THAN
#define | ADC_CMP_GREATER_OR_EQUAL_TO
#define | ADC_TRIGGER_BY_EXT_PIN
#define | ADC_TRIGGER_BY_PWM
#define | ADC_LOW_LEVEL_TRIGGER
#define | ADC_HIGH_LEVEL_TRIGGER
#define | ADC_FALLING_EDGE_TRIGGER
#define | ADC_RISING_EDGE_TRIGGER
#define | ADC_ADF_INT
#define | ADC_CMP0_INT
#define | ADC_CMP1_INT
#define | ADC_INPUT_MODE_SINGLE_END
#define | ADC_INPUT_MODE_DIFFERENTIAL
#define | ADC_OPERATION_MODE_SINGLE
#define | ADC_OPERATION_MODE_SINGLE_CYCLE
#define | ADC_OPERATION_MODE_CONTINUOUS
#define | ADC_DMODE_OUT_FORMAT_UNSIGNED
#define | ADC_DMODE_OUT_FORMAT_2COMPLEMENT

## Detailed Description

## Macro Definition Documentation

## ◆ ADC_ADF_INT

#define ADC_ADF_INT

ADC convert complete interrupt

Definition at line 55 of file adc.h.

## ◆ ADC_CH_0_MASK

#define ADC_CH_0_MASK

ADC channel 0 mask

Definition at line 33 of file adc.h.

## ◆ ADC_CH_10_MASK

#define ADC_CH_10_MASK

ADC channel 10 mask

Definition at line 43 of file adc.h.

## ◆ ADC_CH_11_MASK

#define ADC_CH_11_MASK

ADC channel 11 mask

Definition at line 44 of file adc.h.

## ◆ ADC_CH_1_MASK

#define ADC_CH_1_MASK

ADC channel 1 mask

Definition at line 34 of file adc.h.

## ◆ ADC_CH_2_MASK

#define ADC_CH_2_MASK

ADC channel 2 mask

Definition at line 35 of file adc.h.

## ◆ ADC_CH_3_MASK

#define ADC_CH_3_MASK

ADC channel 3 mask

Definition at line 36 of file adc.h.

## ◆ ADC_CH_4_MASK

#define ADC_CH_4_MASK

ADC channel 4 mask

Definition at line 37 of file adc.h.

## ◆ ADC_CH_5_MASK

#define ADC_CH_5_MASK

ADC channel 5 mask

Definition at line 38 of file adc.h.

## ◆ ADC_CH_6_MASK

#define ADC_CH_6_MASK

ADC channel 6 mask

Definition at line 39 of file adc.h.

## ◆ ADC_CH_7_MASK

#define ADC_CH_7_MASK

ADC channel 7 mask

Definition at line 40 of file adc.h.

## ◆ ADC_CH_8_MASK

#define ADC_CH_8_MASK

ADC channel 8 mask

Definition at line 41 of file adc.h.

## ◆ ADC_CH_9_MASK

#define ADC_CH_9_MASK

ADC channel 9 mask

Definition at line 42 of file adc.h.

## ◆ ADC_CH_BG_MASK

#define ADC_CH_BG_MASK

ADC channel 12 (band-gap ) mask

Definition at line 45 of file adc.h.

## ◆ ADC_CH_TS_MASK

#define ADC_CH_TS_MASK

ADC channel 13 (temperature sensor) mask

Definition at line 46 of file adc.h.

## ◆ ADC_CMP0_INT

#define ADC_CMP0_INT

ADC comparator 0 interrupt

Definition at line 56 of file adc.h.

## ◆ ADC_CMP1_INT

#define ADC_CMP1_INT

ADC comparator 1 interrupt

Definition at line 57 of file adc.h.

## ◆ ADC_CMP_GREATER_OR_EQUAL_TO

#define ADC_CMP_GREATER_OR_EQUAL_TO

ADC compare condition greater or equal to

Definition at line 48 of file adc.h.

## ◆ ADC_CMP_LESS_THAN

#define ADC_CMP_LESS_THAN

ADC compare condition less than

Definition at line 47 of file adc.h.

## ◆ ADC_DMODE_OUT_FORMAT_2COMPLEMENT

#define ADC_DMODE_OUT_FORMAT_2COMPLEMENT

ADC differential mode output format with 2's complement

Definition at line 64 of file adc.h.

## ◆ ADC_DMODE_OUT_FORMAT_UNSIGNED

#define ADC_DMODE_OUT_FORMAT_UNSIGNED

ADC differential mode output format with unsigned

Definition at line 63 of file adc.h.

## ◆ ADC_FALLING_EDGE_TRIGGER

#define ADC_FALLING_EDGE_TRIGGER

External pin falling edge trigger ADC

Definition at line 53 of file adc.h.

## ◆ ADC_HIGH_LEVEL_TRIGGER

#define ADC_HIGH_LEVEL_TRIGGER

External pin high level trigger ADC

Definition at line 52 of file adc.h.

## ◆ ADC_INPUT_MODE_DIFFERENTIAL

#define ADC_INPUT_MODE_DIFFERENTIAL

ADC input mode set to differential

Definition at line 59 of file adc.h.

## ◆ ADC_INPUT_MODE_SINGLE_END

#define ADC_INPUT_MODE_SINGLE_END

ADC input mode set to single end

Definition at line 58 of file adc.h.

## ◆ ADC_LOW_LEVEL_TRIGGER

#define ADC_LOW_LEVEL_TRIGGER

External pin low level trigger ADC

Definition at line 51 of file adc.h.

## ◆ ADC_OPERATION_MODE_CONTINUOUS

#define ADC_OPERATION_MODE_CONTINUOUS

ADC operation mode set to continuous scan

Definition at line 62 of file adc.h.

## ◆ ADC_OPERATION_MODE_SINGLE

#define ADC_OPERATION_MODE_SINGLE

ADC operation mode set to single conversion

Definition at line 60 of file adc.h.

## ◆ ADC_OPERATION_MODE_SINGLE_CYCLE

#define ADC_OPERATION_MODE_SINGLE_CYCLE

ADC operation mode set to single cycle scan

Definition at line 61 of file adc.h.

## ◆ ADC_RISING_EDGE_TRIGGER

#define ADC_RISING_EDGE_TRIGGER

External pin rising edge trigger ADC

Definition at line 54 of file adc.h.

## ◆ ADC_TRIGGER_BY_EXT_PIN

#define ADC_TRIGGER_BY_EXT_PIN

ADC trigger by STADC pin

Definition at line 49 of file adc.h.

## ◆ ADC_TRIGGER_BY_PWM

#define ADC_TRIGGER_BY_PWM

ADC trigger by PWM events

Definition at line 50 of file adc.h.