| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Macros | Functions
pwm.h File Reference

NUC472/NUC442 PWM driver header file. More...

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Macros
#define | PWM_CHANNEL_NUM
#define | PWM_CH0
#define | PWM_CH1
#define | PWM_CH2
#define | PWM_CH3
#define | PWM_CH4
#define | PWM_CH5
#define | PWM_CH_0_MASK
#define | PWM_CH_1_MASK
#define | PWM_CH_2_MASK
#define | PWM_CH_3_MASK
#define | PWM_CH_4_MASK
#define | PWM_CH_5_MASK
#define | PWM_CLK_DIV_1
#define | PWM_CLK_DIV_2
#define | PWM_CLK_DIV_4
#define | PWM_CLK_DIV_8
#define | PWM_CLK_DIV_16
#define | PWM_EDGE_ALIGNED
#define | PWM_CENTER_ALIGNED
#define | PWM_TRIGGER_ADC_RISING_EDGE_POINT
#define | PWM_TRIGGER_ADC_FALLING_EDGE_POINT
#define | PWM_TRIGGER_ADC_CENTER_POINT
#define | PWM_TRIGGER_ADC_PERIOD_POINT
#define | PWM_BRK0_BKP0
#define | PWM_BRK0_CPO0
#define | PWM_BRK0_CPO1
#define | PWM_BRK0_CPO2
#define | PWM_BRK1_LVDBK
#define | PWM_BK1SEL_BKP1
#define | PWM_BK1SEL_CPO0
#define | PWM_BK1SEL_CPO1
#define | PWM_PERIOD_INT_UNDERFLOW
#define | PWM_PERIOD_INT_MATCH_CNR
#define | PWM_DUTY_INT_MATCH_CMR_DN
#define | PWM_DUTY_INT_MATCH_CMR_UP
#define | PWM_FALLING_LATCH_INT_ENABLE
#define | PWM_RISING_LATCH_INT_ENABLE
#define | PWM_RISING_FALLING_LATCH_INT_ENABLE
#define | PWM_FALLING_LATCH_INT_FLAG
#define | PWM_RISING_LATCH_INT_FLAG
#define | PWM_RISING_FALLING_LATCH_INT_FLAG
#define | PWM_TIMEOUT_ERR
#define | PWM_ENABLE_COMPLEMENTARY_MODE(pwm)
| This macro enable complementary mode. More...
#define | PWM_DISABLE_COMPLEMENTARY_MODE(pwm)
| This macro disable complementary mode, and enable independent mode. More...
#define | PWM_ENABLE_GROUP_MODE(pwm)
| This macro enable group mode. More...
#define | PWM_DISABLE_GROUP_MODE(pwm)
| This macro disable group mode. More...
#define | PWM_ENABLE_SYNC_MODE(pwm)
| This macro enable synchronous mode. More...
#define | PWM_DISABLE_SYNC_MODE(pwm)
| This macro disable synchronous mode, and enable independent mode. More...
#define | PWM_ENABLE_OUTPUT_INVERTER(pwm, u32ChannelMask)
| This macro enable output inverter of specified channel(s) More...
#define | PWM_GET_CAPTURE_RISING_DATA(pwm, u32ChannelNum)
| This macro get captured rising data. More...
#define | PWM_GET_CAPTURE_FALLING_DATA(pwm, u32ChannelNum)
| This macro get captured falling data. More...
#define | PWM_MASK_OUTPUT(pwm, u32ChannelMask, u32LevelMask)
| This macro mask output output logic to high or low. More...
#define | PWM_SET_PRESCALER(pwm, u32ChannelNum, u32Prescaler)
| This macro set the prescaler of the selected channel. More...
#define | PWM_SET_DIVIDER(pwm, u32ChannelNum, u32Divider)
| This macro set the divider of the selected channel. More...
#define | PWM_SET_CMR(pwm, u32ChannelNum, u32CMR)
| This macro set the duty of the selected channel. More...
#define | PWM_SET_CNR(pwm, u32ChannelNum, u32CNR)
| This macro set the period of the selected channel. More...
#define | PWM_SET_ALIGNED_TYPE(pwm, u32ChannelMask, u32AlignedType)
| This macro set the PWM aligned type. More...

## Functions
uint32_t | PWM_ConfigOutputChannel (PWM_T *pwm, uint32_t u32ChannelNum, uint32_t u32Frequency, uint32_t u32DutyCycle)
| This function config PWM generator and get the nearest frequency in edge aligned auto-reload mode. More...
uint32_t | PWM_ConfigCaptureChannel (PWM_T *pwm, uint32_t u32ChannelNum, uint32_t u32UnitTimeNsec, uint32_t u32CaptureEdge)
| This function config PWM capture and get the nearest unit time. More...
void | PWM_Start (PWM_T *pwm, uint32_t u32ChannelMask)
| This function start PWM module. More...
void | PWM_Stop (PWM_T *pwm, uint32_t u32ChannelMask)
| This function stop PWM module. More...
void | PWM_ForceStop (PWM_T *pwm, uint32_t u32ChannelMask)
| This function stop PWM generation immediately by clear channel enable bit. More...
void | PWM_EnableADCTrigger (PWM_T *pwm, uint32_t u32ChannelNum, uint32_t u32Condition)
| This function enable selected channel to trigger ADC. More...
void | PWM_DisableADCTrigger (PWM_T *pwm, uint32_t u32ChannelNum)
| This function disable selected channel to trigger ADC. More...
void | PWM_ClearADCTriggerFlag (PWM_T *pwm, uint32_t u32ChannelNum, uint32_t u32Condition)
| This function clear selected channel trigger ADC flag. More...
uint32_t | PWM_GetADCTriggerFlag (PWM_T *pwm, uint32_t u32ChannelNum)
| This function get selected channel trigger ADC flag. More...
void | PWM_EnableFaultBrake (PWM_T *pwm, uint32_t u32ChannelMask, uint32_t u32LevelMask, uint32_t u32BrakeSource)
| This function enable fault brake of selected channels. More...
void | PWM_ClearFaultBrakeFlag (PWM_T *pwm, uint32_t u32BrakeSource)
| This function clear fault brake flag. More...
void | PWM_EnableCapture (PWM_T *pwm, uint32_t u32ChannelMask)
| This function enables PWM capture of selected channels. More...
void | PWM_DisableCapture (PWM_T *pwm, uint32_t u32ChannelMask)
| This function disables PWM capture of selected channels. More...
void | PWM_EnableOutput (PWM_T *pwm, uint32_t u32ChannelMask)
| This function enables PWM output generation of selected channels. More...
void | PWM_DisableOutput (PWM_T *pwm, uint32_t u32ChannelMask)
| This function disables PWM output generation of selected channels. More...
void | PWM_EnableDeadZone (PWM_T *pwm, uint32_t u32ChannelNum, uint32_t u32Duration)
| This function enable Dead zone of selected channel. More...
void | PWM_DisableDeadZone (PWM_T *pwm, uint32_t u32ChannelNum)
| This function disable Dead zone of selected channel. More...
void | PWM_EnableCaptureInt (PWM_T *pwm, uint32_t u32ChannelNum, uint32_t u32Edge)
| This function enable capture interrupt of selected channel. More...
void | PWM_DisableCaptureInt (PWM_T *pwm, uint32_t u32ChannelNum, uint32_t u32Edge)
| This function disable capture interrupt of selected channel. More...
void | PWM_ClearCaptureIntFlag (PWM_T *pwm, uint32_t u32ChannelNum, uint32_t u32Edge)
| This function clear capture interrupt flag of selected channel. More...
uint32_t | PWM_GetCaptureIntFlag (PWM_T *pwm, uint32_t u32ChannelNum)
| This function get capture interrupt flag of selected channel. More...
void | PWM_EnableDutyInt (PWM_T *pwm, uint32_t u32ChannelNum, uint32_t u32IntDutyType)
| This function enable duty interrupt of selected channel. More...
void | PWM_DisableDutyInt (PWM_T *pwm, uint32_t u32ChannelNum)
| This function disable duty interrupt of selected channel. More...
void | PWM_ClearDutyIntFlag (PWM_T *pwm, uint32_t u32ChannelNum)
| This function clears duty interrupt flag of selected channel. More...
uint32_t | PWM_GetDutyIntFlag (PWM_T *pwm, uint32_t u32ChannelNum)
| This function get duty interrupt flag of selected channel. More...
void | PWM_EnableFaultBrakeInt (PWM_T *pwm, uint32_t u32BrakeSource)
| This function enable fault brake interrupt. More...
void | PWM_DisableFaultBrakeInt (PWM_T *pwm, uint32_t u32BrakeSource)
| This function disable fault brake interrupt. More...
void | PWM_ClearFaultBrakeIntFlag (PWM_T *pwm, uint32_t u32BrakeSource)
| This function clear fault brake interrupt of selected source. More...
uint32_t | PWM_GetFaultBrakeIntFlag (PWM_T *pwm, uint32_t u32BrakeSource)
| This function get fault brake interrupt of selected source. More...
void | PWM_EnablePeriodInt (PWM_T *pwm, uint32_t u32ChannelNum, uint32_t u32IntPeriodType)
| This function enable period interrupt of selected channel. More...
void | PWM_DisablePeriodInt (PWM_T *pwm, uint32_t u32ChannelNum)
| This function disable period interrupt of selected channel. More...
void | PWM_ClearPeriodIntFlag (PWM_T *pwm, uint32_t u32ChannelNum)
| This function clear period interrupt of selected channel. More...
uint32_t | PWM_GetPeriodIntFlag (PWM_T *pwm, uint32_t u32ChannelNum)
| This function get period interrupt of selected channel. More...

## Detailed Description

NUC472/NUC442 PWM driver header file.

Version
  V1.00

Revision
  22

Date
  15/11/16 2:08p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013 Nuvoton Technology Corp. All rights reserved.

Definition in file pwm.h.