| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
PDMA_T Struct Reference

`#include <NUC472_442.h>`

Collaboration diagram for PDMA_T:
[legend]

## Data Fields
DSCT_T | DSCT [16]
__IO uint32_t | CHCTL
__O uint32_t | STOP
__O uint32_t | SWREQ
__I uint32_t | TRGSTS
__IO uint32_t | PRISET
__O uint32_t | PRICLR
__IO uint32_t | INTEN
__IO uint32_t | INTSTS
__IO uint32_t | ABTSTS
__IO uint32_t | TDSTS
__IO uint32_t | SCATSTS
__I uint32_t | TACTSTS
__IO uint32_t | SCATBA
__IO uint32_t | REQSEL0_3
__IO uint32_t | REQSEL4_7
__IO uint32_t | REQSEL8_11
__IO uint32_t | REQSEL12_15

## Detailed Description

Definition at line 18227 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h