| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Macros | Functions
wwdt.h File Reference

NUC472/NUC442 WWDT driver header file. More...

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Macros
#define | WWDT_PRESCALER_1
| WWDT setting prescaler to 1. More...
#define | WWDT_PRESCALER_2
| WWDT setting prescaler to 2. More...
#define | WWDT_PRESCALER_4
| WWDT setting prescaler to 4. More...
#define | WWDT_PRESCALER_8
| WWDT setting prescaler to 8. More...
#define | WWDT_PRESCALER_16
| WWDT setting prescaler to 16. More...
#define | WWDT_PRESCALER_32
| WWDT setting prescaler to 32. More...
#define | WWDT_PRESCALER_64
| WWDT setting prescaler to 64. More...
#define | WWDT_PRESCALER_128
| WWDT setting prescaler to 128. More...
#define | WWDT_PRESCALER_192
| WWDT setting prescaler to 192. More...
#define | WWDT_PRESCALER_256
| WWDT setting prescaler to 256. More...
#define | WWDT_PRESCALER_384
| WWDT setting prescaler to 384. More...
#define | WWDT_PRESCALER_512
| WWDT setting prescaler to 512. More...
#define | WWDT_PRESCALER_768
| WWDT setting prescaler to 768. More...
#define | WWDT_PRESCALER_1024
| WWDT setting prescaler to 1024. More...
#define | WWDT_PRESCALER_1536
| WWDT setting prescaler to 1536. More...
#define | WWDT_PRESCALER_2048
| WWDT setting prescaler to 2048. More...
#define | WWDT_RELOAD_WORD
| Fill this value to RLD register to reload WWDT counter. More...
#define | WWDT_CLEAR_RESET_FLAG()
| This macro clear WWDT time-out reset system flag. More...
#define | WWDT_CLEAR_INT_FLAG()
| This macro clear WWDT compare match interrupt flag. More...
#define | WWDT_GET_RESET_FLAG()
| This macro is use to get WWDT time-out reset system flag. More...
#define | WWDT_GET_INT_FLAG()
| This macro is used to indicate WWDT compare match interrupt flag. More...
#define | WWDT_GET_COUNTER()
| This macro to reflects current WWDT counter value. More...
#define | WWDT_RELOAD_COUNTER()
| This macro is used to reload the WWDT counter value to 0x3F. More...

## Functions
void | WWDT_Open (uint32_t u32PreScale, uint32_t u32CmpValue, uint32_t u32EnableInt)
| This function make WWDT module start counting with different counter period and compared window value. More...

## Detailed Description

NUC472/NUC442 WWDT driver header file.

Version
  V1.00

Revision
  9

Date
  14/05/29 1:13p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013 Nuvoton Technology Corp. All rights reserved.

Definition in file wwdt.h.