| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
SYS_T Struct Reference

`#include <NUC472_442.h>`

## Data Fields
__I uint32_t | PDID
__IO uint32_t | RSTSTS
__IO uint32_t | IPRST0
__IO uint32_t | IPRST1
__IO uint32_t | IPRST2
__IO uint32_t | BODCTL
__IO uint32_t | TEMPCTL
__I uint32_t | VCID
__IO uint32_t | PORCTL
__IO uint32_t | VREFCTL
__IO uint32_t | USBPHY
__IO uint32_t | GPA_MFPL
__IO uint32_t | GPA_MFPH
__IO uint32_t | GPB_MFPL
__IO uint32_t | GPB_MFPH
__IO uint32_t | GPC_MFPL
__IO uint32_t | GPC_MFPH
__IO uint32_t | GPD_MFPL
__IO uint32_t | GPD_MFPH
__IO uint32_t | GPE_MFPL
__IO uint32_t | GPE_MFPH
__IO uint32_t | GPF_MFPL
__IO uint32_t | GPF_MFPH
__IO uint32_t | GPG_MFPL
__IO uint32_t | GPG_MFPH
__IO uint32_t | GPH_MFPL
__IO uint32_t | GPH_MFPH
__IO uint32_t | GPI_MFPL
__IO uint32_t | GPI_MFPH
__IO uint32_t | SRAM_INTCTL
__IO uint32_t | SRAM_STATUS
__I uint32_t | SRAM0_ERRADDR
__I uint32_t | SRAM1_ERRADDR
__IO uint32_t | IRCTCTL
__IO uint32_t | IRCTIEN
__IO uint32_t | IRCTISTS
__IO uint32_t | REGLCTL

## Detailed Description

    @addtogroup SYS System Manger Controller(SYS)
    Memory Mapped Structure for SYS Controller

Definition at line 23263 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h