| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Modules | Macros
Smartcard Library Exported Constants
NUC472/NUC442 Library » Smartcard Library
Collaboration diagram for Smartcard Library Exported Constants:

## Modules
| Smartcard Library Exported Structs

## Macros
#define | SCLIB_MAX_ATR_LEN
| Max ATR length. ISO-7816 8.2.1. More...
#define | SCLIB_MIN_ATR_LEN
| Min ATR length, TS and T0. More...
#define | SCLIB_PROTOCOL_UNDEFINED
| There is no active protocol. More...
#define | SCLIB_PROTOCOL_T0
| T=0 is the active protocol. More...
#define | SCLIB_PROTOCOL_T1
| T=1 is the active protocol. More...
#define | SCLIB_SUCCESS
| Command successful without error. More...
#define | SCLIB_ERR_CARD_REMOVED
| Smartcard removed. More...
#define | SCLIB_ERR_OVER_RUN
| Rx FIFO over run. More...
#define | SCLIB_ERR_PARITY_ERROR
| Tx/Rx parity error. More...
#define | SCLIB_ERR_NO_STOP
| Stop bit not found. More...
#define | SCLIB_ERR_SILENT_BYTE
| I/O pin stay at low for longer than 1 character time. More...
#define | SCLIB_ERR_READ
| Smartcard read error. More...
#define | SCLIB_ERR_WRITE
| Smartcard write error. More...
#define | SCLIB_ERR_TIME0OUT
| Smartcard timer 0 timeout. More...
#define | SCLIB_ERR_TIME1OUT
| Smartcard timer 1 timeout. More...
#define | SCLIB_ERR_TIME2OUT
| Smartcard timer 2 timeout. More...
#define | SCLIB_ERR_AUTOCONVENTION
| Smartcard is neither direct nor inverse convention. More...
#define | SCLIB_ERR_CLOCK
| Smartcard clock frequency is not between 1MHz and 5 MHz. More...
#define | SCLIB_ERR_ATR_UNRECOGNIZED
| Unrecognised ATR. More...
#define | SCLIB_ERR_ATR_INVALID_PARAM
| ATR parsing interface bytes error. More...
#define | SCLIB_ERR_ATR_INVALID_TCK
| TCK check byte error. More...
#define | SCLIB_ERR_PPS
| PPS error. More...
#define | SCLIB_ERR_T1_PROTOCOL
| T=1 Protocol Error. More...
#define | SCLIB_ERR_T1_ABORT_RECEIVED
| Received ABORT request. More...
#define | SCLIB_ERR_T1_RESYNCH_RECEIVED
| Received RESYNCH request. More...
#define | SCLIB_ERR_T1_VPP_ERROR_RECEIVED
| Received VPP error. More...
#define | SCLIB_ERR_T1_WTXRES_RECEIVED
| Received BWT extension request. More...
#define | SCLIB_ERR_T1_IFSRES_RECEIVED
| Received max IFS offer. More...
#define | SCLIB_ERR_T1_ABORTRES_RECEIVED
| Received ABORT response. More...
#define | SCLIB_ERR_T1_CHECKSUM
| T=1 block check sum error. More...
#define | SCLIB_ERR_T0_PROTOCOL
| T=0 Protocol Error. More...
#define | SCLIB_ERR_DEACTIVE
| Smartcard is deactivate. More...
#define | SCLIB_ERR_CARDBUSY
| Smartcard is busy, previous transmission is not complete yet. More...

## Detailed Description

## Macro Definition Documentation

## ◆ SCLIB_ERR_ATR_INVALID_PARAM

#define SCLIB_ERR_ATR_INVALID_PARAM

ATR parsing interface bytes error.

Definition at line 66 of file sclib.h.

## ◆ SCLIB_ERR_ATR_INVALID_TCK

#define SCLIB_ERR_ATR_INVALID_TCK

TCK check byte error.

Definition at line 67 of file sclib.h.

## ◆ SCLIB_ERR_ATR_UNRECOGNIZED

#define SCLIB_ERR_ATR_UNRECOGNIZED

Unrecognised ATR.

Definition at line 65 of file sclib.h.

## ◆ SCLIB_ERR_AUTOCONVENTION

#define SCLIB_ERR_AUTOCONVENTION

Smartcard is neither direct nor inverse convention.

Definition at line 61 of file sclib.h.

## ◆ SCLIB_ERR_CARD_REMOVED

#define SCLIB_ERR_CARD_REMOVED

Smartcard removed.

Definition at line 49 of file sclib.h.

## ◆ SCLIB_ERR_CARDBUSY

#define SCLIB_ERR_CARDBUSY

Smartcard is busy, previous transmission is not complete yet.

Definition at line 86 of file sclib.h.

## ◆ SCLIB_ERR_CLOCK

#define SCLIB_ERR_CLOCK

Smartcard clock frequency is not between 1MHz and 5 MHz.

Definition at line 62 of file sclib.h.

## ◆ SCLIB_ERR_DEACTIVE

#define SCLIB_ERR_DEACTIVE

Smartcard is deactivate.

Definition at line 85 of file sclib.h.

## ◆ SCLIB_ERR_NO_STOP

#define SCLIB_ERR_NO_STOP

Stop bit not found.

Definition at line 52 of file sclib.h.

## ◆ SCLIB_ERR_OVER_RUN

#define SCLIB_ERR_OVER_RUN

Rx FIFO over run.

Definition at line 50 of file sclib.h.

## ◆ SCLIB_ERR_PARITY_ERROR

#define SCLIB_ERR_PARITY_ERROR

Tx/Rx parity error.

Definition at line 51 of file sclib.h.

## ◆ SCLIB_ERR_PPS

#define SCLIB_ERR_PPS

PPS error.

Definition at line 68 of file sclib.h.

## ◆ SCLIB_ERR_READ

#define SCLIB_ERR_READ

Smartcard read error.

Definition at line 56 of file sclib.h.

## ◆ SCLIB_ERR_SILENT_BYTE

#define SCLIB_ERR_SILENT_BYTE

I/O pin stay at low for longer than 1 character time.

Definition at line 53 of file sclib.h.

## ◆ SCLIB_ERR_T0_PROTOCOL

#define SCLIB_ERR_T0_PROTOCOL

T=0 Protocol Error.

Definition at line 82 of file sclib.h.

## ◆ SCLIB_ERR_T1_ABORT_RECEIVED

#define SCLIB_ERR_T1_ABORT_RECEIVED

Received ABORT request.

Definition at line 73 of file sclib.h.

## ◆ SCLIB_ERR_T1_ABORTRES_RECEIVED

#define SCLIB_ERR_T1_ABORTRES_RECEIVED

Received ABORT response.

Definition at line 78 of file sclib.h.

## ◆ SCLIB_ERR_T1_CHECKSUM

#define SCLIB_ERR_T1_CHECKSUM

T=1 block check sum error.

Definition at line 79 of file sclib.h.

## ◆ SCLIB_ERR_T1_IFSRES_RECEIVED

#define SCLIB_ERR_T1_IFSRES_RECEIVED

Received max IFS offer.

Definition at line 77 of file sclib.h.

## ◆ SCLIB_ERR_T1_PROTOCOL

#define SCLIB_ERR_T1_PROTOCOL

T=1 Protocol Error.

Definition at line 72 of file sclib.h.

## ◆ SCLIB_ERR_T1_RESYNCH_RECEIVED

#define SCLIB_ERR_T1_RESYNCH_RECEIVED

Received RESYNCH request.

Definition at line 74 of file sclib.h.

## ◆ SCLIB_ERR_T1_VPP_ERROR_RECEIVED

#define SCLIB_ERR_T1_VPP_ERROR_RECEIVED

Received VPP error.

Definition at line 75 of file sclib.h.

## ◆ SCLIB_ERR_T1_WTXRES_RECEIVED

#define SCLIB_ERR_T1_WTXRES_RECEIVED

Received BWT extension request.

Definition at line 76 of file sclib.h.

## ◆ SCLIB_ERR_TIME0OUT

#define SCLIB_ERR_TIME0OUT

Smartcard timer 0 timeout.

Definition at line 58 of file sclib.h.

## ◆ SCLIB_ERR_TIME1OUT

#define SCLIB_ERR_TIME1OUT

Smartcard timer 1 timeout.

Definition at line 59 of file sclib.h.

## ◆ SCLIB_ERR_TIME2OUT

#define SCLIB_ERR_TIME2OUT

Smartcard timer 2 timeout.

Definition at line 60 of file sclib.h.

## ◆ SCLIB_ERR_WRITE

#define SCLIB_ERR_WRITE

Smartcard write error.

Definition at line 57 of file sclib.h.

## ◆ SCLIB_MAX_ATR_LEN

#define SCLIB_MAX_ATR_LEN

Max ATR length. ISO-7816 8.2.1.

Definition at line 39 of file sclib.h.

## ◆ SCLIB_MIN_ATR_LEN

#define SCLIB_MIN_ATR_LEN

Min ATR length, TS and T0.

Definition at line 40 of file sclib.h.

## ◆ SCLIB_PROTOCOL_T0

#define SCLIB_PROTOCOL_T0

T=0 is the active protocol.

Definition at line 44 of file sclib.h.

## ◆ SCLIB_PROTOCOL_T1

#define SCLIB_PROTOCOL_T1

T=1 is the active protocol.

Definition at line 45 of file sclib.h.

## ◆ SCLIB_PROTOCOL_UNDEFINED

#define SCLIB_PROTOCOL_UNDEFINED

There is no active protocol.

Definition at line 43 of file sclib.h.

## ◆ SCLIB_SUCCESS

#define SCLIB_SUCCESS

Command successful without error.

Definition at line 47 of file sclib.h.