| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
STR_CANMASK_T Struct Reference
NUC472/NUC442 Device Driver » CAN Driver » CAN Exported Type Defines

`#include <can.h>`

## Data Fields
uint8_t | u8Xtd
uint8_t | u8Dir
uint32_t | u32Id
uint8_t | u8IdType

## Detailed Description

CAN mask message structure.

Definition at line 65 of file can.h.

The documentation for this struct was generated from the following file:

- StdDriver/inc/can.h