| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
CAN_T Struct Reference

`#include <NUC472_442.h>`

Collaboration diagram for CAN_T:
[legend]

## Data Fields
__IO uint32_t | CON
__IO uint32_t | STATUS
__IO uint32_t | ERR
__IO uint32_t | BTIME
__IO uint32_t | IIDR
__IO uint32_t | TEST
__IO uint32_t | BRPE
__I uint32_t | RESERVE0 [1]
__IO CAN_IF_T | IF [2]
__I uint32_t | RESERVE1 [8]
__IO uint32_t | TXREQ1
__IO uint32_t | TXREQ2
__I uint32_t | RESERVE2 [6]
__IO uint32_t | NDAT1
__IO uint32_t | NDAT2
__I uint32_t | RESERVE3 [6]
__IO uint32_t | IPND1
__IO uint32_t | IPND2
__I uint32_t | RESERVE4 [6]
__IO uint32_t | MVLD1
__IO uint32_t | MVLD2
__IO uint32_t | WU_EN
__IO uint32_t | WU_STATUS

## Detailed Description

Definition at line 1125 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h