| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
PS2_T Struct Reference

`#include <NUC472_442.h>`

## Data Fields
__IO uint32_t | CTL
__IO uint32_t | TXDAT0
__IO uint32_t | TXDAT1
__IO uint32_t | TXDAT2
__IO uint32_t | TXDAT3
__I uint32_t | RXDAT
__IO uint32_t | STATUS
__IO uint32_t | INTSTS

## Detailed Description

    @addtogroup PS2 PS/2 Device Controller(PS2)
    Memory Mapped Structure for PS2 Controller

Definition at line 18746 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h