| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Macros | Functions
sd.c File Reference

NUC472/NUC442 SD driver source file. More...

`#include <stdio.h>`
`#include <stdlib.h>`
`#include <string.h>`
`#include "NUC472_442.h"`
Include dependency graph for sd.c:

Go to the source code of this file.

## Macros
#define | SD_BLOCK_SIZE 512

## Functions
void | SD_Open (uint32_t u32CardDetSrc)
| This function use to reset SD function and select card detection source and pin. More...
void | SD_Probe (uint32_t u32CardNum)
| This function use to initial SD card. More...
uint32_t | SD_Read (uint32_t u32CardNum, uint8_t *pu8BufAddr, uint32_t u32StartSec, uint32_t u32SecCount)
| This function use to read data from SD card. More...
uint32_t | SD_Write (uint32_t u32CardNum, uint8_t *pu8BufAddr, uint32_t u32StartSec, uint32_t u32SecCount)
| This function use to write data to SD card. More...

## Detailed Description

NUC472/NUC442 SD driver source file.

Version
  V1.00

Revision
  16

Date
  15/11/26 10:45a

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013 Nuvoton Technology Corp. All rights reserved.

Definition in file sd.c.