<map id="StdDriver/src/retarget.c" name="StdDriver/src/retarget.c">
<area shape="rect" id="node1" title="NUC472 Series Debug Port and Semihost Setting Source File." alt="" coords="2035,5,2190,32"/>
<area shape="rect" id="node2" title=" " alt="" coords="269,229,330,256"/>
<area shape="rect" id="node3" href="$da/d08/_n_u_c472__442_8h.html" title="NUC472/NUC442 peripheral access layer header file. This file contains all the peripheral register&#39;s d..." alt="" coords="1447,80,1557,107"/>
<area shape="rect" id="node4" title=" " alt="" coords="2597,155,2687,181"/>
<area shape="rect" id="node5" href="$d1/d5e/system___n_u_c472__442_8h.html" title="NUC472/NUC442 system clock definition file." alt="" coords="5,155,164,181"/>
<area shape="rect" id="node6" title=" " alt="" coords="133,229,199,256"/>
<area shape="rect" id="node7" href="$d9/d87/sys_8h.html" title="NUC472/NUC442 SYS Header File." alt="" coords="311,155,365,181"/>
<area shape="rect" id="node8" href="$d3/d89/clk_8h.html" title="NUC472/NUC442 CLK Header File." alt="" coords="390,155,441,181"/>
<area shape="rect" id="node9" href="$dc/d2f/acmp_8h.html" title="NUC472/NUC442 Analog Comparator(ACMP) driver header file." alt="" coords="465,155,531,181"/>
<area shape="rect" id="node10" href="$d7/d19/adc_8h.html" title="NUC472/NUC442 ADC driver header file." alt="" coords="555,155,609,181"/>
<area shape="rect" id="node11" href="$da/da5/eadc_8h.html" title="NUC472/NUC442 EADC driver header file." alt="" coords="634,155,695,181"/>
<area shape="rect" id="node12" href="$d0/dda/cap_8h.html" title="NUC470 series Image Capture Driver Header File." alt="" coords="720,155,775,181"/>
<area shape="rect" id="node13" href="$da/da0/crypto_8h.html" title="Cryptographic Accelerator driver header file." alt="" coords="799,155,869,181"/>
<area shape="rect" id="node14" href="$d1/d47/pdma_8h.html" title="NUC472/NUC442 PDMA driver header file." alt="" coords="893,155,959,181"/>
<area shape="rect" id="node15" href="$da/d96/ebi_8h.html" title="NUC472/NUC442 EBI driver header file." alt="" coords="983,155,1034,181"/>
<area shape="rect" id="node16" href="$d6/d55/emac_8h.html" title="NUC472/NUC442 EMAC driver header file." alt="" coords="1059,155,1124,181"/>
<area shape="rect" id="node17" href="$dc/d00/fmc_8h.html" title="NUC472/NUC442 Flash Memory Controller Driver Header File." alt="" coords="1148,155,1203,181"/>
<area shape="rect" id="node18" href="$d6/d7c/gpio_8h.html" title="NUC472/NUC442 GPIO driver header file." alt="" coords="1227,155,1284,181"/>
<area shape="rect" id="node19" href="$d5/daf/i2c_8h.html" title="NUC472/NUC442 I2C driver header file." alt="" coords="1309,155,1359,181"/>
<area shape="rect" id="node20" href="$d6/db9/pwm_8h.html" title="NUC472/NUC442 PWM driver header file." alt="" coords="1384,155,1444,181"/>
<area shape="rect" id="node21" href="$dc/d9b/epwm_8h.html" title="NUC472/NUC442 EPWM driver header file." alt="" coords="1469,155,1535,181"/>
<area shape="rect" id="node22" href="$dc/d1b/rtc_8h.html" title="NUC472/NUC442 RTC driver header file." alt="" coords="1559,155,1607,181"/>
<area shape="rect" id="node23" href="$d9/d50/sc_8h.html" title="NUC472/NUC442 Smartcard (SC) driver header file." alt="" coords="1632,155,1679,181"/>
<area shape="rect" id="node24" href="$dc/d0b/scuart_8h.html" title=" " alt="" coords="1703,155,1773,181"/>
<area shape="rect" id="node25" href="$da/d87/spi_8h.html" title="NUC472/NUC442 SPI driver header file." alt="" coords="1797,155,1847,181"/>
<area shape="rect" id="node26" href="$d5/dd0/timer_8h.html" title="NUC472/NUC442 TIMER driver header file." alt="" coords="1872,155,1935,181"/>
<area shape="rect" id="node27" href="$d2/d86/uart_8h.html" title="NUC472/NUC442 UART driver header file." alt="" coords="1959,155,2013,181"/>
<area shape="rect" id="node28" href="$da/ddf/usbd_8h.html" title="NUC472/NUC442 USBD driver header file." alt="" coords="2038,155,2099,181"/>
<area shape="rect" id="node29" href="$d0/de2/wdt_8h.html" title="NUC472/NUC442 WDT driver header file." alt="" coords="2123,155,2177,181"/>
<area shape="rect" id="node30" href="$dd/d09/wwdt_8h.html" title="NUC472/NUC442 WWDT driver header file." alt="" coords="2201,155,2264,181"/>
<area shape="rect" id="node31" href="$d1/da9/i2s_8h.html" title=" " alt="" coords="2289,155,2339,181"/>
<area shape="rect" id="node32" href="$d7/da8/can_8h.html" title="NUC472/NUC442 CAN driver header file." alt="" coords="2364,155,2419,181"/>
<area shape="rect" id="node33" href="$d6/d23/sd_8h.html" title="NUC472/NUC442 SD driver header file." alt="" coords="240,155,287,181"/>
<area shape="rect" id="node34" href="$d8/d29/ps2_8h.html" title="NUC472/NUC442 PS2 Driver Header File." alt="" coords="2443,155,2497,181"/>
<area shape="rect" id="node35" href="$dc/de6/crc_8h.html" title="NUC472/NUC442 series CRC driver header file." alt="" coords="2522,155,2573,181"/>
</map>
