| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
SC_T Struct Reference

`#include <NUC472_442.h>`

## Data Fields
__IO uint32_t | DAT
__IO uint32_t | CTL
__IO uint32_t | ALTCTL
__IO uint32_t | EGT
__IO uint32_t | RXTOUT
__IO uint32_t | ETUCTL
__IO uint32_t | INTEN
__IO uint32_t | INTSTS
__IO uint32_t | STATUS
__IO uint32_t | PINCTL
__IO uint32_t | TMRCTL0
__IO uint32_t | TMRCTL1
__IO uint32_t | TMRCTL2
__IO uint32_t | UARTCTL
__I uint32_t | TMRDAT0
__I uint32_t | TMRDAT1_2

## Detailed Description

    @addtogroup SC Smart Card Host Interface Controller(SC)
    Memory Mapped Structure for SC Controller

Definition at line 21114 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h