| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
EBI_T Struct Reference

`#include <NUC472_442.h>`

## Data Fields
__IO uint32_t | CTL
__IO uint32_t | TCTL [4]
__IO uint32_t | KEY0
__IO uint32_t | KEY1
__IO uint32_t | KEY2
__IO uint32_t | KEY3

## Detailed Description

    @addtogroup EBI External Bus Interface Controller(EBI)
    Memory Mapped Structure for EBI Controller

Definition at line 11569 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h