| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Functions
epwm.c File Reference

NUC472/NUC442 EPWM driver source file. More...

`#include "NUC472_442.h"`
Include dependency graph for epwm.c:

Go to the source code of this file.

## Functions
uint32_t | EPWM_ConfigOutputChannel (EPWM_T *pwm, uint32_t u32ChannelNum, uint32_t u32Frequency, uint32_t u32DutyCycle)
| This function config PWM generator and get the nearest frequency in edge aligned auto-reload mode. More...
void | EPWM_Start (EPWM_T *pwm, uint32_t u32ChannelMask)
| This function start PWM module. More...
void | EPWM_Stop (EPWM_T *pwm, uint32_t u32ChannelMask)
| This function stop PWM module. More...
void | EPWM_ForceStop (EPWM_T *pwm, uint32_t u32ChannelMask)
| This function stop PWM generation immediately by clear channel enable bit. More...
void | EPWM_EnableFaultBrake (EPWM_T *pwm, uint32_t u32ChannelMask, uint32_t u32LevelMask, uint32_t u32BrakeSource)
| This function enable fault brake of selected channels. More...
void | EPWM_ClearFaultBrakeFlag (EPWM_T *pwm, uint32_t u32BrakeSource)
| This function clear fault brake flag. More...
void | EPWM_EnableOutput (EPWM_T *pwm, uint32_t u32ChannelMask)
| This function enables PWM output generation of selected channels. More...
void | EPWM_DisableOutput (EPWM_T *pwm, uint32_t u32ChannelMask)
| This function disables PWM output generation of selected channels. More...
void | EPWM_EnableDeadZone (EPWM_T *pwm, uint32_t u32ChannelNum, uint32_t u32Duration)
| This function enable Dead zone of selected channel. More...
void | EPWM_DisableDeadZone (EPWM_T *pwm, uint32_t u32ChannelNum)
| This function disable Dead zone of selected channel. More...
void | EPWM_EnableDutyInt (EPWM_T *pwm, uint32_t u32ChannelNum, uint32_t u32IntDutyType)
| This function enable duty interrupt of selected channel. More...
void | EPWM_DisableDutyInt (EPWM_T *pwm, uint32_t u32ChannelNum)
| This function disable duty interrupt of selected channel. More...
void | EPWM_ClearDutyIntFlag (EPWM_T *pwm, uint32_t u32ChannelNum)
| This function clears duty interrupt flag of selected channel. More...
uint32_t | EPWM_GetDutyIntFlag (EPWM_T *pwm, uint32_t u32ChannelNum)
| This function get duty interrupt flag of selected channel. More...
void | EPWM_EnableFaultBrakeInt (EPWM_T *pwm, uint32_t u32BrakeSource)
| This function enable fault brake interrupt. More...
void | EPWM_DisableFaultBrakeInt (EPWM_T *pwm, uint32_t u32BrakeSource)
| This function disable fault brake interrupt. More...
void | EPWM_ClearFaultBrakeIntFlag (EPWM_T *pwm, uint32_t u32BrakeSource)
| This function clear fault brake interrupt of selected source. More...
uint32_t | EPWM_GetFaultBrakeIntFlag (EPWM_T *pwm, uint32_t u32BrakeSource)
| This function get fault brake interrupt of selected source. More...
void | EPWM_EnablePeriodInt (EPWM_T *pwm, uint32_t u32ChannelNum, uint32_t u32IntPeriodType)
| This function enable period interrupt of selected channel. More...
void | EPWM_DisablePeriodInt (EPWM_T *pwm, uint32_t u32ChannelNum)
| This function disable period interrupt of selected channel. More...
void | EPWM_ClearPeriodIntFlag (EPWM_T *pwm, uint32_t u32ChannelNum)
| This function clear period interrupt of selected channel. More...
uint32_t | EPWM_GetPeriodIntFlag (EPWM_T *pwm, uint32_t u32ChannelNum)
| This function get period interrupt of selected channel. More...

## Detailed Description

NUC472/NUC442 EPWM driver source file.

Version
  V1.00

Revision
  3

Date
  15/11/18 2:33p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2014 Nuvoton Technology Corp. All rights reserved.

Definition in file epwm.c.