| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Structures
Here are the data structures with brief descriptions:

C ACMP_T |
C ADC_T |
C CAN_IF_T |
C CAN_T |
C CAP_T |
C CLK_T |
C CRC_T |
C CRPT_T |
C disk_data_t |
C DSCT_T |
C EADC_T |
C EBI_T |
C ECAP_T |
C EMAC_T |
C EPWM_T |
C FMC_T |
C GPIO_DB_T |
C GPIO_T |
C I2C_T |
C I2S_T |
C iso_pkt_t |
C mass_disk_t |
C OPA_T |
C OTG_T |
C PDMA_T |
C PS2_T |
C PWM_T |
C QEI_T |
C RTC_T |
C S_RTC_TIME_DATA_T | RTC define Time Data Struct
C s_usbd_info |
C SC_T |
C SCLIB_CARD_INFO_T | A structure holds smartcard information
C SD_info_t |
C SDH_T |
C SPI_T |
C STR_CANMASK_T |
C STR_CANMSG_T |
C SYS_T |
C TIMER_T |
C uac_dev_t |
C UART_T |
C urb_t |
C usb_device |
C USBD_CMD_STRUCT |
C USBD_EP_T | USBD endpoints register
C USBD_T |
C USBH_T |
C usbhid_dev |
C WDT_T |
C WWDT_T |