<map id="USBH_SubmitUrb" name="USBH_SubmitUrb">
<area shape="rect" id="node1" title="Submit an URB to USB core for transfer data." alt="" coords="236,81,363,108"/>
<area shape="rect" id="node2" href="$d2/daf/group___n_u_c472__442___u_s_b_h___a_s___e_x_p_o_r_t_e_d___f_u_n_c_t_i_o_n_s.html#gaffdb9af72c444a85f97d14f15afcfcfd" title="Start to receive audio data from UAC device via isochronous in pipe." alt="" coords="28,5,165,32"/>
<area shape="rect" id="node3" href="$d2/daf/group___n_u_c472__442___u_s_b_h___a_s___e_x_p_o_r_t_e_d___f_u_n_c_t_i_o_n_s.html#ga077af2035b32e5d9564adfb364ccb5ce" title="Start to send audio data to UAC device via isochronous out pipe." alt="" coords="23,56,171,83"/>
<area shape="rect" id="node4" href="$d3/dd0/group___n_u_c472__442___u_s_b_h___h_i_d___e_x_p_o_r_t_e_d___f_u_n_c_t_i_o_n_s.html#ga239689e9888b50ea0dbfdff6578eca1a" title="Start purge the USB interrupt in transfer." alt="" coords="5,107,188,133"/>
<area shape="rect" id="node5" href="$d3/dd0/group___n_u_c472__442___u_s_b_h___h_i_d___e_x_p_o_r_t_e_d___f_u_n_c_t_i_o_n_s.html#gab60bfbd7f4919798c828006abae92445" title="Start purge the USB interrupt out transfer." alt="" coords="5,157,188,184"/>
</map>
