| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Functions
adc.c File Reference

NUC472/NUC442 ADC driver source file. More...

`#include "NUC472_442.h"`
Include dependency graph for adc.c:

Go to the source code of this file.

## Functions
void | ADC_Open (ADC_T *adc, uint32_t u32InputMode, uint32_t u32OpMode, uint32_t u32ChMask)
| This API configures ADC module to be ready for convert the input from selected channel. More...
void | ADC_Close (ADC_T *adc)
| Disable ADC module. More...
void | ADC_EnableHWTrigger (ADC_T *adc, uint32_t u32Source, uint32_t u32Param)
| Configure the hardware trigger condition and enable hardware trigger. More...
void | ADC_DisableHWTrigger (ADC_T *adc)
| Disable hardware trigger ADC function. More...
void | ADC_EnableInt (ADC_T *adc, uint32_t u32Mask)
| Enable the interrupt(s) selected by u32Mask parameter. More...
void | ADC_DisableInt (ADC_T *adc, uint32_t u32Mask)
| Disable the interrupt(s) selected by u32Mask parameter. More...

## Detailed Description

NUC472/NUC442 ADC driver source file.

Version
  V1.00

Revision
  13

Date
  14/05/29 1:13p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013 Nuvoton Technology Corp. All rights reserved.

Definition in file adc.c.