| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Modules | Macros | Variables
SCUART Exported Constants
NUC472/NUC442 Device Driver » SCUART Driver
Collaboration diagram for SCUART Exported Constants:

## Modules
| SCUART Exported Functions

## Macros
#define | SCUART_CHAR_LEN_5
#define | SCUART_CHAR_LEN_6
#define | SCUART_CHAR_LEN_7
#define | SCUART_CHAR_LEN_8
#define | SCUART_PARITY_NONE
#define | SCUART_PARITY_ODD
#define | SCUART_PARITY_EVEN
#define | SCUART_STOP_BIT_1
#define | SCUART_STOP_BIT_2
#define | SCUART_TIMEOUT_ERR

## Variables
int32_t | g_SCUART_i32ErrCode

## Detailed Description

## Macro Definition Documentation

## ◆ SCUART_CHAR_LEN_5

#define SCUART_CHAR_LEN_5

Set SCUART word length to 5 bits

Definition at line 32 of file scuart.h.

## ◆ SCUART_CHAR_LEN_6

#define SCUART_CHAR_LEN_6

Set SCUART word length to 6 bits

Definition at line 33 of file scuart.h.

## ◆ SCUART_CHAR_LEN_7

#define SCUART_CHAR_LEN_7

Set SCUART word length to 7 bits

Definition at line 34 of file scuart.h.

## ◆ SCUART_CHAR_LEN_8

#define SCUART_CHAR_LEN_8

Set SCUART word length to 8 bits

Definition at line 35 of file scuart.h.

## ◆ SCUART_PARITY_EVEN

#define SCUART_PARITY_EVEN

Set SCUART transfer with even parity

Definition at line 39 of file scuart.h.

## ◆ SCUART_PARITY_NONE

#define SCUART_PARITY_NONE

Set SCUART transfer with no parity

Definition at line 37 of file scuart.h.

## ◆ SCUART_PARITY_ODD

#define SCUART_PARITY_ODD

Set SCUART transfer with odd parity

Definition at line 38 of file scuart.h.

## ◆ SCUART_STOP_BIT_1

#define SCUART_STOP_BIT_1

Set SCUART transfer with one stop bit

Definition at line 41 of file scuart.h.

## ◆ SCUART_STOP_BIT_2

#define SCUART_STOP_BIT_2

Set SCUART transfer with two stop bits

Definition at line 42 of file scuart.h.

## ◆ SCUART_TIMEOUT_ERR

#define SCUART_TIMEOUT_ERR

SCUART operation abort due to timeout error

Definition at line 44 of file scuart.h.

## Variable Documentation

## ◆ g_SCUART_i32ErrCode

int32_t g_SCUART_i32ErrCode
| extern

SCUART global error code

Definition at line 27 of file scuart.c.