| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - t -

- T : SCLIB_CARD_INFO_T
- TACTSTS : PDMA_T
- TALM : RTC_T
- TAMP0PCTL : RTC_T
- TAMP1PCTL : RTC_T
- TAMPCTL : RTC_T
- TAMPSTS : RTC_T
- TAMSK : RTC_T
- TCTL : EBI_T
- TDES0_CNT : CRPT_T
- TDES0_DADDR : CRPT_T
- TDES0_IVH : CRPT_T
- TDES0_IVL : CRPT_T
- TDES0_KEY1H : CRPT_T
- TDES0_KEY1L : CRPT_T
- TDES0_KEY2H : CRPT_T
- TDES0_KEY2L : CRPT_T
- TDES0_KEY3H : CRPT_T
- TDES0_KEY3L : CRPT_T
- TDES0_SADDR : CRPT_T
- TDES1_CNT : CRPT_T
- TDES1_DADDR : CRPT_T
- TDES1_IVH : CRPT_T
- TDES1_IVL : CRPT_T
- TDES1_KEY1H : CRPT_T
- TDES1_KEY1L : CRPT_T
- TDES1_KEY2H : CRPT_T
- TDES1_KEY2L : CRPT_T
- TDES1_KEY3H : CRPT_T
- TDES1_KEY3L : CRPT_T
- TDES1_SADDR : CRPT_T
- TDES2_CNT : CRPT_T
- TDES2_DADDR : CRPT_T
- TDES2_IVH : CRPT_T
- TDES2_IVL : CRPT_T
- TDES2_KEY1H : CRPT_T
- TDES2_KEY1L : CRPT_T
- TDES2_KEY2H : CRPT_T
- TDES2_KEY2L : CRPT_T
- TDES2_KEY3H : CRPT_T
- TDES2_KEY3L : CRPT_T
- TDES2_SADDR : CRPT_T
- TDES3_CNT : CRPT_T
- TDES3_DADDR : CRPT_T
- TDES3_IVH : CRPT_T
- TDES3_IVL : CRPT_T
- TDES3_KEY1H : CRPT_T
- TDES3_KEY1L : CRPT_T
- TDES3_KEY2H : CRPT_T
- TDES3_KEY2L : CRPT_T
- TDES3_KEY3H : CRPT_T
- TDES3_KEY3L : CRPT_T
- TDES3_SADDR : CRPT_T
- TDES_CTL : CRPT_T
- TDES_DATIN : CRPT_T
- TDES_DATOUT : CRPT_T
- TDES_FDBCKH : CRPT_T
- TDES_FDBCKL : CRPT_T
- TDES_STS : CRPT_T
- TDSTS : PDMA_T
- TEMPCTL : SYS_T
- TEST : CAN_T, USBD_T
- TICK : RTC_T
- TIME : RTC_T
- timeout : urb_t
- TMRCTL0 : SC_T
- TMRCTL1 : SC_T
- TMRCTL2 : SC_T
- TMRDAT0 : SC_T
- TMRDAT1_2 : SC_T
- TOCTL : I2C_T
- toggle : usb_device
- totalSectorN : disk_data_t
- TOUT : SDH_T, UART_T
- transfer_buffer : urb_t
- transfer_buffer_length : urb_t
- transfer_flags : urb_t
- TRGADCSTS : PWM_T
- TRGADCTL : PWM_T
- TRGSTS : PDMA_T
- TSADDEND : EMAC_T
- TSCTL : EMAC_T
- TSINC : EMAC_T
- TSSEC : EMAC_T
- TSSUBSEC : EMAC_T
- TX : I2S_T, SPI_T
- TXDAT0 : PS2_T
- TXDAT1 : PS2_T
- TXDAT2 : PS2_T
- TXDAT3 : PS2_T
- TXDSA : EMAC_T
- TXREQ1 : CAN_T
- TXREQ2 : CAN_T
- TXST : EMAC_T