| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
SDH_T Struct Reference

`#include <NUC472_442.h>`

## Data Fields
uint32_t | FB [32]
__IO uint32_t | DMACTL
__IO uint32_t | DMASA
__I uint32_t | DMABCNT
__IO uint32_t | DMAINTEN
__IO uint32_t | DMAINTSTS
__IO uint32_t | GCTL
__IO uint32_t | GINTEN
__I uint32_t | GINTSTS
__IO uint32_t | CTL
__IO uint32_t | CMDARG
__IO uint32_t | INTEN
__IO uint32_t | INTSTS
__I uint32_t | RESP0
__I uint32_t | RESP1
__IO uint32_t | BLEN
__IO uint32_t | TOUT

## Detailed Description

    @addtogroup SDH SD Card Host Interface(SDH)
    Memory Mapped Structure for SDH Controller

Definition at line 22056 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h