| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
usb_device Struct Reference
NUC472/NUC442 Device Driver » USBH Driver » USBH Exported Constants » USBH Exported Structures

`#include <usbh_core.h>`

Collaboration diagram for usb_device:
[legend]

## Data Fields
USB_DEV_DESC_T | descriptor
int | devnum
int | slow
int | speed
uint32_t | toggle [2]
uint32_t | halted [2]
struct usb_device * | parent
int | hub_port
USB_BUS_T * | bus
signed char | act_config
char | act_iface
char | iface_alternate
EP_INFO_T | ep_list [MAX_ENDPOINTS]
int | ep_list_cnt
int | have_langid
int | string_langid
void * | hcpriv
int | maxchild
struct usb_device * | children [USB_MAXCHILDREN]
USB_DRIVER_T * | driver [MAX_DRIVER_PER_DEV]
int | driver_cnt

## Detailed Description

URB structure

USB device structure

Definition at line 665 of file usbh_core.h.

The documentation for this struct was generated from the following file:

- UsbHostLib/INCLUDE/usbh_core.h