| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

File List
Here is a list of all files with brief descriptions:
[detail level 123456]

▼ Device |
▼ Nuvoton |
► NUC472_442 |
► Include |
NUC472_442.h | NUC472/NUC442 peripheral access layer header file. This file contains all the peripheral register's definitions, bits definitions and memory mapping for NuMicro NUC472/NUC442 MCU
system_NUC472_442.h | NUC472/NUC442 system clock definition file
► Source |
► GCC |
_syscalls.c |
semihosting.h |
system_NUC472_442.c | NUC472/NUC442 system clock init code and assert handler
▼ SmartcardLib |
▼ Include |
sclib.h | Smartcard library header file
▼ StdDriver |
▼ inc |
acmp.h | NUC472/NUC442 Analog Comparator(ACMP) driver header file
adc.h | NUC472/NUC442 ADC driver header file
can.h | NUC472/NUC442 CAN driver header file
cap.h | NUC470 series Image Capture Driver Header File
clk.h | NUC472/NUC442 CLK Header File
crc.h | NUC472/NUC442 series CRC driver header file
crypto.h | Cryptographic Accelerator driver header file
eadc.h | NUC472/NUC442 EADC driver header file
ebi.h | NUC472/NUC442 EBI driver header file
emac.h | NUC472/NUC442 EMAC driver header file
epwm.h | NUC472/NUC442 EPWM driver header file
fmc.h | NUC472/NUC442 Flash Memory Controller Driver Header File
gpio.h | NUC472/NUC442 GPIO driver header file
i2c.h | NUC472/NUC442 I2C driver header file
i2s.h |
pdma.h | NUC472/NUC442 PDMA driver header file
ps2.h | NUC472/NUC442 PS2 Driver Header File
pwm.h | NUC472/NUC442 PWM driver header file
rtc.h | NUC472/NUC442 RTC driver header file
sc.h | NUC472/NUC442 Smartcard (SC) driver header file
scuart.h |
sd.h | NUC472/NUC442 SD driver header file
spi.h | NUC472/NUC442 SPI driver header file
sys.h | NUC472/NUC442 SYS Header File
timer.h | NUC472/NUC442 TIMER driver header file
uart.h | NUC472/NUC442 UART driver header file
usbd.h | NUC472/NUC442 USBD driver header file
wdt.h | NUC472/NUC442 WDT driver header file
wwdt.h | NUC472/NUC442 WWDT driver header file
▼ src |
acmp.c | NUC472/NUC442 Analog Comparator(ACMP) driver source file
adc.c | NUC472/NUC442 ADC driver source file
can.c | NUC472/NUC442 CAN driver source file
cap.c | NUC472/NUC442 CAP driver source file
clk.c | NUC472/NUC442 CLK driver source file
crc.c | NUC472/NUC442 CRC driver source file
crypto.c | Cryptographic Accelerator driver source file
eadc.c | NUC472/NUC442 EADC driver source file
ebi.c | NUC472/NUC442 EBI driver source file
emac.c | NUC472/NUC442 EMAC driver source file
epwm.c | NUC472/NUC442 EPWM driver source file
fmc.c | NUC472/NUC442 FMC driver source file
gpio.c | NUC472/NUC442 GPIO driver source file
i2c.c | NUC472/NUC442 I2C driver source file
i2s.c |
pdma.c | NUC472/NUC442 PDMA driver source file
ps2.c |
pwm.c | NUC472/NUC442 PWM driver source file
retarget.c | NUC472 Series Debug Port and Semihost Setting Source File
retarget_isp.c |
rtc.c | NUC472/NUC442 RTC driver source file
sc.c | NUC472/NUC442 Smartcard(SC) driver source file
scuart.c | NUC472/NUC442 Smartcard UART mode (SCUART) driver source file
sd.c | NUC472/NUC442 SD driver source file
spi.c | NUC472/NUC442 SPI driver source file
sys.c | NUC472/NUC442 SYS driver source file
timer.c | NUC472/NUC442 TIMER driver source file
uart.c | NUC472/NUC442 UART driver source file
usbd.c | NUC472/NUC442 USBD driver source file
wdt.c | NUC472/NUC442 WDT driver source file
wwdt.c | NUC472/NUC442 WWDT driver source file
▼ UsbHostLib |
▼ INCLUDE |
► inc_mass |
Umas.h |
UmasProtocol.h |
UmasScsi.h |
UmasScsiGlue.h |
UmasTransport.h |
unusual_devs.h |
usbh_config.h | USB Host core configuration file
usbh_core.h | USB Host core driver header file
usbh_err_code.h |
usbh_hid.h |
usbh_hub.h |
usbh_list.h |
usbh_ohci.h |
usbh_uac.h |
usbh_umas.h | USB Host Mass Storage driver header file
▼ SOURCE |
► AUDIOCLASS |
uac.h |
uac_core.c |
uac_driver.c | NUC472/NUC442 MCU USB Host Audio Class driver
uac_parser.c | NUC472/NUC442 MCU USB Host Audio Class driver
► Core |
usbh_core.c | NUC472/NUC442 MCU USB Host Library core
usbh_debug.c | NUC472/NUC442 MCU USB Host library
usbh_hub.c | NUC472/NUC442 MCU USB Host Library Hub class driver
usbh_ohci.c | NUC472/NUC442 MCU USB Host OHCI driver
usbh_support.c |
► Hid |
hid_core.c | NUC472/NUC442 MCU USB Host HID library core
hid_driver.c | NUC472/NUC442 MCU USB Host HID driver
► LW_HCD |
lw_umass.c | Light-weight USB mass storage class driver
lw_umass.h |
lw_usbh.c | Light-Weight USB Host driver
lw_usbh.h |
usb.h |
► MassStor |
Umas_FATFS.c | NUC472/NUC442 MCU USB Host Mass Storage driver for FATFS
UmasDebug.c | NUC472/NUC442 MCU USB Host Mass Storage Library
UmasDriver.c | NUC472/NUC442 MCU USB Host Mass Storage Library
UmasProtocol.c | NUC472/NUC442 MCU USB Host Mass Storage Library
UmasTransport.c | NUC472/NUC442 MCU USB Host Mass Storage driver