| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
EADC_T Struct Reference

`#include <NUC472_442.h>`

## Data Fields
__I uint32_t | AD0DAT0
__I uint32_t | AD0DAT1
__I uint32_t | AD0DAT2
__I uint32_t | AD0DAT3
__I uint32_t | AD0DAT4
__I uint32_t | AD0DAT5
__I uint32_t | AD0DAT6
__I uint32_t | AD0DAT7
__I uint32_t | AD1DAT0
__I uint32_t | AD1DAT1
__I uint32_t | AD1DAT2
__I uint32_t | AD1DAT3
__I uint32_t | AD1DAT4
__I uint32_t | AD1DAT5
__I uint32_t | AD1DAT6
__I uint32_t | AD1DAT7
__IO uint32_t | CTL
__O uint32_t | SWTRG
__I uint32_t | PENDSTS
__IO uint32_t | ADIFOV
__IO uint32_t | OVSTS
__IO uint32_t | AD0SPCTL0
__IO uint32_t | AD0SPCTL1
__IO uint32_t | AD0SPCTL2
__IO uint32_t | AD0SPCTL3
__IO uint32_t | AD0SPCTL4
__IO uint32_t | AD0SPCTL5
__IO uint32_t | AD0SPCTL6
__IO uint32_t | AD0SPCTL7
__IO uint32_t | AD1SPCTL0
__IO uint32_t | AD1SPCTL1
__IO uint32_t | AD1SPCTL2
__IO uint32_t | AD1SPCTL3
__IO uint32_t | AD1SPCTL4
__IO uint32_t | AD1SPCTL5
__IO uint32_t | AD1SPCTL6
__IO uint32_t | AD1SPCTL7
__IO uint32_t | SIMUSEL
__IO uint32_t | CMP [2]
__I uint32_t | STATUS0
__IO uint32_t | STATUS1
__IO uint32_t | EXTSMPT
__I uint32_t | AD0DDAT0
__I uint32_t | AD0DDAT1
__I uint32_t | AD0DDAT2
__I uint32_t | AD0DDAT3
__I uint32_t | AD1DDAT0
__I uint32_t | AD1DDAT1
__I uint32_t | AD1DDAT2
__I uint32_t | AD1DDAT3
__IO uint32_t | DBMEN
__IO uint32_t | INTSRC [4]
__IO uint32_t | AD0TRGEN0
__IO uint32_t | AD0TRGEN1
__IO uint32_t | AD0TRGEN2
__IO uint32_t | AD0TRGEN3
__IO uint32_t | AD1TRGEN0
__IO uint32_t | AD1TRGEN1
__IO uint32_t | AD1TRGEN2
__IO uint32_t | AD1TRGEN3

## Detailed Description

    @addtogroup EADC Enhanced Analog to Digital Converter(EADC)
    Memory Mapped Structure for EADC Controller

Definition at line 7417 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h