| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
SPI_T Struct Reference

`#include <NUC472_442.h>`

## Data Fields
__IO uint32_t | CTL
__IO uint32_t | CLKDIV
__IO uint32_t | SSCTL
__IO uint32_t | PDMACTL
__IO uint32_t | FIFOCTL
__IO uint32_t | STATUS
__O uint32_t | TX
__I uint32_t | RX

## Detailed Description

    @addtogroup SPI Serial Peripheral Interface Controller(SPI)
    Memory Mapped Structure for SPI Controller

Definition at line 22695 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h