| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Functions
usbd.c File Reference

NUC472/NUC442 USBD driver source file. More...

`#include "NUC472_442.h"`
Include dependency graph for usbd.c:

Go to the source code of this file.

## Functions
void | USBD_Open (S_USBD_INFO_T *param, CLASS_REQ pfnClassReq, SET_INTERFACE_REQ pfnSetInterface)
| USBD Initial. More...
void | USBD_Start (void)
| USBD Start. More...
void | USBD_ProcessSetupPacket (void)
| Process Setup Packet. More...
int | USBD_GetDescriptor (void)
| Get Descriptor request. More...
void | USBD_StandardRequest (void)
| Process USB standard request. More...
void | USBD_UpdateDeviceState (void)
| Update Device State. More...
void | USBD_PrepareCtrlIn (uint8_t *pu8Buf, uint32_t u32Size)
| Prepare Control IN transaction. More...
void | USBD_CtrlIn (void)
| Start Control IN transfer. More...
void | USBD_CtrlOut (uint8_t *pu8Buf, uint32_t u32Size)
| Start Control OUT transaction. More...
void | USBD_SwReset (void)
| Clear all software flags. More...
void | USBD_SetVendorRequest (VENDOR_REQ pfnVendorReq)
| USBD Set Vendor Request. More...

## Detailed Description

NUC472/NUC442 USBD driver source file.

Version
  V1.00

Revision
  18

Date
  15/11/30 1:41p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2014 Nuvoton Technology Corp. All rights reserved.

Definition in file usbd.c.