| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Macros | Functions
EMAC Exported Functions
NUC472/NUC442 Device Driver » EMAC Driver » EMAC Exported Constants
Collaboration diagram for EMAC Exported Functions:

## Macros
#define | EMAC_ENABLE_TX()
| Enable EMAC Tx function. More...
#define | EMAC_ENABLE_RX()
| Enable EMAC Rx function. More...
#define | EMAC_DISABLE_TX()
| Disable EMAC Tx function. More...
#define | EMAC_DISABLE_RX()
| Disable EMAC Rx function. More...
#define | EMAC_ENABLE_MAGIC_PKT_WAKEUP()
| Enable EMAC Magic Packet Wakeup function. More...
#define | EMAC_DISABLE_MAGIC_PKT_WAKEUP()
| Disable EMAC Magic Packet Wakeup function. More...
#define | EMAC_ENABLE_MII_INTF()
| Enable EMAC MII interface. More...
#define | EMAC_ENABLE_RECV_BCASTPKT()
| Enable EMAC to receive broadcast packets. More...
#define | EMAC_DISABLE_RECV_BCASTPKT()
| Disable EMAC to receive broadcast packets. More...
#define | EMAC_ENABLE_RECV_MCASTPKT()
| Enable EMAC to receive multicast packets. More...
#define | EMAC_DISABLE_RECV_MCASTPKT()
| Disable EMAC Magic Packet Wakeup function. More...
#define | EMAC_GET_ALARM_FLAG()
| Check if EMAC time stamp alarm interrupt occurred or not. More...
#define | EMAC_CLR_ALARM_FLAG()
| Clear EMAC time stamp alarm interrupt flag. More...

## Functions
int32_t | EMAC_Open (uint8_t *pu8MacAddr)
| Initialize EMAC interface, including descriptors, MAC address, and PHY. More...
void | EMAC_Close (void)
| This function stop all receive and transmit activity and disable MAC interface. More...
void | EMAC_SetMacAddr (uint8_t *pu8MacAddr)
| Set the device MAC address. More...
void | EMAC_EnableCamEntry (uint32_t u32Entry, uint8_t *pu8MacAddr)
| Fill a CAM entry for MAC address comparison. More...
void | EMAC_DisableCamEntry (uint32_t u32Entry)
| Disable a specified CAM entry. More...
uint32_t | EMAC_RecvPkt (uint8_t *pu8Data, uint32_t *pu32Size)
| Receive an Ethernet packet. More...
uint32_t | EMAC_RecvPktTS (uint8_t *pu8Data, uint32_t *pu32Size, uint32_t *pu32Sec, uint32_t *pu32Nsec)
| Receive an Ethernet packet and the time stamp while it's received. More...
void | EMAC_RecvPktDone (void)
| Clean up process after a packet is received. More...
uint32_t | EMAC_SendPkt (uint8_t *pu8Data, uint32_t u32Size)
| Send an Ethernet packet. More...
uint32_t | EMAC_SendPktDone (void)
| Clean up process after packet(s) are sent. More...
uint32_t | EMAC_SendPktDoneTS (uint32_t *pu32Sec, uint32_t *pu32Nsec)
| Clean up process after a packet is sent, and get the time stamp while packet is sent. More...
void | EMAC_EnableTS (uint32_t u32Sec, uint32_t u32Nsec)
| Enable IEEE1588 time stamp function and set current time. More...
void | EMAC_DisableTS (void)
| Disable IEEE1588 time stamp function. More...
void | EMAC_GetTime (uint32_t *pu32Sec, uint32_t *pu32Nsec)
| Get current time stamp. More...
void | EMAC_SetTime (uint32_t u32Sec, uint32_t u32Nsec)
| Set current time stamp. More...
void | EMAC_UpdateTime (uint32_t u32Neg, uint32_t u32Sec, uint32_t u32Nsec)
| Add a offset to current time. More...
void | EMAC_EnableAlarm (uint32_t u32Sec, uint32_t u32Nsec)
| Enable alarm function and set alarm time. More...
void | EMAC_DisableAlarm (void)
| Disable alarm function. More...

## Detailed Description

## Macro Definition Documentation

## ◆ EMAC_CLR_ALARM_FLAG

#define EMAC_CLR_ALARM_FLAG | ( |  | ) |

Clear EMAC time stamp alarm interrupt flag.

Parameters

  None |

Returns
  None

Definition at line 159 of file emac.h.

## ◆ EMAC_DISABLE_MAGIC_PKT_WAKEUP

#define EMAC_DISABLE_MAGIC_PKT_WAKEUP | ( |  | ) |

Disable EMAC Magic Packet Wakeup function.

Parameters

  None |

Returns
  None

Definition at line 99 of file emac.h.

## ◆ EMAC_DISABLE_RECV_BCASTPKT

#define EMAC_DISABLE_RECV_BCASTPKT | ( |  | ) |

Disable EMAC to receive broadcast packets.

Parameters

  None |

Returns
  None

Definition at line 125 of file emac.h.

## ◆ EMAC_DISABLE_RECV_MCASTPKT

#define EMAC_DISABLE_RECV_MCASTPKT | ( |  | ) |

Disable EMAC Magic Packet Wakeup function.

Parameters

  None |

Returns
  None

Definition at line 141 of file emac.h.

## ◆ EMAC_DISABLE_RX

#define EMAC_DISABLE_RX | ( |  | ) |

Disable EMAC Rx function.

Parameters

  None |

Returns
  None

Definition at line 82 of file emac.h.

## ◆ EMAC_DISABLE_TX

#define EMAC_DISABLE_TX | ( |  | ) |

Disable EMAC Tx function.

Parameters

  None |

Returns
  None

Definition at line 73 of file emac.h.

## ◆ EMAC_ENABLE_MAGIC_PKT_WAKEUP

#define EMAC_ENABLE_MAGIC_PKT_WAKEUP | ( |  | ) |

Enable EMAC Magic Packet Wakeup function.

Parameters

  None |

Returns
  None

Definition at line 90 of file emac.h.

## ◆ EMAC_ENABLE_MII_INTF

#define EMAC_ENABLE_MII_INTF | ( |  | ) |

Enable EMAC MII interface.

Parameters

  None |

Returns
  None

After calling EMAC_Open, EMAC use RMII interface by default, but can switch to MII interface by calling this macro

Definition at line 109 of file emac.h.

## ◆ EMAC_ENABLE_RECV_BCASTPKT

#define EMAC_ENABLE_RECV_BCASTPKT | ( |  | ) |

Enable EMAC to receive broadcast packets.

Parameters

  None |

Returns
  None

Definition at line 117 of file emac.h.

## ◆ EMAC_ENABLE_RECV_MCASTPKT

#define EMAC_ENABLE_RECV_MCASTPKT | ( |  | ) |

Enable EMAC to receive multicast packets.

Parameters

  None |

Returns
  None

Definition at line 133 of file emac.h.

## ◆ EMAC_ENABLE_RX

#define EMAC_ENABLE_RX | ( |  | ) |

Enable EMAC Rx function.

Parameters

  None |

Returns
  None

Definition at line 65 of file emac.h.

## ◆ EMAC_ENABLE_TX

#define EMAC_ENABLE_TX | ( |  | ) |

Enable EMAC Tx function.

Parameters

  None |

Returns
  None

Definition at line 56 of file emac.h.

## ◆ EMAC_GET_ALARM_FLAG

#define EMAC_GET_ALARM_FLAG | ( |  | ) |

Check if EMAC time stamp alarm interrupt occurred or not.

Parameters

  None |

Returns
  If time stamp alarm interrupt occurred or not

Return values

  0 | Alarm interrupt does not occur
  1 | Alarm interrupt occurred

Definition at line 151 of file emac.h.

## Function Documentation

## ◆ EMAC_Close()

void EMAC_Close | ( | void |  | ) |

This function stop all receive and transmit activity and disable MAC interface.

Parameters

  None |

Returns
  None

Definition at line 456 of file emac.c.

## ◆ EMAC_DisableAlarm()

void EMAC_DisableAlarm | ( | void |  | ) |

Disable alarm function.

Parameters

  None |

Returns
  None

Definition at line 959 of file emac.c.

## ◆ EMAC_DisableCamEntry()

void EMAC_DisableCamEntry | ( | uint32_t | u32Entry | ) |

Disable a specified CAM entry.

Parameters

  [in] | u32Entry | CAM entry to be disabled

Returns
  None

Definition at line 500 of file emac.c.

## ◆ EMAC_DisableTS()

void EMAC_DisableTS | ( | void |  | ) |

Disable IEEE1588 time stamp function.

Parameters

  None |

Returns
  None

Definition at line 905 of file emac.c.

## ◆ EMAC_EnableAlarm()

void EMAC_EnableAlarm | ( | uint32_t | u32Sec,
|  | uint32_t | u32Nsec
| ) |  |

Enable alarm function and set alarm time.

Parameters

  [in] | u32Sec | Second value to trigger alarm
  [in] | u32Nsec | Nano second value to trigger alarm

Returns
  None

Definition at line 945 of file emac.c.

## ◆ EMAC_EnableCamEntry()

void EMAC_EnableCamEntry | ( | uint32_t | u32Entry,
|  | uint8_t * | pu8MacAddr
| ) |  |

Fill a CAM entry for MAC address comparison.

Parameters

  [in] | u32Entry | MAC entry to fill. Entry 0 is used to store device MAC address, do not overwrite the setting in it.
  [in] | pu8MacAddr | Pointer to uint8_t array holds MAC address

Returns
  None

Definition at line 478 of file emac.c.

Here is the caller graph for this function:

## ◆ EMAC_EnableTS()

void EMAC_EnableTS | ( | uint32_t | u32Sec,
|  | uint32_t | u32Nsec
| ) |  |

Enable IEEE1588 time stamp function and set current time.

Parameters

  [in] | u32Sec | Second value
  [in] | u32Nsec | Nano second value

Returns
  None

Definition at line 877 of file emac.c.

Here is the call graph for this function:

## ◆ EMAC_GetTime()

void EMAC_GetTime | ( | uint32_t * | pu32Sec,
|  | uint32_t * | pu32Nsec
| ) |  |

Get current time stamp.

Parameters

  [out] | pu32Sec | Current second value
  [out] | pu32Nsec | Current nano second value

Returns
  None

Definition at line 916 of file emac.c.

## ◆ EMAC_Open()

int32_t EMAC_Open | ( | uint8_t * | pu8MacAddr | ) |

Initialize EMAC interface, including descriptors, MAC address, and PHY.

Parameters

  [in] | pu8MacAddr | Pointer to uint8_t array holds MAC address

Return values

  0 | success
  EMAC_TIMEOUT_ERR | Initial PHY and auto-negotiation failed due to timeout error

Note
  This API sets EMAC to work in RMII mode, but could configure to MII mode later with EMAC_ENABLE_MII_INTF macro
  This API configures EMAC to receive all broadcast and multicast packets, but could configure to other settings with EMAC_ENABLE_RECV_BCASTPKT, EMAC_DISABLE_RECV_BCASTPKT, EMAC_ENABLE_RECV_MCASTPKT, and EMAC_DISABLE_RECV_MCASTPKT
  Receive(RX) and transmit(TX) are not enabled yet, application must call EMAC_ENABLE_RX and EMAC_ENABLE_TX to enable receive and transmit function.

Definition at line 417 of file emac.c.

Here is the call graph for this function:

## ◆ EMAC_RecvPkt()

uint32_t EMAC_RecvPkt | ( | uint8_t * | pu8Data,
|  | uint32_t * | pu32Size
| ) |  |

Receive an Ethernet packet.

Parameters

  [in] | pu8Data | Pointer to a buffer to store received packet (4 byte CRC removed)
  [in] | pu32Size | Received packet size (without 4 byte CRC).

Returns
  Packet receive success or not

Return values

  0 | No packet available for receive
  1 | A packet is received
  EMAC_BUS_ERR | Bus error

Note
  Return 0 doesn't guarantee the packet will be sent and received successfully.

Definition at line 516 of file emac.c.

## ◆ EMAC_RecvPktDone()

void EMAC_RecvPktDone | ( | void |  | ) |

Clean up process after a packet is received.

Parameters

  None |

Returns
  None

EMAC Rx interrupt service routine must call this API to release the resource use by receive process

Note
  Application can only call this function once every time EMAC_RecvPkt or EMAC_RecvPktTS returns 1

Definition at line 649 of file emac.c.

## ◆ EMAC_RecvPktTS()

uint32_t EMAC_RecvPktTS | ( | uint8_t * | pu8Data,
|  | uint32_t * | pu32Size,
|  | uint32_t * | pu32Sec,
|  | uint32_t * | pu32Nsec
| ) |  |

Receive an Ethernet packet and the time stamp while it's received.

Parameters

  [out] | pu8Data | Pointer to a buffer to store received packet (4 byte CRC removed)
  [out] | pu32Size | Received packet size (without 4 byte CRC).
  [out] | pu32Sec | Second value while packet sent
  [out] | pu32Nsec | Nano second value while packet sent

Returns
  Packet receive success or not

Return values

  0 | No packet available for receive
  1 | A packet is received
  EMAC_BUS_ERR | Bus error

Note
  Return 0 doesn't guarantee the packet will be sent and received successfully.
  Largest Ethernet packet is 1514 bytes after stripped CRC, application must give a buffer large enough to store such packet

Definition at line 584 of file emac.c.

## ◆ EMAC_SendPkt()

uint32_t EMAC_SendPkt | ( | uint8_t * | pu8Data,
|  | uint32_t | u32Size
| ) |  |

Send an Ethernet packet.

Parameters

  [in] | pu8Data | Pointer to a buffer holds the packet to transmit
  [in] | u32Size | Packet size (without 4 byte CRC).

Returns
  Packet transmit success or not

Return values

  0 | Transmit failed due to descriptor unavailable.
  1 | Packet is copied to descriptor and triggered to transmit.

Note
  Return 1 doesn't guarantee the packet will be sent and received successfully.

Definition at line 682 of file emac.c.

## ◆ EMAC_SendPktDone()

uint32_t EMAC_SendPktDone | ( | void |  | ) |

Clean up process after packet(s) are sent.

Parameters

  None |

Returns
  Number of packet sent between two function calls

Return values

  EMAC_BUS_ERR | Bus error
  Otherwise | Number of packet sent between two function calls

EMAC Tx interrupt service routine must call this API or EMAC_SendPktDoneTS to release the resource use by transmit process

Definition at line 723 of file emac.c.

## ◆ EMAC_SendPktDoneTS()

uint32_t EMAC_SendPktDoneTS | ( | uint32_t * | pu32Sec,
|  | uint32_t * | pu32Nsec
| ) |  |

Clean up process after a packet is sent, and get the time stamp while packet is sent.

Parameters

  [in] | pu32Sec | Second value while packet sent
  [in] | pu32Nsec | Nano second value while packet sent

Returns
  If a packet sent successfully

Return values

  0 | No packet sent successfully, and the value in *pu32Sec and *pu32Nsec are meaningless
  1 | A packet sent successfully, and the value in *pu32Sec and *pu32Nsec is the time stamp while packet sent
  EMAC_BUS_ERR | Bus error

EMAC Tx interrupt service routine must call this API or EMAC_SendPktDone to release the resource use by transmit process

Definition at line 802 of file emac.c.

## ◆ EMAC_SetMacAddr()

void EMAC_SetMacAddr | ( | uint8_t * | pu8MacAddr | ) |

Set the device MAC address.

Parameters

  [in] | pu8MacAddr | Pointer to uint8_t array holds MAC address

Returns
  None

Definition at line 466 of file emac.c.

Here is the call graph for this function:
Here is the caller graph for this function:

## ◆ EMAC_SetTime()

void EMAC_SetTime | ( | uint32_t | u32Sec,
|  | uint32_t | u32Nsec
| ) |  |

Set current time stamp.

Parameters

  [in] | u32Sec | Second value
  [in] | u32Nsec | Nano second value

Returns
  None

Definition at line 929 of file emac.c.

## ◆ EMAC_UpdateTime()

void EMAC_UpdateTime | ( | uint32_t | u32Neg,
|  | uint32_t | u32Sec,
|  | uint32_t | u32Nsec
| ) |  |

Add a offset to current time.

Parameters

  [in] | u32Neg | Offset is negative value (u32Neg == 1) or positive value (u32Neg == 0).
  [in] | u32Sec | Second value to add to current time
  [in] | u32Nsec | Nano second value to add to current time

Returns
  None

Definition at line 973 of file emac.c.