<map id="StdDriver/inc/timer.h" name="StdDriver/inc/timer.h">
<area shape="rect" id="node1" title="NUC472/NUC442 TIMER driver header file." alt="" coords="3601,5,3739,32"/>
<area shape="rect" id="node2" href="$da/d08/_n_u_c472__442_8h.html" title="NUC472/NUC442 peripheral access layer header file. This file contains all the peripheral register&#39;s d..." alt="" coords="3577,80,3763,121"/>
<area shape="rect" id="node3" href="$d6/d83/system___n_u_c472__442_8c.html" title="NUC472/NUC442 system clock init code and assert handler." alt="" coords="5,169,241,211"/>
<area shape="rect" id="node4" href="$d8/de4/sclib_8h.html" title="Smartcard library header file." alt="" coords="266,169,410,211"/>
<area shape="rect" id="node5" href="$d1/da9/i2s_8h.html" title=" " alt="" coords="435,177,561,203"/>
<area shape="rect" id="node6" href="$d8/d29/ps2_8h.html" title="NUC472/NUC442 PS2 Driver Header File." alt="" coords="586,177,717,203"/>
<area shape="rect" id="node7" href="$d8/db0/ps2_8c.html" title=" " alt="" coords="636,259,768,285"/>
<area shape="rect" id="node8" href="$d3/df1/acmp_8c.html" title="NUC472/NUC442 Analog Comparator(ACMP) driver source file." alt="" coords="792,177,935,203"/>
<area shape="rect" id="node9" href="$de/d01/adc_8c.html" title="NUC472/NUC442 ADC driver source file." alt="" coords="959,177,1091,203"/>
<area shape="rect" id="node10" href="$d0/dd7/can_8c.html" title="NUC472/NUC442 CAN driver source file." alt="" coords="1115,177,1247,203"/>
<area shape="rect" id="node11" href="$da/d9b/cap_8c.html" title="NUC472/NUC442 CAP driver source file." alt="" coords="1271,177,1403,203"/>
<area shape="rect" id="node12" href="$de/da0/clk_8c.html" title="NUC472/NUC442 CLK driver source file." alt="" coords="1427,177,1555,203"/>
<area shape="rect" id="node13" href="$d8/d13/crc_8c.html" title="NUC472/NUC442 CRC driver source file." alt="" coords="1580,177,1709,203"/>
<area shape="rect" id="node14" href="$df/dee/crypto_8c.html" title="Cryptographic Accelerator driver source file." alt="" coords="1734,177,1881,203"/>
<area shape="rect" id="node15" href="$d2/d01/eadc_8c.html" title="NUC472/NUC442 EADC driver source file." alt="" coords="1905,177,2043,203"/>
<area shape="rect" id="node16" href="$d1/d7e/ebi_8c.html" title="NUC472/NUC442 EBI driver source file." alt="" coords="2067,177,2195,203"/>
<area shape="rect" id="node17" href="$dc/def/emac_8c.html" title="NUC472/NUC442 EMAC driver source file." alt="" coords="2220,177,2363,203"/>
<area shape="rect" id="node18" href="$de/d46/epwm_8c.html" title="NUC472/NUC442 EPWM driver source file." alt="" coords="2387,177,2532,203"/>
<area shape="rect" id="node19" href="$d0/dbc/fmc_8c.html" title="NUC472/NUC442 FMC driver source file." alt="" coords="2556,177,2688,203"/>
<area shape="rect" id="node20" href="$d8/da0/gpio_8c.html" title="NUC472/NUC442 GPIO driver source file." alt="" coords="2712,177,2847,203"/>
<area shape="rect" id="node21" href="$d9/dcb/i2c_8c.html" title="NUC472/NUC442 I2C driver source file." alt="" coords="2871,177,2999,203"/>
<area shape="rect" id="node22" href="$d8/d6d/i2s_8c.html" title=" " alt="" coords="3023,177,3151,203"/>
<area shape="rect" id="node23" href="$d2/d14/pdma_8c.html" title="NUC472/NUC442 PDMA driver source file." alt="" coords="3176,177,3319,203"/>
<area shape="rect" id="node24" href="$de/d5c/pwm_8c.html" title="NUC472/NUC442 PWM driver source file." alt="" coords="3343,177,3482,203"/>
<area shape="rect" id="node25" href="$d3/d3d/retarget_8c.html" title="NUC472 Series Debug Port and Semihost Setting Source File." alt="" coords="3506,177,3661,203"/>
<area shape="rect" id="node26" href="$dd/d5b/retarget__isp_8c.html" title=" " alt="" coords="3685,169,3829,211"/>
<area shape="rect" id="node27" href="$d4/dcc/rtc_8c.html" title="NUC472/NUC442 RTC driver source file." alt="" coords="3853,177,3980,203"/>
<area shape="rect" id="node28" href="$df/d60/sc_8c.html" title="NUC472/NUC442 Smartcard(SC) driver source file." alt="" coords="4005,177,4130,203"/>
<area shape="rect" id="node29" href="$df/d4a/scuart_8c.html" title="NUC472/NUC442 Smartcard UART mode (SCUART) driver source file." alt="" coords="4154,177,4301,203"/>
<area shape="rect" id="node30" href="$df/d7c/sd_8c.html" title="NUC472/NUC442 SD driver source file." alt="" coords="4325,177,4450,203"/>
<area shape="rect" id="node31" href="$da/d00/spi_8c.html" title="NUC472/NUC442 SPI driver source file." alt="" coords="4474,177,4602,203"/>
<area shape="rect" id="node32" href="$d8/d91/sys_8c.html" title="NUC472/NUC442 SYS driver source file." alt="" coords="4627,177,4759,203"/>
<area shape="rect" id="node33" href="$df/d41/timer_8c.html" title="NUC472/NUC442 TIMER driver source file." alt="" coords="4783,177,4923,203"/>
<area shape="rect" id="node34" href="$d1/d87/uart_8c.html" title="NUC472/NUC442 UART driver source file." alt="" coords="4947,177,5081,203"/>
<area shape="rect" id="node35" href="$dc/dd9/usbd_8c.html" title="NUC472/NUC442 USBD driver source file." alt="" coords="5105,177,5243,203"/>
<area shape="rect" id="node36" href="$db/d1a/wdt_8c.html" title="NUC472/NUC442 WDT driver source file." alt="" coords="5267,177,5398,203"/>
<area shape="rect" id="node37" href="$d9/d90/wwdt_8c.html" title="NUC472/NUC442 WWDT driver source file." alt="" coords="5423,177,5563,203"/>
<area shape="rect" id="node38" href="$da/dca/uac__core_8c.html" title=" " alt="" coords="5587,169,5822,211"/>
<area shape="rect" id="node39" href="$da/dd9/uac__driver_8c.html" title="NUC472/NUC442 MCU USB Host Audio Class driver." alt="" coords="5846,169,6081,211"/>
<area shape="rect" id="node40" href="$dc/dea/uac__parser_8c.html" title="NUC472/NUC442 MCU USB Host Audio Class driver." alt="" coords="6105,169,6339,211"/>
<area shape="rect" id="node41" href="$de/d48/usbh__core_8c.html" title="NUC472/NUC442 MCU USB Host Library core." alt="" coords="6363,169,6542,211"/>
<area shape="rect" id="node42" href="$da/df8/usbh__debug_8c.html" title="NUC472/NUC442 MCU USB Host library." alt="" coords="6566,169,6745,211"/>
<area shape="rect" id="node43" href="$db/dee/usbh__hub_8c.html" title="NUC472/NUC442 MCU USB Host Library Hub class driver." alt="" coords="6769,169,6947,211"/>
<area shape="rect" id="node44" href="$d2/d1c/usbh__ohci_8c.html" title="NUC472/NUC442 MCU USB Host OHCI driver." alt="" coords="6971,169,7150,211"/>
<area shape="rect" id="node45" href="$d5/d7e/usbh__support_8c.html" title=" " alt="" coords="7174,169,7353,211"/>
<area shape="rect" id="node46" href="$d0/d8a/hid__core_8c.html" title="NUC472/NUC442 MCU USB Host HID library core." alt="" coords="7377,169,7547,211"/>
<area shape="rect" id="node47" href="$d3/d98/hid__driver_8c.html" title="NUC472/NUC442 MCU USB Host HID driver." alt="" coords="7571,169,7742,211"/>
<area shape="rect" id="node48" href="$d8/d4b/lw__umass_8c.html" title="Light&#45;weight USB mass storage class driver." alt="" coords="7767,169,7939,211"/>
<area shape="rect" id="node49" href="$d8/d25/lw__usbh_8c.html" title="Light&#45;Weight USB Host driver." alt="" coords="7963,169,8135,211"/>
<area shape="rect" id="node50" href="$d0/d4c/_umas_debug_8c.html" title="NUC472/NUC442 MCU USB Host Mass Storage Library." alt="" coords="8159,169,8367,211"/>
</map>
