| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Macros | Functions
adc.h File Reference

NUC472/NUC442 ADC driver header file. More...

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Macros
#define | ADC_CH_0_MASK
#define | ADC_CH_1_MASK
#define | ADC_CH_2_MASK
#define | ADC_CH_3_MASK
#define | ADC_CH_4_MASK
#define | ADC_CH_5_MASK
#define | ADC_CH_6_MASK
#define | ADC_CH_7_MASK
#define | ADC_CH_8_MASK
#define | ADC_CH_9_MASK
#define | ADC_CH_10_MASK
#define | ADC_CH_11_MASK
#define | ADC_CH_BG_MASK
#define | ADC_CH_TS_MASK
#define | ADC_CMP_LESS_THAN
#define | ADC_CMP_GREATER_OR_EQUAL_TO
#define | ADC_TRIGGER_BY_EXT_PIN
#define | ADC_TRIGGER_BY_PWM
#define | ADC_LOW_LEVEL_TRIGGER
#define | ADC_HIGH_LEVEL_TRIGGER
#define | ADC_FALLING_EDGE_TRIGGER
#define | ADC_RISING_EDGE_TRIGGER
#define | ADC_ADF_INT
#define | ADC_CMP0_INT
#define | ADC_CMP1_INT
#define | ADC_INPUT_MODE_SINGLE_END
#define | ADC_INPUT_MODE_DIFFERENTIAL
#define | ADC_OPERATION_MODE_SINGLE
#define | ADC_OPERATION_MODE_SINGLE_CYCLE
#define | ADC_OPERATION_MODE_CONTINUOUS
#define | ADC_DMODE_OUT_FORMAT_UNSIGNED
#define | ADC_DMODE_OUT_FORMAT_2COMPLEMENT
#define | ADC_GET_CONVERSION_DATA(adc, u32ChNum)
| Get the latest ADC conversion data. More...
#define | ADC_GET_INT_FLAG(adc, u32Mask)
| Return the user-specified interrupt flags. More...
#define | ADC_CLR_INT_FLAG(adc, u32Mask)
| This macro clear the selected interrupt status bits. More...
#define | ADC_IS_BUSY(adc)
| Get the busy state of ADC. More...
#define | ADC_IS_DATA_OVERRUN(adc, u32ChNum)
| Check if the ADC conversion data is over written or not. More...
#define | ADC_IS_DATA_VALID(adc, u32ChNum)
| Check if the ADC conversion data is valid or not. More...
#define | ADC_POWER_DOWN(adc)
| Power down ADC module. More...
#define | ADC_POWER_ON(adc)
| Power on ADC module. More...
#define | ADC_ENABLE_CMP0(adc, u32ChNum, u32Condition, u32Data, u32MatchCount)
| Configure the comparator 0 and enable it. More...
#define | ADC_DISABLE_CMP0(adc)
| Disable comparator 0. More...
#define | ADC_ENABLE_CMP1(adc, u32ChNum, u32Condition, u32Data, u32MatchCount)
| Configure the comparator 1 and enable it. More...
#define | ADC_DISABLE_CMP1(adc)
| Disable comparator 1. More...
#define | ADC_SET_INPUT_CHANNEL(adc, u32Mask)
| Set ADC input channel. Enabled channel will be converted while ADC starts. More...
#define | ADC_START_CONV(adc)
| Start the A/D conversion. More...
#define | ADC_STOP_CONV(adc)
| Stop the A/D conversion. More...
#define | ADC_SET_DMOF(adc, u32Format)
| Set the output format in differential input mode. More...
#define | ADC_ENABLE_PDMA(adc)
| Enable PDMA transfer. More...
#define | ADC_DISABLE_PDMA(adc)
| Disable PDMA transfer. More...
#define | ADC_GET_PDMA_DATA(adc)
| Get PDMA current transfer data. More...

## Functions
void | ADC_Open (ADC_T *adc, uint32_t u32InputMode, uint32_t u32OpMode, uint32_t u32ChMask)
| This API configures ADC module to be ready for convert the input from selected channel. More...
void | ADC_Close (ADC_T *adc)
| Disable ADC module. More...
void | ADC_EnableHWTrigger (ADC_T *adc, uint32_t u32Source, uint32_t u32Param)
| Configure the hardware trigger condition and enable hardware trigger. More...
void | ADC_DisableHWTrigger (ADC_T *adc)
| Disable hardware trigger ADC function. More...
void | ADC_EnableInt (ADC_T *adc, uint32_t u32Mask)
| Enable the interrupt(s) selected by u32Mask parameter. More...
void | ADC_DisableInt (ADC_T *adc, uint32_t u32Mask)
| Disable the interrupt(s) selected by u32Mask parameter. More...

## Detailed Description

NUC472/NUC442 ADC driver header file.

Version
  V1.00

Revision
  23

Date
  15/11/16 2:12p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013 Nuvoton Technology Corp. All rights reserved.

Definition in file adc.h.