| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
EMAC_T Struct Reference

`#include <NUC472_442.h>`

## Data Fields
__IO uint32_t | CAMCTL
__IO uint32_t | CAMEN
__IO uint32_t | CAM0M
__IO uint32_t | CAM0L
__IO uint32_t | CAM1M
__IO uint32_t | CAM1L
__IO uint32_t | CAM2M
__IO uint32_t | CAM2L
__IO uint32_t | CAM3M
__IO uint32_t | CAM3L
__IO uint32_t | CAM4M
__IO uint32_t | CAM4L
__IO uint32_t | CAM5M
__IO uint32_t | CAM5L
__IO uint32_t | CAM6M
__IO uint32_t | CAM6L
__IO uint32_t | CAM7M
__IO uint32_t | CAM7L
__IO uint32_t | CAM8M
__IO uint32_t | CAM8L
__IO uint32_t | CAM9M
__IO uint32_t | CAM9L
__IO uint32_t | CAM10M
__IO uint32_t | CAM10L
__IO uint32_t | CAM11M
__IO uint32_t | CAM11L
__IO uint32_t | CAM12M
__IO uint32_t | CAM12L
__IO uint32_t | CAM13M
__IO uint32_t | CAM13L
__IO uint32_t | CAM14M
__IO uint32_t | CAM14L
__IO uint32_t | CAM15MSB
__IO uint32_t | CAM15LSB
__IO uint32_t | TXDSA
__IO uint32_t | RXDSA
__IO uint32_t | CTL
__IO uint32_t | MIIMDAT
__IO uint32_t | MIIMCTL
__IO uint32_t | FIFOCTL
__O uint32_t | TXST
__O uint32_t | RXST
__IO uint32_t | MRFL
__IO uint32_t | INTEN
__IO uint32_t | INTSTS
__IO uint32_t | GENSTS
__IO uint32_t | MPCNT
__I uint32_t | RPCNT
__IO uint32_t | FRSTS
__I uint32_t | CTXDSA
__I uint32_t | CTXBSA
__I uint32_t | CRXDSA
__I uint32_t | CRXBSA
__IO uint32_t | TSCTL
__I uint32_t | TSSEC
__I uint32_t | TSSUBSEC
__IO uint32_t | TSINC
__IO uint32_t | TSADDEND
__IO uint32_t | UPDSEC
__IO uint32_t | UPDSUBSEC
__IO uint32_t | ALMSEC
__IO uint32_t | ALMSUBSEC

## Detailed Description

    @addtogroup EMAC Ethernet MAC Controller(EMAC)
    Memory Mapped Structure for EMAC Controller

Definition at line 11751 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h