<map id="SmartcardLib/Include/sclib.h" name="SmartcardLib/Include/sclib.h">
<area shape="rect" id="node1" title="Smartcard library header file." alt="" coords="1431,5,1575,47"/>
<area shape="rect" id="node2" href="$da/d08/_n_u_c472__442_8h.html" title="NUC472/NUC442 peripheral access layer header file. This file contains all the peripheral register&#39;s d..." alt="" coords="1448,95,1557,121"/>
<area shape="rect" id="node3" title=" " alt="" coords="5,169,96,196"/>
<area shape="rect" id="node4" href="$d1/d5e/system___n_u_c472__442_8h.html" title="NUC472/NUC442 system clock definition file." alt="" coords="121,169,279,196"/>
<area shape="rect" id="node5" title=" " alt="" coords="226,244,291,271"/>
<area shape="rect" id="node6" href="$d9/d87/sys_8h.html" title="NUC472/NUC442 SYS Header File." alt="" coords="355,169,410,196"/>
<area shape="rect" id="node7" href="$d3/d89/clk_8h.html" title="NUC472/NUC442 CLK Header File." alt="" coords="435,169,485,196"/>
<area shape="rect" id="node8" href="$dc/d2f/acmp_8h.html" title="NUC472/NUC442 Analog Comparator(ACMP) driver header file." alt="" coords="510,169,575,196"/>
<area shape="rect" id="node9" href="$d7/d19/adc_8h.html" title="NUC472/NUC442 ADC driver header file." alt="" coords="599,169,654,196"/>
<area shape="rect" id="node10" href="$da/da5/eadc_8h.html" title="NUC472/NUC442 EADC driver header file." alt="" coords="679,169,740,196"/>
<area shape="rect" id="node11" href="$d0/dda/cap_8h.html" title="NUC470 series Image Capture Driver Header File." alt="" coords="765,169,819,196"/>
<area shape="rect" id="node12" href="$da/da0/crypto_8h.html" title="Cryptographic Accelerator driver header file." alt="" coords="844,169,913,196"/>
<area shape="rect" id="node13" href="$d1/d47/pdma_8h.html" title="NUC472/NUC442 PDMA driver header file." alt="" coords="938,169,1003,196"/>
<area shape="rect" id="node14" href="$da/d96/ebi_8h.html" title="NUC472/NUC442 EBI driver header file." alt="" coords="1028,169,1079,196"/>
<area shape="rect" id="node15" href="$d6/d55/emac_8h.html" title="NUC472/NUC442 EMAC driver header file." alt="" coords="1103,169,1169,196"/>
<area shape="rect" id="node16" href="$dc/d00/fmc_8h.html" title="NUC472/NUC442 Flash Memory Controller Driver Header File." alt="" coords="1193,169,1247,196"/>
<area shape="rect" id="node17" href="$d6/d7c/gpio_8h.html" title="NUC472/NUC442 GPIO driver header file." alt="" coords="1271,169,1329,196"/>
<area shape="rect" id="node18" href="$d5/daf/i2c_8h.html" title="NUC472/NUC442 I2C driver header file." alt="" coords="1353,169,1404,196"/>
<area shape="rect" id="node19" href="$d6/db9/pwm_8h.html" title="NUC472/NUC442 PWM driver header file." alt="" coords="1429,169,1489,196"/>
<area shape="rect" id="node20" href="$dc/d9b/epwm_8h.html" title="NUC472/NUC442 EPWM driver header file." alt="" coords="1513,169,1580,196"/>
<area shape="rect" id="node21" href="$dc/d1b/rtc_8h.html" title="NUC472/NUC442 RTC driver header file." alt="" coords="1604,169,1652,196"/>
<area shape="rect" id="node22" href="$d9/d50/sc_8h.html" title="NUC472/NUC442 Smartcard (SC) driver header file." alt="" coords="1677,169,1723,196"/>
<area shape="rect" id="node23" href="$dc/d0b/scuart_8h.html" title=" " alt="" coords="1748,169,1817,196"/>
<area shape="rect" id="node24" href="$da/d87/spi_8h.html" title="NUC472/NUC442 SPI driver header file." alt="" coords="1841,169,1892,196"/>
<area shape="rect" id="node25" href="$d5/dd0/timer_8h.html" title="NUC472/NUC442 TIMER driver header file." alt="" coords="1917,169,1979,196"/>
<area shape="rect" id="node26" href="$d2/d86/uart_8h.html" title="NUC472/NUC442 UART driver header file." alt="" coords="2003,169,2058,196"/>
<area shape="rect" id="node27" href="$da/ddf/usbd_8h.html" title="NUC472/NUC442 USBD driver header file." alt="" coords="2083,169,2144,196"/>
<area shape="rect" id="node28" href="$d0/de2/wdt_8h.html" title="NUC472/NUC442 WDT driver header file." alt="" coords="2168,169,2221,196"/>
<area shape="rect" id="node29" href="$dd/d09/wwdt_8h.html" title="NUC472/NUC442 WWDT driver header file." alt="" coords="2246,169,2309,196"/>
<area shape="rect" id="node30" href="$d1/da9/i2s_8h.html" title=" " alt="" coords="2333,169,2384,196"/>
<area shape="rect" id="node31" href="$d7/da8/can_8h.html" title="NUC472/NUC442 CAN driver header file." alt="" coords="2409,169,2463,196"/>
<area shape="rect" id="node32" href="$d6/d23/sd_8h.html" title="NUC472/NUC442 SD driver header file." alt="" coords="2487,169,2534,196"/>
<area shape="rect" id="node34" href="$d8/d29/ps2_8h.html" title="NUC472/NUC442 PS2 Driver Header File." alt="" coords="2558,169,2613,196"/>
<area shape="rect" id="node35" href="$dc/de6/crc_8h.html" title="NUC472/NUC442 series CRC driver header file." alt="" coords="2637,169,2688,196"/>
<area shape="rect" id="node33" title=" " alt="" coords="2480,244,2541,271"/>
</map>
