| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
FMC_T Struct Reference

`#include <NUC472_442.h>`

## Data Fields
__IO uint32_t | ISPCTL
__IO uint32_t | ISPADDR
__IO uint32_t | ISPDAT
__IO uint32_t | ISPCMD
__IO uint32_t | ISPTRG
__I uint32_t | DFBA
__IO uint32_t | FTCTL
__IO uint32_t | ISPSTS
__IO uint32_t | FBWP
__IO uint32_t | MPDAT0
__IO uint32_t | MPDAT1
__IO uint32_t | MPDAT2
__IO uint32_t | MPDAT3
__IO uint32_t | MPSTS
__IO uint32_t | MPADDR

## Detailed Description

    @addtogroup FMC Flash Memory Controller(FMC)
    Memory Mapped Structure for FMC Controller

Definition at line 14590 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h