<map id="USBD_GetStall" name="USBD_GetStall">
<area shape="rect" id="node1" title="Get USB endpoint stall state." alt="" coords="455,5,567,32"/>
<area shape="rect" id="node2" href="$d3/d74/group___n_u_c472__442___u_s_b_d___e_x_p_o_r_t_e_d___f_u_n_c_t_i_o_n_s.html#ga159182802cc4a2a791a5dd4e331f16db" title="Process USB standard request." alt="" coords="241,5,407,32"/>
<area shape="rect" id="node3" href="$d3/d74/group___n_u_c472__442___u_s_b_d___e_x_p_o_r_t_e_d___f_u_n_c_t_i_o_n_s.html#gacd570f497a414e36c393904ad108d3d2" title="Process Setup Packet." alt="" coords="5,5,193,32"/>
</map>
