| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Functions
ps2.c File Reference
`#include <stdio.h>`
`#include "NUC472_442.h"`
`#include "ps2.h"`
Include dependency graph for ps2.c:

Go to the source code of this file.

## Functions
void | PS2_EnableInt (uint32_t u32Mask)
| The function is used to enable PS2 specified interrupt. More...
void | PS2_DisableInt (uint32_t u32Mask)
| The function is used to disable PS2 specified interrupt. More...
void | PS2_Open (void)
| This function use to enable PS2 function and set one byte per trnasfer. More...
void | PS2_Close (void)
| This function use to disable PS2 function. More...
uint8_t | PS2_Read (void)
| This function use to read PS2 Rx data. More...
int32_t | PS2_Write (uint32_t *pu32Buf, uint32_t u32ByteCount)
| This function use to transmit PS2 data. More...