| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Functions
ebi.c File Reference

NUC472/NUC442 EBI driver source file. More...

`#include "NUC472_442.h"`
`#include "ebi.h"`
Include dependency graph for ebi.c:

Go to the source code of this file.

## Functions
void | EBI_Open (uint32_t u32Bank, uint32_t u32DataWidth, uint32_t u32TimingClass, uint32_t u32BusMode, uint32_t u32CSActiveLevel)
| Initialize EBI for Bank 0~3. More...
void | EBI_Close (uint32_t u32Bank)
| Disable EBI for bank 0~3. More...
void | EBI_SetBusTiming (uint32_t u32Bank, uint32_t u32TimingConfig, uint32_t u32MclkDiv)
| Set EBI bus timings. More...
void | EBI_EnableCrypto (uint32_t u32Bank, uint32_t *u32Key)
| Enable encrypt/decrypt function and set key for EBI bank 0~3. More...
void | EBI_DisbleCrypto (uint32_t u32Bank)
| Disable encrypt/decrypt function for EBI bank 0~3. More...

## Detailed Description

NUC472/NUC442 EBI driver source file.

Version
  V0.10

Revision
  8

Date
  15/06/23 5:40p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2014 Nuvoton Technology Corp. All rights reserved.

Definition in file ebi.c.