<map id="CLK_GetHCLKFreq" name="CLK_GetHCLKFreq">
<area shape="rect" id="node1" title="Get HCLK frequency." alt="" coords="176,5,311,32"/>
<area shape="rect" id="node2" href="$d7/d6b/group___n_u_c472__442___e_m_a_c___e_x_p_o_r_t_e_d___f_u_n_c_t_i_o_n_s.html#gaf44ae41597ba26a0100555afdb2f7ff7" title="Enable IEEE1588 time stamp function and set current time." alt="" coords="5,5,128,32"/>
</map>
