| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Modules | Macros
SYS Exported Constants
NUC472/NUC442 Device Driver » SYS Driver
Collaboration diagram for SYS Exported Constants:

## Modules
| SYS Exported Functions

## Macros
#define | PDMA_RST
#define | EBI_RST
#define | USBH_RST
#define | EMAC_RST
#define | SDH_RST
#define | CRC_RST
#define | CAP_RST
#define | CRYPTO_RST
#define | GPIO_RST
#define | TMR0_RST
#define | TMR1_RST
#define | TMR2_RST
#define | TMR3_RST
#define | ACMP_RST
#define | I2C0_RST
#define | I2C1_RST
#define | I2C2_RST
#define | I2C3_RST
#define | SPI0_RST
#define | SPI1_RST
#define | SPI2_RST
#define | SPI3_RST
#define | UART0_RST
#define | UART1_RST
#define | UART2_RST
#define | UART3_RST
#define | UART4_RST
#define | UART5_RST
#define | CAN0_RST
#define | CAN1_RST
#define | OTG_RST
#define | USBD_RST
#define | ADC_RST
#define | I2S0_RST
#define | I2S1_RST
#define | PS2_RST
#define | SC0_RST
#define | SC1_RST
#define | SC2_RST
#define | SC3_RST
#define | SC4_RST
#define | SC5_RST
#define | I2C4_RST
#define | PWM0_RST
#define | PWM1_RST
#define | QEI0_RST
#define | QEI1_RST
#define | SYS_BODCTL_BODVL_2_2V
#define | SYS_BODCTL_BODVL_2_7V
#define | SYS_BODCTL_BODVL_3_8V
#define | SYS_BODCTL_BODVL_4_5V
#define | SYS_BODCTL_BODRSTEN
#define | SYS_BODCTL_BODINTEN
#define | SYS_BODCTL_BODLPM
#define | SYS_BODCTL_BODOUT
#define | SYS_BODCTL_LVREN
#define | SYS_VREFCTL_VREF_2_65V
#define | SYS_VREFCTL_VREF_2_048V
#define | SYS_VREFCTL_VREF_3_072V
#define | SYS_VREFCTL_VREF_4_096V
#define | SYS_VREFCTL_VREF_AVDD
#define | SYS_VREFCTL_ADCMODESEL_EADC
#define | SYS_VREFCTL_ADCMODESEL_ADC
#define | SYS_VREFCTL_PWMSYNCMODE_EN
#define | SYS_USBPHY_USBROLE_OTG_V33_EN
#define | SYS_USBPHY_USBROLE_STD_USBD
#define | SYS_USBPHY_USBROLE_STD_USBH
#define | SYS_USBPHY_USBROLE_ID_DEPH
#define | SYS_USBPHY_USBROLE_ON_THE_GO
#define | SYS_GPA_MFPL_PA0MFP_GPIO
#define | SYS_GPA_MFPL_PA0MFP_TAMPER0
#define | SYS_GPA_MFPL_PA0MFP_SC0_CD
#define | SYS_GPA_MFPL_PA0MFP_CAN1_RXD
#define | SYS_GPA_MFPL_PA0MFP_INT0
#define | SYS_GPA_MFPL_PA1MFP_GPIO
#define | SYS_GPA_MFPL_PA1MFP_TAMPER1
#define | SYS_GPA_MFPL_PA1MFP_SC5_CD
#define | SYS_GPA_MFPL_PA1MFP_CAN1_TXD
#define | SYS_GPA_MFPL_PA1MFP_EBI_A22
#define | SYS_GPA_MFPL_PA2MFP_GPIO
#define | SYS_GPA_MFPL_PA2MFP_SC2_DAT
#define | SYS_GPA_MFPL_PA2MFP_SPI3_MISO0
#define | SYS_GPA_MFPL_PA2MFP_I2S0_MCLK
#define | SYS_GPA_MFPL_PA2MFP_BRAKE11
#define | SYS_GPA_MFPL_PA2MFP_CAP_SFIELD
#define | SYS_GPA_MFPL_PA2MFP_EBI_A12
#define | SYS_GPA_MFPL_PA3MFP_GPIO
#define | SYS_GPA_MFPL_PA3MFP_SC2_CLK
#define | SYS_GPA_MFPL_PA3MFP_SPI3_MOSI0
#define | SYS_GPA_MFPL_PA3MFP_I2S0_DO
#define | SYS_GPA_MFPL_PA3MFP_BRAKE10
#define | SYS_GPA_MFPL_PA3MFP_EBI_A13
#define | SYS_GPA_MFPL_PA4MFP_GPIO
#define | SYS_GPA_MFPL_PA4MFP_SC2_PWR
#define | SYS_GPA_MFPL_PA4MFP_SPI3_CLK
#define | SYS_GPA_MFPL_PA4MFP_I2S0_DI
#define | SYS_GPA_MFPL_PA4MFP_QEI1_Z
#define | SYS_GPA_MFPL_PA4MFP_EBI_A14
#define | SYS_GPA_MFPL_PA4MFP_ECAP1_IC2
#define | SYS_GPA_MFPL_PA5MFP_GPIO
#define | SYS_GPA_MFPL_PA5MFP_SC2_RST
#define | SYS_GPA_MFPL_PA5MFP_SPI3_SS0
#define | SYS_GPA_MFPL_PA5MFP_I2S0_BCLK
#define | SYS_GPA_MFPL_PA5MFP_PWM0_CH0
#define | SYS_GPA_MFPL_PA5MFP_PWM0_0
#define | SYS_GPA_MFPL_PA5MFP_QEI1_B
#define | SYS_GPA_MFPL_PA5MFP_EBI_A15
#define | SYS_GPA_MFPL_PA5MFP_ECAP1_IC1
#define | SYS_GPA_MFPL_PA6MFP_GPIO
#define | SYS_GPA_MFPL_PA6MFP_SC2_CD
#define | SYS_GPA_MFPL_PA6MFP_I2S0_LRCK
#define | SYS_GPA_MFPL_PA6MFP_PWM0_CH1
#define | SYS_GPA_MFPL_PA6MFP_PWM0_1
#define | SYS_GPA_MFPL_PA6MFP_QEI1_A
#define | SYS_GPA_MFPL_PA6MFP_CAN1_TXD
#define | SYS_GPA_MFPL_PA6MFP_EBI_A16
#define | SYS_GPA_MFPL_PA6MFP_ECAP1_IC0
#define | SYS_GPA_MFPL_PA7MFP_GPIO
#define | SYS_GPA_MFPL_PA7MFP_SC0_CLK
#define | SYS_GPA_MFPL_PA7MFP_SPI3_SS0
#define | SYS_GPA_MFPL_PA7MFP_PWM1_CH3
#define | SYS_GPA_MFPL_PA7MFP_PWM1_3
#define | SYS_GPA_MFPL_PA7MFP_EPWM0_CH5
#define | SYS_GPA_MFPL_PA7MFP_EPWM0_5
#define | SYS_GPA_MFPL_PA7MFP_EBI_A17
#define | SYS_GPA_MFPH_PA8MFP_GPIO
#define | SYS_GPA_MFPH_PA8MFP_SC0_RST
#define | SYS_GPA_MFPH_PA8MFP_SPI3_CLK
#define | SYS_GPA_MFPH_PA8MFP_PWM1_CH2
#define | SYS_GPA_MFPH_PA8MFP_PWM1_2
#define | SYS_GPA_MFPH_PA8MFP_EPWM0_CH4
#define | SYS_GPA_MFPH_PA8MFP_EPWM0_4
#define | SYS_GPA_MFPH_PA8MFP_EBI_A18
#define | SYS_GPA_MFPH_PA9MFP_GPIO
#define | SYS_GPA_MFPH_PA9MFP_SC0_PWR
#define | SYS_GPA_MFPH_PA9MFP_SPI3_MISO0
#define | SYS_GPA_MFPH_PA9MFP_PWM1_CH1
#define | SYS_GPA_MFPH_PA9MFP_PWM1_1
#define | SYS_GPA_MFPH_PA9MFP_EPWM0_CH3
#define | SYS_GPA_MFPH_PA9MFP_EPWM0_3
#define | SYS_GPA_MFPH_PA9MFP_EBI_A19
#define | SYS_GPA_MFPH_PA10MFP_GPIO
#define | SYS_GPA_MFPH_PA10MFP_SC0_DAT
#define | SYS_GPA_MFPH_PA10MFP_SPI3_MOSI0
#define | SYS_GPA_MFPH_PA10MFP_PWM1_CH0
#define | SYS_GPA_MFPH_PA10MFP_PWM1_0
#define | SYS_GPA_MFPH_PA10MFP_EPWM0_CH2
#define | SYS_GPA_MFPH_PA10MFP_EPWM0_2
#define | SYS_GPA_MFPH_PA10MFP_EBI_A20
#define | SYS_GPA_MFPH_PA11MFP_GPIO
#define | SYS_GPA_MFPH_PA11MFP_UART0_RTS
#define | SYS_GPA_MFPH_PA11MFP_SPI3_MISO1
#define | SYS_GPA_MFPH_PA11MFP_PWM0_CH5
#define | SYS_GPA_MFPH_PA11MFP_PWM0_5
#define | SYS_GPA_MFPH_PA11MFP_EPWM0_CH1
#define | SYS_GPA_MFPH_PA11MFP_EPWM0_1
#define | SYS_GPA_MFPH_PA11MFP_EBI_AD0
#define | SYS_GPA_MFPH_PA12MFP_GPIO
#define | SYS_GPA_MFPH_PA12MFP_UART0_CTS
#define | SYS_GPA_MFPH_PA12MFP_SPI3_MOSI1
#define | SYS_GPA_MFPH_PA12MFP_PWM0_CH4
#define | SYS_GPA_MFPH_PA12MFP_PWM0_4
#define | SYS_GPA_MFPH_PA12MFP_EPWM0_CH0
#define | SYS_GPA_MFPH_PA12MFP_EPWM0_0
#define | SYS_GPA_MFPH_PA12MFP_EBI_AD1
#define | SYS_GPA_MFPH_PA13MFP_GPIO
#define | SYS_GPA_MFPH_PA13MFP_UART0_RXD
#define | SYS_GPA_MFPH_PA13MFP_SC3_DAT
#define | SYS_GPA_MFPH_PA13MFP_PWM1_CH4
#define | SYS_GPA_MFPH_PA13MFP_PWM1_4
#define | SYS_GPA_MFPH_PA13MFP_EBI_AD2
#define | SYS_GPA_MFPH_PA14MFP_GPIO
#define | SYS_GPA_MFPH_PA14MFP_UART0_TXD
#define | SYS_GPA_MFPH_PA14MFP_SC3_CLK
#define | SYS_GPA_MFPH_PA14MFP_PWM1_CH5
#define | SYS_GPA_MFPH_PA14MFP_PWM1_5
#define | SYS_GPA_MFPH_PA14MFP_EBI_AD3
#define | SYS_GPA_MFPH_PA15MFP_GPIO
#define | SYS_GPA_MFPH_PA15MFP_SC3_PWR
#define | SYS_GPA_MFPH_PA15MFP_UART2_RTS
#define | SYS_GPA_MFPH_PA15MFP_I2C0_SCL
#define | SYS_GPA_MFPH_PA15MFP_EBI_A21
#define | SYS_GPB_MFPL_PB0MFP_GPIO
#define | SYS_GPB_MFPL_PB0MFP_USB0_OTG5V_ST
#define | SYS_GPB_MFPL_PB0MFP_I2C4_SCL
#define | SYS_GPB_MFPL_PB0MFP_INT1
#define | SYS_GPB_MFPL_PB1MFP_GPIO
#define | SYS_GPB_MFPL_PB1MFP_USB0_OTG5V_EN
#define | SYS_GPB_MFPL_PB1MFP_I2C4_SDA
#define | SYS_GPB_MFPL_PB1MFP_TM1_CNT_OUT
#define | SYS_GPB_MFPL_PB2MFP_GPIO
#define | SYS_GPB_MFPL_PB2MFP_UART1_RXD
#define | SYS_GPB_MFPL_PB2MFP_SPI2_SS0
#define | SYS_GPB_MFPL_PB2MFP_USB1_D_N
#define | SYS_GPB_MFPL_PB2MFP_EBI_AD4
#define | SYS_GPB_MFPL_PB3MFP_GPIO
#define | SYS_GPB_MFPL_PB3MFP_UART1_TXD
#define | SYS_GPB_MFPL_PB3MFP_SPI2_CLK
#define | SYS_GPB_MFPL_PB3MFP_USB1_D_P
#define | SYS_GPB_MFPL_PB3MFP_EBI_AD5
#define | SYS_GPB_MFPL_PB4MFP_GPIO
#define | SYS_GPB_MFPL_PB4MFP_UART1_RTS
#define | SYS_GPB_MFPL_PB4MFP_SPI2_MISO0
#define | SYS_GPB_MFPL_PB4MFP_UART4_RXD
#define | SYS_GPB_MFPL_PB4MFP_TM0_CNT_OUT
#define | SYS_GPB_MFPL_PB4MFP_EBI_AD6
#define | SYS_GPB_MFPL_PB5MFP_GPIO
#define | SYS_GPB_MFPL_PB5MFP_UART1_CTS
#define | SYS_GPB_MFPL_PB5MFP_SPI2_MOSI0
#define | SYS_GPB_MFPL_PB5MFP_UART4_TXD
#define | SYS_GPB_MFPL_PB5MFP_EBI_AD7
#define | SYS_GPB_MFPL_PB6MFP_GPIO
#define | SYS_GPB_MFPL_PB6MFP_I2C2_SCL
#define | SYS_GPB_MFPL_PB6MFP_BRAKE01
#define | SYS_GPB_MFPL_PB6MFP_UART4_RTS
#define | SYS_GPB_MFPL_PB6MFP_PWM1_CH4
#define | SYS_GPB_MFPL_PB6MFP_PWM1_4
#define | SYS_GPB_MFPL_PB6MFP_EPWM1_CH0
#define | SYS_GPB_MFPL_PB6MFP_EPWM1_0
#define | SYS_GPB_MFPL_PB6MFP_EBI_AD8
#define | SYS_GPB_MFPL_PB7MFP_GPIO
#define | SYS_GPB_MFPL_PB7MFP_I2C2_SDA
#define | SYS_GPB_MFPL_PB7MFP_BRAKE00
#define | SYS_GPB_MFPL_PB7MFP_UART4_CTS
#define | SYS_GPB_MFPL_PB7MFP_PWM1_CH5
#define | SYS_GPB_MFPL_PB7MFP_PWM1_5
#define | SYS_GPB_MFPL_PB7MFP_EPWM1_CH1
#define | SYS_GPB_MFPL_PB7MFP_EPWM1_1
#define | SYS_GPB_MFPL_PB7MFP_ETM_TRACE_DATA3
#define | SYS_GPB_MFPL_PB7MFP_EBI_AD9
#define | SYS_GPB_MFPH_PB8MFP_GPIO
#define | SYS_GPB_MFPH_PB8MFP_UART5_CTS
#define | SYS_GPB_MFPH_PB8MFP_EPWM1_CH2
#define | SYS_GPB_MFPH_PB8MFP_EPWM1_2
#define | SYS_GPB_MFPH_PB8MFP_ETM_TRACE_DATA2
#define | SYS_GPB_MFPH_PB8MFP_EBI_AD10
#define | SYS_GPB_MFPH_PB9MFP_GPIO
#define | SYS_GPB_MFPH_PB9MFP_UART5_RTS
#define | SYS_GPB_MFPH_PB9MFP_EPWM1_CH3
#define | SYS_GPB_MFPH_PB9MFP_EPWM1_3
#define | SYS_GPB_MFPH_PB9MFP_ETM_TRACE_DATA1
#define | SYS_GPB_MFPH_PB9MFP_EBI_AD11
#define | SYS_GPB_MFPH_PB10MFP_GPIO
#define | SYS_GPB_MFPH_PB10MFP_UART5_TXD
#define | SYS_GPB_MFPH_PB10MFP_EPWM1_CH4
#define | SYS_GPB_MFPH_PB10MFP_EPWM1_4
#define | SYS_GPB_MFPH_PB10MFP_ETM_TRACE_DATA0
#define | SYS_GPB_MFPH_PB10MFP_EBI_AD12
#define | SYS_GPB_MFPH_PB11MFP_GPIO
#define | SYS_GPB_MFPH_PB11MFP_UART5_RXD
#define | SYS_GPB_MFPH_PB11MFP_EPWM1_CH5
#define | SYS_GPB_MFPH_PB11MFP_EPWM1_5
#define | SYS_GPB_MFPH_PB11MFP_ETM_TRACE_CLK
#define | SYS_GPB_MFPH_PB11MFP_EBI_AD13
#define | SYS_GPB_MFPH_PB12MFP_GPIO
#define | SYS_GPB_MFPH_PB12MFP_UART4_RTS
#define | SYS_GPB_MFPH_PB12MFP_SPI2_MISO1
#define | SYS_GPB_MFPH_PB12MFP_CAN0_RXD
#define | SYS_GPB_MFPH_PB12MFP_EMAC_MII_MDC
#define | SYS_GPB_MFPH_PB12MFP_EBI_AD14
#define | SYS_GPB_MFPH_PB13MFP_GPIO
#define | SYS_GPB_MFPH_PB13MFP_UART4_CTS
#define | SYS_GPB_MFPH_PB13MFP_SPI2_MOSI1
#define | SYS_GPB_MFPH_PB13MFP_CAN0_TXD
#define | SYS_GPB_MFPH_PB13MFP_EMAC_MII_MDIO
#define | SYS_GPB_MFPH_PB13MFP_EBI_AD15
#define | SYS_GPB_MFPH_PB14MFP_GPIO
#define | SYS_GPB_MFPH_PB14MFP_I2S1_MCLK
#define | SYS_GPB_MFPH_PB14MFP_SC1_RST
#define | SYS_GPB_MFPH_PB14MFP_BRAKE01
#define | SYS_GPB_MFPH_PB14MFP_EMAC_MII_MDC
#define | SYS_GPB_MFPH_PB15MFP_GPIO
#define | SYS_GPB_MFPH_PB15MFP_I2S1_DO
#define | SYS_GPB_MFPH_PB15MFP_SC1_DAT
#define | SYS_GPB_MFPH_PB15MFP_BRAKE00
#define | SYS_GPB_MFPH_PB15MFP_EMAC_MII_MDIO
#define | SYS_GPC_MFPL_PC0MFP_GPIO
#define | SYS_GPC_MFPL_PC0MFP_I2S1_DI
#define | SYS_GPC_MFPL_PC0MFP_SC1_DAT
#define | SYS_GPC_MFPL_PC0MFP_UART4_RXD
#define | SYS_GPC_MFPL_PC0MFP_EMAC_REFCLK
#define | SYS_GPC_MFPL_PC0MFP_EBI_MCLK
#define | SYS_GPC_MFPL_PC0MFP_INT2
#define | SYS_GPC_MFPL_PC1MFP_GPIO
#define | SYS_GPC_MFPL_PC1MFP_I2S1_BCLK
#define | SYS_GPC_MFPL_PC1MFP_SC1_CLK
#define | SYS_GPC_MFPL_PC1MFP_UART4_TXD
#define | SYS_GPC_MFPL_PC1MFP_TM3_CNT_OUT
#define | SYS_GPC_MFPL_PC1MFP_EMAC_MII_RXERR
#define | SYS_GPC_MFPL_PC1MFP_EBI_AD13
#define | SYS_GPC_MFPL_PC2MFP_GPIO
#define | SYS_GPC_MFPL_PC2MFP_I2S1_LRCK
#define | SYS_GPC_MFPL_PC2MFP_SC1_PWR
#define | SYS_GPC_MFPL_PC2MFP_UART4_RTS
#define | SYS_GPC_MFPL_PC2MFP_SPI0_SS0
#define | SYS_GPC_MFPL_PC2MFP_EMAC_MII_RXDV
#define | SYS_GPC_MFPL_PC2MFP_EBI_AD12
#define | SYS_GPC_MFPL_PC3MFP_GPIO
#define | SYS_GPC_MFPL_PC3MFP_I2S1_MCLK
#define | SYS_GPC_MFPL_PC3MFP_SC1_CD
#define | SYS_GPC_MFPL_PC3MFP_UART4_CTS
#define | SYS_GPC_MFPL_PC3MFP_SPI0_MISO1
#define | SYS_GPC_MFPL_PC3MFP_QEI0_Z
#define | SYS_GPC_MFPL_PC3MFP_EMAC_MII_RXD1
#define | SYS_GPC_MFPL_PC3MFP_EBI_AD11
#define | SYS_GPC_MFPL_PC3MFP_ECAP0_IC2
#define | SYS_GPC_MFPL_PC4MFP_GPIO
#define | SYS_GPC_MFPL_PC4MFP_I2S1_DO
#define | SYS_GPC_MFPL_PC4MFP_SC1_RST
#define | SYS_GPC_MFPL_PC4MFP_SPI0_MOSI1
#define | SYS_GPC_MFPL_PC4MFP_QEI0_B
#define | SYS_GPC_MFPL_PC4MFP_EMAC_MII_RXD0
#define | SYS_GPC_MFPL_PC4MFP_EBI_AD10
#define | SYS_GPC_MFPL_PC4MFP_ECAP0_IC1
#define | SYS_GPC_MFPL_PC5MFP_GPIO
#define | SYS_GPC_MFPL_PC5MFP_CLK_O
#define | SYS_GPC_MFPL_PC5MFP_CLKO
#define | SYS_GPC_MFPL_PC5MFP_QEI0_A
#define | SYS_GPC_MFPL_PC5MFP_EMAC_MII_RXCLK
#define | SYS_GPC_MFPL_PC5MFP_EBI_MCLK
#define | SYS_GPC_MFPL_PC5MFP_ECAP0_IC0
#define | SYS_GPC_MFPL_PC6MFP_GPIO
#define | SYS_GPC_MFPL_PC6MFP_TM2_EXT
#define | SYS_GPC_MFPL_PC6MFP_SPI0_MISO0
#define | SYS_GPC_MFPL_PC6MFP_TM2_CNT_OUT
#define | SYS_GPC_MFPL_PC6MFP_EMAC_MII_TXD0
#define | SYS_GPC_MFPL_PC6MFP_EBI_AD9
#define | SYS_GPC_MFPL_PC7MFP_GPIO
#define | SYS_GPC_MFPL_PC7MFP_TM1_EXT
#define | SYS_GPC_MFPL_PC7MFP_SPI0_MOSI0
#define | SYS_GPC_MFPL_PC7MFP_EMAC_MII_TXD1
#define | SYS_GPC_MFPL_PC7MFP_EBI_AD8
#define | SYS_GPC_MFPH_PC8MFP_GPIO
#define | SYS_GPC_MFPH_PC8MFP_TM0_EXT
#define | SYS_GPC_MFPH_PC8MFP_SPI0_CLK
#define | SYS_GPC_MFPH_PC8MFP_EMAC_MII_TXEN
#define | SYS_GPC_MFPH_PC9MFP_GPIO
#define | SYS_GPC_MFPH_PC9MFP_STADC
#define | SYS_GPC_MFPH_PC9MFP_UART2_CTS
#define | SYS_GPC_MFPH_PC9MFP_SC3_RST
#define | SYS_GPC_MFPH_PC9MFP_I2C0_SDA
#define | SYS_GPC_MFPH_PC9MFP_CAP_DATA1
#define | SYS_GPC_MFPH_PC9MFP_I2C3_SCL
#define | SYS_GPC_MFPH_PC9MFP_EBI_A22
#define | SYS_GPC_MFPH_PC9MFP_SD1_DAT0
#define | SYS_GPC_MFPH_PC9MFP_EBI_A6
#define | SYS_GPC_MFPH_PC10MFP_GPIO
#define | SYS_GPC_MFPH_PC10MFP_SC3_CD
#define | SYS_GPC_MFPH_PC10MFP_UART2_RXD
#define | SYS_GPC_MFPH_PC10MFP_PWM0_CH2
#define | SYS_GPC_MFPH_PC10MFP_PWM0_2
#define | SYS_GPC_MFPH_PC10MFP_EBI_A23
#define | SYS_GPC_MFPH_PC10MFP_EBI_AD2
#define | SYS_GPC_MFPH_PC11MFP_GPIO
#define | SYS_GPC_MFPH_PC11MFP_UART2_TXD
#define | SYS_GPC_MFPH_PC11MFP_PWM0_CH3
#define | SYS_GPC_MFPH_PC11MFP_PWM0_3
#define | SYS_GPC_MFPH_PC11MFP_EBI_A24
#define | SYS_GPC_MFPH_PC11MFP_EBI_AD3
#define | SYS_GPC_MFPH_PC12MFP_GPIO
#define | SYS_GPC_MFPH_PC12MFP_SPI1_SS0
#define | SYS_GPC_MFPH_PC12MFP_SC4_CD
#define | SYS_GPC_MFPH_PC12MFP_SD1_CDn
#define | SYS_GPC_MFPH_PC12MFP_CAP_DATA7
#define | SYS_GPC_MFPH_PC12MFP_ETM_TRACE_DATA3
#define | SYS_GPC_MFPH_PC12MFP_EBI_A0
#define | SYS_GPC_MFPH_PC13MFP_GPIO
#define | SYS_GPC_MFPH_PC13MFP_SPI1_MOSI1
#define | SYS_GPC_MFPH_PC13MFP_SC4_RST
#define | SYS_GPC_MFPH_PC13MFP_SD1_CMD
#define | SYS_GPC_MFPH_PC13MFP_CAP_DATA6
#define | SYS_GPC_MFPH_PC13MFP_ETM_TRACE_DATA2
#define | SYS_GPC_MFPH_PC13MFP_EBI_A1
#define | SYS_GPC_MFPH_PC14MFP_GPIO
#define | SYS_GPC_MFPH_PC14MFP_SPI1_MISO1
#define | SYS_GPC_MFPH_PC14MFP_SC4_PWR
#define | SYS_GPC_MFPH_PC14MFP_TM3_EXT
#define | SYS_GPC_MFPH_PC14MFP_SD1_CLK
#define | SYS_GPC_MFPH_PC14MFP_CAP_DATA5
#define | SYS_GPC_MFPH_PC14MFP_ETM_TRACE_DATA1
#define | SYS_GPC_MFPH_PC14MFP_EBI_A2
#define | SYS_GPC_MFPH_PC15MFP_GPIO
#define | SYS_GPC_MFPH_PC15MFP_SPI1_MOSI0
#define | SYS_GPC_MFPH_PC15MFP_SC4_DAT
#define | SYS_GPC_MFPH_PC15MFP_SD1_DAT3
#define | SYS_GPC_MFPH_PC15MFP_CAP_DATA4
#define | SYS_GPC_MFPH_PC15MFP_ETM_TRACE_DATA0
#define | SYS_GPC_MFPH_PC15MFP_EBI_A3
#define | SYS_GPD_MFPL_PD0MFP_GPIO
#define | SYS_GPD_MFPL_PD0MFP_SPI1_MISO0
#define | SYS_GPD_MFPL_PD0MFP_SC4_CLK
#define | SYS_GPD_MFPL_PD0MFP_SD1_DAT2
#define | SYS_GPD_MFPL_PD0MFP_CAP_DATA3
#define | SYS_GPD_MFPL_PD0MFP_ETM_TRACE_CLK
#define | SYS_GPD_MFPL_PD0MFP_EBI_A4
#define | SYS_GPD_MFPL_PD0MFP_INT3
#define | SYS_GPD_MFPL_PD1MFP_GPIO
#define | SYS_GPD_MFPL_PD1MFP_SPI1_CLK
#define | SYS_GPD_MFPL_PD1MFP_TM0_CNT_OUT
#define | SYS_GPD_MFPL_PD1MFP_SD1_DAT1
#define | SYS_GPD_MFPL_PD1MFP_CAP_DATA2
#define | SYS_GPD_MFPL_PD1MFP_EBI_A5
#define | SYS_GPD_MFPL_PD2MFP_GPIO
#define | SYS_GPD_MFPL_PD2MFP_STADC
#define | SYS_GPD_MFPL_PD2MFP_I2C3_SCL
#define | SYS_GPD_MFPL_PD2MFP_SD1_DAT0
#define | SYS_GPD_MFPL_PD2MFP_CAP_DATA1
#define | SYS_GPD_MFPL_PD2MFP_EBI_A6
#define | SYS_GPD_MFPL_PD3MFP_GPIO
#define | SYS_GPD_MFPL_PD3MFP_SC5_CLK
#define | SYS_GPD_MFPL_PD3MFP_I2C3_SDA
#define | SYS_GPD_MFPL_PD3MFP_ACMP2_O
#define | SYS_GPD_MFPL_PD3MFP_SD0_CDn
#define | SYS_GPD_MFPL_PD3MFP_CAP_DATA0
#define | SYS_GPD_MFPL_PD3MFP_JTAG_TDO
#define | SYS_GPD_MFPL_PD3MFP_EBI_A7
#define | SYS_GPD_MFPL_PD4MFP_GPIO
#define | SYS_GPD_MFPL_PD4MFP_SC5_CD
#define | SYS_GPD_MFPL_PD4MFP_UART3_RXD
#define | SYS_GPD_MFPL_PD4MFP_ACMP1_O
#define | SYS_GPD_MFPL_PD4MFP_CAP_SCLK
#define | SYS_GPD_MFPL_PD4MFP_JTAG_TDI
#define | SYS_GPD_MFPL_PD4MFP_EBI_A8
#define | SYS_GPD_MFPL_PD5MFP_GPIO
#define | SYS_GPD_MFPL_PD5MFP_SC5_RST
#define | SYS_GPD_MFPL_PD5MFP_UART3_TXD
#define | SYS_GPD_MFPL_PD5MFP_CAP_VSYNC
#define | SYS_GPD_MFPL_PD5MFP_JTAG_nTRST
#define | SYS_GPD_MFPL_PD5MFP_EBI_A9
#define | SYS_GPD_MFPL_PD6MFP_GPIO
#define | SYS_GPD_MFPL_PD6MFP_SC5_PWR
#define | SYS_GPD_MFPL_PD6MFP_UART3_RTS
#define | SYS_GPD_MFPL_PD6MFP_SD0_CMD
#define | SYS_GPD_MFPL_PD6MFP_CAP_HSYNC
#define | SYS_GPD_MFPL_PD6MFP_EBI_A10
#define | SYS_GPD_MFPL_PD7MFP_GPIO
#define | SYS_GPD_MFPL_PD7MFP_SC5_DAT
#define | SYS_GPD_MFPL_PD7MFP_UART3_CTS
#define | SYS_GPD_MFPL_PD7MFP_SD0_CLK
#define | SYS_GPD_MFPL_PD7MFP_CAP_PIXCLK
#define | SYS_GPD_MFPL_PD7MFP_EBI_A11
#define | SYS_GPD_MFPH_PD8MFP_GPIO
#define | SYS_GPD_MFPH_PD8MFP_SPI3_MISO1
#define | SYS_GPD_MFPH_PD8MFP_I2C0_SCL
#define | SYS_GPD_MFPH_PD9MFP_GPIO
#define | SYS_GPD_MFPH_PD9MFP_SPI3_MOSI1
#define | SYS_GPD_MFPH_PD9MFP_I2C0_SDA
#define | SYS_GPD_MFPH_PD10MFP_GPIO
#define | SYS_GPD_MFPH_PD10MFP_SC3_DAT
#define | SYS_GPD_MFPH_PD10MFP_I2C4_SCL
#define | SYS_GPD_MFPH_PD11MFP_GPIO
#define | SYS_GPD_MFPH_PD11MFP_SC3_RST
#define | SYS_GPD_MFPH_PD11MFP_TM3_CNT_OUT
#define | SYS_GPD_MFPH_PD12MFP_GPIO
#define | SYS_GPD_MFPH_PD12MFP_SC3_CLK
#define | SYS_GPD_MFPH_PD12MFP_I2C4_SDA
#define | SYS_GPD_MFPH_PD13MFP_GPIO
#define | SYS_GPD_MFPH_PD13MFP_SPI1_SS0
#define | SYS_GPD_MFPH_PD13MFP_UART5_CTS
#define | SYS_GPD_MFPH_PD13MFP_ECAP0_IC2
#define | SYS_GPD_MFPH_PD14MFP_GPIO
#define | SYS_GPD_MFPH_PD14MFP_SPI1_CLK
#define | SYS_GPD_MFPH_PD14MFP_UART5_RTS
#define | SYS_GPD_MFPH_PD14MFP_ECAP0_IC1
#define | SYS_GPD_MFPH_PD15MFP_GPIO
#define | SYS_GPD_MFPH_PD15MFP_SPI1_MISO0
#define | SYS_GPD_MFPH_PD15MFP_UART5_TXD
#define | SYS_GPD_MFPH_PD15MFP_ECAP0_IC0
#define | SYS_GPE_MFPL_PE0MFP_GPIO
#define | SYS_GPE_MFPL_PE0MFP_ADC0_0
#define | SYS_GPE_MFPL_PE0MFP_INT4
#define | SYS_GPE_MFPL_PE1MFP_GPIO
#define | SYS_GPE_MFPL_PE1MFP_ADC0_1
#define | SYS_GPE_MFPL_PE1MFP_TM2_CNT_OUT
#define | SYS_GPE_MFPL_PE2MFP_GPIO
#define | SYS_GPE_MFPL_PE2MFP_ADC0_2
#define | SYS_GPE_MFPL_PE2MFP_ACMP0_O
#define | SYS_GPE_MFPL_PE2MFP_SPI0_MISO0
#define | SYS_GPE_MFPL_PE3MFP_GPIO
#define | SYS_GPE_MFPL_PE3MFP_ADC0_3
#define | SYS_GPE_MFPL_PE3MFP_ACMP0_P3
#define | SYS_GPE_MFPL_PE3MFP_SPI0_MOSI0
#define | SYS_GPE_MFPL_PE4MFP_GPIO
#define | SYS_GPE_MFPL_PE4MFP_ADC0_4
#define | SYS_GPE_MFPL_PE4MFP_ACMP0_P2
#define | SYS_GPE_MFPL_PE4MFP_SPI0_SS0
#define | SYS_GPE_MFPL_PE5MFP_GPIO
#define | SYS_GPE_MFPL_PE5MFP_ADC0_5
#define | SYS_GPE_MFPL_PE5MFP_ACMP0_P1
#define | SYS_GPE_MFPL_PE5MFP_SPI0_CLK
#define | SYS_GPE_MFPL_PE5MFP_SD0_CDn
#define | SYS_GPE_MFPL_PE6MFP_GPIO
#define | SYS_GPE_MFPL_PE6MFP_ADC0_6
#define | SYS_GPE_MFPL_PE6MFP_ACMP0_P0
#define | SYS_GPE_MFPL_PE6MFP_SPI0_MISO0
#define | SYS_GPE_MFPL_PE6MFP_SD0_CMD
#define | SYS_GPE_MFPL_PE6MFP_EBI_nWR
#define | SYS_GPE_MFPL_PE7MFP_GPIO
#define | SYS_GPE_MFPL_PE7MFP_ADC0_7
#define | SYS_GPE_MFPL_PE7MFP_ACMP0_N
#define | SYS_GPE_MFPL_PE7MFP_SPI0_MOSI0
#define | SYS_GPE_MFPL_PE7MFP_SD0_CLK
#define | SYS_GPE_MFPL_PE7MFP_EBI_nRD
#define | SYS_GPE_MFPH_PE8MFP_GPIO
#define | SYS_GPE_MFPH_PE8MFP_ADC0_8
#define | SYS_GPE_MFPH_PE8MFP_ADC1_0
#define | SYS_GPE_MFPH_PE8MFP_ACMP1_N
#define | SYS_GPE_MFPH_PE8MFP_TM1_CNT_OUT
#define | SYS_GPE_MFPH_PE8MFP_SD0_DAT3
#define | SYS_GPE_MFPH_PE8MFP_EBI_ALE
#define | SYS_GPE_MFPH_PE9MFP_GPIO
#define | SYS_GPE_MFPH_PE9MFP_ADC0_9
#define | SYS_GPE_MFPH_PE9MFP_ADC1_1
#define | SYS_GPE_MFPH_PE9MFP_ACMP1_P0
#define | SYS_GPE_MFPH_PE9MFP_SD0_DAT2
#define | SYS_GPE_MFPH_PE9MFP_EBI_nWRH
#define | SYS_GPE_MFPH_PE10MFP_GPIO
#define | SYS_GPE_MFPH_PE10MFP_ADC0_10
#define | SYS_GPE_MFPH_PE10MFP_ADC1_2
#define | SYS_GPE_MFPH_PE10MFP_ACMP1_P1
#define | SYS_GPE_MFPH_PE10MFP_SPI0_MISO1
#define | SYS_GPE_MFPH_PE10MFP_SD0_DAT1
#define | SYS_GPE_MFPH_PE10MFP_EBI_nWRL
#define | SYS_GPE_MFPH_PE11MFP_GPIO
#define | SYS_GPE_MFPH_PE11MFP_ADC0_11
#define | SYS_GPE_MFPH_PE11MFP_ADC1_3
#define | SYS_GPE_MFPH_PE11MFP_ACMP1_P2
#define | SYS_GPE_MFPH_PE11MFP_SPI0_MOSI1
#define | SYS_GPE_MFPH_PE11MFP_SD0_DAT0
#define | SYS_GPE_MFPH_PE11MFP_ACMP2_P3
#define | SYS_GPE_MFPH_PE11MFP_EBI_nCS0
#define | SYS_GPE_MFPH_PE12MFP_GPIO
#define | SYS_GPE_MFPH_PE12MFP_ADC1_4
#define | SYS_GPE_MFPH_PE12MFP_ACMP1_P3
#define | SYS_GPE_MFPH_PE12MFP_ACMP2_P2
#define | SYS_GPE_MFPH_PE12MFP_EBI_nCS1
#define | SYS_GPE_MFPH_PE13MFP_GPIO
#define | SYS_GPE_MFPH_PE13MFP_ADC1_5
#define | SYS_GPE_MFPH_PE13MFP_ACMP2_P1
#define | SYS_GPE_MFPH_PE13MFP_EBI_nCS2
#define | SYS_GPE_MFPH_PE14MFP_GPIO
#define | SYS_GPE_MFPH_PE14MFP_ADC1_6
#define | SYS_GPE_MFPH_PE14MFP_ACMP2_P0
#define | SYS_GPE_MFPH_PE14MFP_EBI_nCS3
#define | SYS_GPE_MFPH_PE15MFP_GPIO
#define | SYS_GPE_MFPH_PE15MFP_ADC1_7
#define | SYS_GPE_MFPH_PE15MFP_ACMP2_N
#define | SYS_GPF_MFPL_PF0MFP_GPIO
#define | SYS_GPF_MFPL_PF0MFP_SPI1_MOSI0
#define | SYS_GPF_MFPL_PF0MFP_UART5_RXD
#define | SYS_GPF_MFPL_PF0MFP_INT5
#define | SYS_GPF_MFPL_PF1MFP_GPIO
#define | SYS_GPF_MFPL_PF1MFP_SPI2_MOSI1
#define | SYS_GPF_MFPL_PF2MFP_GPIO
#define | SYS_GPF_MFPL_PF2MFP_SPI3_SS0
#define | SYS_GPF_MFPL_PF2MFP_SD0_DAT3
#define | SYS_GPF_MFPL_PF2MFP_EMAC_MII_RXD3
#define | SYS_GPF_MFPL_PF3MFP_GPIO
#define | SYS_GPF_MFPL_PF3MFP_SPI3_CLK
#define | SYS_GPF_MFPL_PF3MFP_SD0_DAT2
#define | SYS_GPF_MFPL_PF3MFP_EMAC_MII_RXD2
#define | SYS_GPF_MFPL_PF4MFP_GPIO
#define | SYS_GPF_MFPL_PF4MFP_SPI3_MISO0
#define | SYS_GPF_MFPL_PF4MFP_SD0_DAT1
#define | SYS_GPF_MFPL_PF4MFP_EMAC_MII_COL0
#define | SYS_GPF_MFPL_PF5MFP_GPIO
#define | SYS_GPF_MFPL_PF5MFP_SPI3_MOSI0
#define | SYS_GPF_MFPL_PF5MFP_SD0_DAT0
#define | SYS_GPF_MFPL_PF5MFP_EMAC_MII_CRS
#define | SYS_GPF_MFPL_PF6MFP_GPIO
#define | SYS_GPF_MFPL_PF6MFP_UART2_RXD
#define | SYS_GPF_MFPL_PF6MFP_SD0_CDn
#define | SYS_GPF_MFPL_PF6MFP_EMAC_MII_TXCLK
#define | SYS_GPF_MFPL_PF7MFP_GPIO
#define | SYS_GPF_MFPL_PF7MFP_UART2_TXD
#define | SYS_GPF_MFPL_PF7MFP_SD0_CMD
#define | SYS_GPF_MFPL_PF7MFP_EMAC_MII_TXD3
#define | SYS_GPF_MFPH_PF8MFP_GPIO
#define | SYS_GPF_MFPH_PF8MFP_UART2_RTS
#define | SYS_GPF_MFPH_PF8MFP_SD0_CLK
#define | SYS_GPF_MFPH_PF8MFP_EMAC_MII_TXD2
#define | SYS_GPF_MFPH_PF9MFP_GPIO
#define | SYS_GPF_MFPH_PF9MFP_OPA0_IN_P
#define | SYS_GPF_MFPH_PF9MFP_OPA0_P
#define | SYS_GPF_MFPH_PF9MFP_PWM0_CH0
#define | SYS_GPF_MFPH_PF9MFP_PWM0_0
#define | SYS_GPF_MFPH_PF10MFP_GPIO
#define | SYS_GPF_MFPH_PF10MFP_OPA0_IN_N
#define | SYS_GPF_MFPH_PF10MFP_OPA0_N
#define | SYS_GPF_MFPH_PF10MFP_PWM0_CH1
#define | SYS_GPF_MFPH_PF10MFP_PWM0_1
#define | SYS_GPF_MFPH_PF11MFP_GPIO
#define | SYS_GPF_MFPH_PF11MFP_OPA0_O
#define | SYS_GPF_MFPH_PF11MFP_UART1_RTS
#define | SYS_GPF_MFPH_PF12MFP_GPIO
#define | SYS_GPF_MFPH_PF12MFP_OPA1_IN_P
#define | SYS_GPF_MFPH_PF12MFP_OPA1_P
#define | SYS_GPF_MFPH_PF12MFP_UART1_CTS
#define | SYS_GPF_MFPH_PF13MFP_GPIO
#define | SYS_GPF_MFPH_PF13MFP_OPA1_IN_N
#define | SYS_GPF_MFPH_PF13MFP_OPA1_N
#define | SYS_GPF_MFPH_PF13MFP_UART1_TXD
#define | SYS_GPF_MFPH_PF14MFP_GPIO
#define | SYS_GPF_MFPH_PF14MFP_OPA1_O
#define | SYS_GPF_MFPH_PF14MFP_UART1_RXD
#define | SYS_GPF_MFPH_PF15MFP_GPIO
#define | SYS_GPF_MFPH_PF15MFP_UART0_RTS
#define | SYS_GPG_MFPL_PG0MFP_GPIO
#define | SYS_GPG_MFPL_PG0MFP_UART0_CTS
#define | SYS_GPG_MFPL_PG0MFP_INT6
#define | SYS_GPG_MFPL_PG1MFP_GPIO
#define | SYS_GPG_MFPL_PG1MFP_UART0_RXD
#define | SYS_GPG_MFPL_PG2MFP_GPIO
#define | SYS_GPG_MFPL_PG2MFP_UART0_TXD
#define | SYS_GPG_MFPL_PG3MFP_GPIO
#define | SYS_GPG_MFPL_PG3MFP_PS2_CLK
#define | SYS_GPG_MFPL_PG3MFP_I2S1_DO
#define | SYS_GPG_MFPL_PG3MFP_SC1_RST
#define | SYS_GPG_MFPL_PG4MFP_GPIO
#define | SYS_GPG_MFPL_PG4MFP_PS2_DAT
#define | SYS_GPG_MFPL_PG4MFP_I2S1_DI
#define | SYS_GPG_MFPL_PG4MFP_SC1_PWR
#define | SYS_GPG_MFPL_PG5MFP_GPIO
#define | SYS_GPG_MFPL_PG5MFP_I2S1_BCLK
#define | SYS_GPG_MFPL_PG5MFP_SC1_DAT
#define | SYS_GPG_MFPL_PG6MFP_GPIO
#define | SYS_GPG_MFPL_PG6MFP_I2S1_LRCK
#define | SYS_GPG_MFPL_PG6MFP_SC1_CLK
#define | SYS_GPG_MFPL_PG7MFP_GPIO
#define | SYS_GPG_MFPL_PG7MFP_SPI2_MISO0
#define | SYS_GPG_MFPL_PG7MFP_I2S1_MCLK
#define | SYS_GPG_MFPL_PG7MFP_SC1_CD
#define | SYS_GPG_MFPL_PG7MFP_SC3_RST
#define | SYS_GPG_MFPH_PG8MFP_GPIO
#define | SYS_GPG_MFPH_PG8MFP_SPI2_MOSI0
#define | SYS_GPG_MFPH_PG8MFP_I2S1_DO
#define | SYS_GPG_MFPH_PG8MFP_UART4_RTS
#define | SYS_GPG_MFPH_PG8MFP_SC3_DAT
#define | SYS_GPG_MFPH_PG9MFP_GPIO
#define | SYS_GPG_MFPH_PG9MFP_SPI2_CLK
#define | SYS_GPG_MFPH_PG9MFP_I2S1_DI
#define | SYS_GPG_MFPH_PG9MFP_UART4_CTS
#define | SYS_GPG_MFPH_PG9MFP_SC3_CLK
#define | SYS_GPG_MFPH_PG10MFP_GPIO
#define | SYS_GPG_MFPH_PG10MFP_ICE_CLK
#define | SYS_GPG_MFPH_PG10MFP_JTAG_TCLK
#define | SYS_GPG_MFPH_PG11MFP_GPIO
#define | SYS_GPG_MFPH_PG11MFP_ICE_DAT
#define | SYS_GPG_MFPH_PG11MFP_JTAG_TMS
#define | SYS_GPG_MFPH_PG12MFP_GPIO
#define | SYS_GPG_MFPH_PG12MFP_XT1_OUT
#define | SYS_GPG_MFPH_PG13MFP_GPIO
#define | SYS_GPG_MFPH_PG13MFP_XT1_IN
#define | SYS_GPG_MFPH_PG14MFP_GPIO
#define | SYS_GPG_MFPH_PG14MFP_X32K_OUT
#define | SYS_GPG_MFPH_PG14MFP_I2C1_SDA
#define | SYS_GPG_MFPH_PG15MFP_GPIO
#define | SYS_GPG_MFPH_PG15MFP_X32K_IN
#define | SYS_GPG_MFPH_PG15MFP_I2C1_SCL
#define | SYS_GPH_MFPL_PH0MFP_GPIO
#define | SYS_GPH_MFPL_PH0MFP_I2C1_SCL
#define | SYS_GPH_MFPL_PH0MFP_UART4_RXD
#define | SYS_GPH_MFPL_PH0MFP_CAN1_RXD
#define | SYS_GPH_MFPL_PH0MFP_INT7
#define | SYS_GPH_MFPL_PH1MFP_GPIO
#define | SYS_GPH_MFPL_PH1MFP_UART4_TXD
#define | SYS_GPH_MFPL_PH1MFP_I2C1_SDA
#define | SYS_GPH_MFPL_PH1MFP_CAN1_TXD
#define | SYS_GPH_MFPL_PH2MFP_GPIO
#define | SYS_GPH_MFPL_PH2MFP_UART2_CTS
#define | SYS_GPH_MFPL_PH3MFP_GPIO
#define | SYS_GPH_MFPL_PH3MFP_I2C3_SCL
#define | SYS_GPH_MFPL_PH4MFP_GPIO
#define | SYS_GPH_MFPL_PH4MFP_I2C3_SDA
#define | SYS_GPH_MFPL_PH5MFP_GPIO
#define | SYS_GPH_MFPL_PH5MFP_SPI2_SS0
#define | SYS_GPH_MFPL_PH6MFP_GPIO
#define | SYS_GPH_MFPL_PH6MFP_SPI2_CLK
#define | SYS_GPH_MFPL_PH7MFP_GPIO
#define | SYS_GPH_MFPL_PH7MFP_SPI2_MISO0
#define | SYS_GPH_MFPH_PH8MFP_GPIO
#define | SYS_GPH_MFPH_PH8MFP_SPI2_MOSI0
#define | SYS_GPH_MFPH_PH9MFP_GPIO
#define | SYS_GPH_MFPH_PH9MFP_SPI2_MISO1
#define | SYS_GPH_MFPH_PH10MFP_GPIO
#define | SYS_GPH_MFPH_PH10MFP_SPI2_MOSI1
#define | SYS_GPH_MFPH_PH11MFP_GPIO
#define | SYS_GPH_MFPH_PH11MFP_UART3_RXD
#define | SYS_GPH_MFPH_PH12MFP_GPIO
#define | SYS_GPH_MFPH_PH12MFP_UART3_TXD
#define | SYS_GPH_MFPH_PH13MFP_GPIO
#define | SYS_GPH_MFPH_PH13MFP_UART3_RTS
#define | SYS_GPH_MFPH_PH14MFP_GPIO
#define | SYS_GPH_MFPH_PH14MFP_UART3_CTS
#define | SYS_GPH_MFPH_PH15MFP_GPIO
#define | SYS_GPH_MFPH_PH15MFP_SC5_CLK
#define | SYS_GPI_MFPL_PI0MFP_GPIO
#define | SYS_GPI_MFPL_PI0MFP_SC5_RST
#define | SYS_GPI_MFPL_PI1MFP_GPIO
#define | SYS_GPI_MFPL_PI1MFP_SC5_PWR
#define | SYS_GPI_MFPL_PI2MFP_GPIO
#define | SYS_GPI_MFPL_PI2MFP_SC5_DAT
#define | SYS_GPI_MFPL_PI3MFP_GPIO
#define | SYS_GPI_MFPL_PI3MFP_SPI3_SS0
#define | SYS_GPI_MFPL_PI4MFP_GPIO
#define | SYS_GPI_MFPL_PI4MFP_SPI3_CLK
#define | SYS_GPI_MFPL_PI5MFP_GPIO
#define | SYS_GPI_MFPL_PI5MFP_SPI3_MISO0
#define | SYS_GPI_MFPL_PI6MFP_GPIO
#define | SYS_GPI_MFPL_PI6MFP_SPI3_MOSI0
#define | SYS_GPI_MFPL_PI7MFP_GPIO
#define | SYS_GPI_MFPL_PI7MFP_I2C2_SCL
#define | SYS_GPI_MFPL_PI7MFP_SPI3_MISO1
#define | SYS_GPI_MFPH_PI8MFP_GPIO
#define | SYS_GPI_MFPH_PI8MFP_I2C2_SDA
#define | SYS_GPI_MFPH_PI8MFP_SPI3_MOSI1
#define | SYS_GPI_MFPH_PI9MFP_GPIO
#define | SYS_GPI_MFPH_PI9MFP_I2C4_SCL
#define | SYS_GPI_MFPH_PI10MFP_GPIO
#define | SYS_GPI_MFPH_PI11MFP_GPIO
#define | SYS_GPI_MFPH_PI11MFP_SPI2_SS0
#define | SYS_GPI_MFPH_PI11MFP_I2S1_BCLK
#define | SYS_GPI_MFPH_PI11MFP_I2C4_SCL
#define | SYS_GPI_MFPH_PI11MFP_SC3_PWR
#define | SYS_GPI_MFPH_PI12MFP_GPIO
#define | SYS_GPI_MFPH_PI12MFP_SPI2_MISO1
#define | SYS_GPI_MFPH_PI12MFP_I2S1_LRCK
#define | SYS_GPI_MFPH_PI12MFP_I2C4_SDA
#define | SYS_GPI_MFPH_PI12MFP_SC3_CD
#define | SYS_GPI_MFPH_PI13MFP_GPIO
#define | SYS_GPI_MFPH_PI14MFP_GPIO
#define | SYS_GPI_MFPH_PI15MFP_GPIO

## Detailed Description

## Macro Definition Documentation

## ◆ ACMP_RST

#define ACMP_RST

Reset ACMP

Definition at line 49 of file sys.h.

## ◆ ADC_RST

#define ADC_RST

Reset ADC

Definition at line 68 of file sys.h.

## ◆ CAN0_RST

#define CAN0_RST

Reset CAN0

Definition at line 64 of file sys.h.

## ◆ CAN1_RST

#define CAN1_RST

Reset CAN1

Definition at line 65 of file sys.h.

## ◆ CAP_RST

#define CAP_RST

Reset CAP

Definition at line 42 of file sys.h.

## ◆ CRC_RST

#define CRC_RST

Reset CRC

Definition at line 41 of file sys.h.

## ◆ CRYPTO_RST

#define CRYPTO_RST

Reset CRYPTO

Definition at line 43 of file sys.h.

## ◆ EBI_RST

#define EBI_RST

Reset EBI

Definition at line 37 of file sys.h.

## ◆ EMAC_RST

#define EMAC_RST

Reset EMAC

Definition at line 39 of file sys.h.

## ◆ GPIO_RST

#define GPIO_RST

Reset GPIO

Definition at line 44 of file sys.h.

## ◆ I2C0_RST

#define I2C0_RST

Reset I2C0

Definition at line 50 of file sys.h.

## ◆ I2C1_RST

#define I2C1_RST

Reset I2C1

Definition at line 51 of file sys.h.

## ◆ I2C2_RST

#define I2C2_RST

Reset I2C2

Definition at line 52 of file sys.h.

## ◆ I2C3_RST

#define I2C3_RST

Reset I2C3

Definition at line 53 of file sys.h.

## ◆ I2C4_RST

#define I2C4_RST

Reset I2C4

Definition at line 78 of file sys.h.

## ◆ I2S0_RST

#define I2S0_RST

Reset I2S0

Definition at line 69 of file sys.h.

## ◆ I2S1_RST

#define I2S1_RST

Reset I2S1

Definition at line 70 of file sys.h.

## ◆ OTG_RST

#define OTG_RST

Reset OTG

Definition at line 66 of file sys.h.

## ◆ PDMA_RST

#define PDMA_RST

Reset PDMA

Definition at line 36 of file sys.h.

## ◆ PS2_RST

#define PS2_RST

Reset PS2

Definition at line 71 of file sys.h.

## ◆ PWM0_RST

#define PWM0_RST

Reset PWM0

Definition at line 79 of file sys.h.

## ◆ PWM1_RST

#define PWM1_RST

Reset PWM1

Definition at line 80 of file sys.h.

## ◆ QEI0_RST

#define QEI0_RST

Reset QEI0

Definition at line 81 of file sys.h.

## ◆ QEI1_RST

#define QEI1_RST

Reset QEI1

Definition at line 82 of file sys.h.

## ◆ SC0_RST

#define SC0_RST

Reset SC0

Definition at line 72 of file sys.h.

## ◆ SC1_RST

#define SC1_RST

Reset SC1

Definition at line 73 of file sys.h.

## ◆ SC2_RST

#define SC2_RST

Reset SC2

Definition at line 74 of file sys.h.

## ◆ SC3_RST

#define SC3_RST

Reset SC3

Definition at line 75 of file sys.h.

## ◆ SC4_RST

#define SC4_RST

Reset SC4

Definition at line 76 of file sys.h.

## ◆ SC5_RST

#define SC5_RST

Reset SC5

Definition at line 77 of file sys.h.

## ◆ SDH_RST

#define SDH_RST

Reset SDIO

Definition at line 40 of file sys.h.

## ◆ SPI0_RST

#define SPI0_RST

Reset SPI0

Definition at line 54 of file sys.h.

## ◆ SPI1_RST

#define SPI1_RST

Reset SPI1

Definition at line 55 of file sys.h.

## ◆ SPI2_RST

#define SPI2_RST

Reset SPI2

Definition at line 56 of file sys.h.

## ◆ SPI3_RST

#define SPI3_RST

Reset SPI3

Definition at line 57 of file sys.h.

## ◆ SYS_BODCTL_BODINTEN

#define SYS_BODCTL_BODINTEN

Enable interrupt function of BOD.

Definition at line 92 of file sys.h.

## ◆ SYS_BODCTL_BODLPM

#define SYS_BODCTL_BODLPM

BOD work in low power mode.

Definition at line 93 of file sys.h.

## ◆ SYS_BODCTL_BODOUT

#define SYS_BODCTL_BODOUT

Output of BOD IP.

Definition at line 94 of file sys.h.

## ◆ SYS_BODCTL_BODRSTEN

#define SYS_BODCTL_BODRSTEN

Enable reset function of BOD.

Definition at line 91 of file sys.h.

## ◆ SYS_BODCTL_BODVL_2_2V

#define SYS_BODCTL_BODVL_2_2V

Threshold voltage of BOD is selected 2.2V

Definition at line 87 of file sys.h.

## ◆ SYS_BODCTL_BODVL_2_7V

#define SYS_BODCTL_BODVL_2_7V

Threshold voltage of BOD is selected 2.7V

Definition at line 88 of file sys.h.

## ◆ SYS_BODCTL_BODVL_3_8V

#define SYS_BODCTL_BODVL_3_8V

Threshold voltage of BOD is selected 3.82V

Definition at line 89 of file sys.h.

## ◆ SYS_BODCTL_BODVL_4_5V

#define SYS_BODCTL_BODVL_4_5V

Threshold voltage of BOD is selected 4.5V

Definition at line 90 of file sys.h.

## ◆ SYS_BODCTL_LVREN

#define SYS_BODCTL_LVREN

Enable LVR function.

Definition at line 95 of file sys.h.

## ◆ SYS_GPA_MFPH_PA10MFP_EBI_A20

#define SYS_GPA_MFPH_PA10MFP_EBI_A20

GPA_MFPH PA10 setting for EBI_A20

Definition at line 230 of file sys.h.

## ◆ SYS_GPA_MFPH_PA10MFP_EPWM0_2

#define SYS_GPA_MFPH_PA10MFP_EPWM0_2

GPA_MFPH PA10 setting for EPWM0_CH2

Definition at line 229 of file sys.h.

## ◆ SYS_GPA_MFPH_PA10MFP_EPWM0_CH2

#define SYS_GPA_MFPH_PA10MFP_EPWM0_CH2

GPA_MFPH PA10 setting for EPWM0_CH2

Definition at line 228 of file sys.h.

## ◆ SYS_GPA_MFPH_PA10MFP_GPIO

#define SYS_GPA_MFPH_PA10MFP_GPIO

GPA_MFPH PA10 setting for GPIO

Definition at line 223 of file sys.h.

## ◆ SYS_GPA_MFPH_PA10MFP_PWM1_0

#define SYS_GPA_MFPH_PA10MFP_PWM1_0

GPA_MFPH PA10 setting for PWM1_CH0

Definition at line 227 of file sys.h.

## ◆ SYS_GPA_MFPH_PA10MFP_PWM1_CH0

#define SYS_GPA_MFPH_PA10MFP_PWM1_CH0

GPA_MFPH PA10 setting for PWM1_CH0

Definition at line 226 of file sys.h.

## ◆ SYS_GPA_MFPH_PA10MFP_SC0_DAT

#define SYS_GPA_MFPH_PA10MFP_SC0_DAT

GPA_MFPH PA10 setting for SC0_DAT

Definition at line 224 of file sys.h.

## ◆ SYS_GPA_MFPH_PA10MFP_SPI3_MOSI0

#define SYS_GPA_MFPH_PA10MFP_SPI3_MOSI0

GPA_MFPH PA10 setting for SPI3_MOSI0

Definition at line 225 of file sys.h.

## ◆ SYS_GPA_MFPH_PA11MFP_EBI_AD0

#define SYS_GPA_MFPH_PA11MFP_EBI_AD0

GPA_MFPH PA11 setting for EBI_AD0

Definition at line 240 of file sys.h.

## ◆ SYS_GPA_MFPH_PA11MFP_EPWM0_1

#define SYS_GPA_MFPH_PA11MFP_EPWM0_1

GPA_MFPH PA11 setting for EPWM0_CH1

Definition at line 239 of file sys.h.

## ◆ SYS_GPA_MFPH_PA11MFP_EPWM0_CH1

#define SYS_GPA_MFPH_PA11MFP_EPWM0_CH1

GPA_MFPH PA11 setting for EPWM0_CH1

Definition at line 238 of file sys.h.

## ◆ SYS_GPA_MFPH_PA11MFP_GPIO

#define SYS_GPA_MFPH_PA11MFP_GPIO

GPA_MFPH PA11 setting for GPIO

Definition at line 233 of file sys.h.

## ◆ SYS_GPA_MFPH_PA11MFP_PWM0_5

#define SYS_GPA_MFPH_PA11MFP_PWM0_5

GPA_MFPH PA11 setting for PWM0_CH5

Definition at line 237 of file sys.h.

## ◆ SYS_GPA_MFPH_PA11MFP_PWM0_CH5

#define SYS_GPA_MFPH_PA11MFP_PWM0_CH5

GPA_MFPH PA11 setting for PWM0_CH5

Definition at line 236 of file sys.h.

## ◆ SYS_GPA_MFPH_PA11MFP_SPI3_MISO1

#define SYS_GPA_MFPH_PA11MFP_SPI3_MISO1

GPA_MFPH PA11 setting for SPI3_MISO1

Definition at line 235 of file sys.h.

## ◆ SYS_GPA_MFPH_PA11MFP_UART0_RTS

#define SYS_GPA_MFPH_PA11MFP_UART0_RTS

GPA_MFPH PA11 setting for UART0_RTS

Definition at line 234 of file sys.h.

## ◆ SYS_GPA_MFPH_PA12MFP_EBI_AD1

#define SYS_GPA_MFPH_PA12MFP_EBI_AD1

GPA_MFPH PA12 setting for EBI_AD1

Definition at line 250 of file sys.h.

## ◆ SYS_GPA_MFPH_PA12MFP_EPWM0_0

#define SYS_GPA_MFPH_PA12MFP_EPWM0_0

GPA_MFPH PA12 setting for EPWM0_CH0

Definition at line 249 of file sys.h.

## ◆ SYS_GPA_MFPH_PA12MFP_EPWM0_CH0

#define SYS_GPA_MFPH_PA12MFP_EPWM0_CH0

GPA_MFPH PA12 setting for EPWM0_CH0

Definition at line 248 of file sys.h.

## ◆ SYS_GPA_MFPH_PA12MFP_GPIO

#define SYS_GPA_MFPH_PA12MFP_GPIO

GPA_MFPH PA12 setting for GPIO

Definition at line 243 of file sys.h.

## ◆ SYS_GPA_MFPH_PA12MFP_PWM0_4

#define SYS_GPA_MFPH_PA12MFP_PWM0_4

GPA_MFPH PA12 setting for PWM0_CH4

Definition at line 247 of file sys.h.

## ◆ SYS_GPA_MFPH_PA12MFP_PWM0_CH4

#define SYS_GPA_MFPH_PA12MFP_PWM0_CH4

GPA_MFPH PA12 setting for PWM0_CH4

Definition at line 246 of file sys.h.

## ◆ SYS_GPA_MFPH_PA12MFP_SPI3_MOSI1

#define SYS_GPA_MFPH_PA12MFP_SPI3_MOSI1

GPA_MFPH PA12 setting for SPI3_MOSI1

Definition at line 245 of file sys.h.

## ◆ SYS_GPA_MFPH_PA12MFP_UART0_CTS

#define SYS_GPA_MFPH_PA12MFP_UART0_CTS

GPA_MFPH PA12 setting for UART0_CTS

Definition at line 244 of file sys.h.

## ◆ SYS_GPA_MFPH_PA13MFP_EBI_AD2

#define SYS_GPA_MFPH_PA13MFP_EBI_AD2

GPA_MFPH PA13 setting for EBI_AD2

Definition at line 258 of file sys.h.

## ◆ SYS_GPA_MFPH_PA13MFP_GPIO

#define SYS_GPA_MFPH_PA13MFP_GPIO

GPA_MFPH PA13 setting for GPIO

Definition at line 253 of file sys.h.

## ◆ SYS_GPA_MFPH_PA13MFP_PWM1_4

#define SYS_GPA_MFPH_PA13MFP_PWM1_4

GPA_MFPH PA13 setting for PWM1_CH4

Definition at line 257 of file sys.h.

## ◆ SYS_GPA_MFPH_PA13MFP_PWM1_CH4

#define SYS_GPA_MFPH_PA13MFP_PWM1_CH4

GPA_MFPH PA13 setting for PWM1_CH4

Definition at line 256 of file sys.h.

## ◆ SYS_GPA_MFPH_PA13MFP_SC3_DAT

#define SYS_GPA_MFPH_PA13MFP_SC3_DAT

GPA_MFPH PA13 setting for SC3_DAT

Definition at line 255 of file sys.h.

## ◆ SYS_GPA_MFPH_PA13MFP_UART0_RXD

#define SYS_GPA_MFPH_PA13MFP_UART0_RXD

GPA_MFPH PA13 setting for UART0_RXD

Definition at line 254 of file sys.h.

## ◆ SYS_GPA_MFPH_PA14MFP_EBI_AD3

#define SYS_GPA_MFPH_PA14MFP_EBI_AD3

GPA_MFPH PA14 setting for EBI_AD3

Definition at line 266 of file sys.h.

## ◆ SYS_GPA_MFPH_PA14MFP_GPIO

#define SYS_GPA_MFPH_PA14MFP_GPIO

GPA_MFPH PA14 setting for GPIO

Definition at line 261 of file sys.h.

## ◆ SYS_GPA_MFPH_PA14MFP_PWM1_5

#define SYS_GPA_MFPH_PA14MFP_PWM1_5

GPA_MFPH PA14 setting for PWM1_CH5

Definition at line 265 of file sys.h.

## ◆ SYS_GPA_MFPH_PA14MFP_PWM1_CH5

#define SYS_GPA_MFPH_PA14MFP_PWM1_CH5

GPA_MFPH PA14 setting for PWM1_CH5

Definition at line 264 of file sys.h.

## ◆ SYS_GPA_MFPH_PA14MFP_SC3_CLK

#define SYS_GPA_MFPH_PA14MFP_SC3_CLK

GPA_MFPH PA14 setting for SC3_CLK

Definition at line 263 of file sys.h.

## ◆ SYS_GPA_MFPH_PA14MFP_UART0_TXD

#define SYS_GPA_MFPH_PA14MFP_UART0_TXD

GPA_MFPH PA14 setting for UART0_TXD

Definition at line 262 of file sys.h.

## ◆ SYS_GPA_MFPH_PA15MFP_EBI_A21

#define SYS_GPA_MFPH_PA15MFP_EBI_A21

GPA_MFPH PA15 setting for EBI_A21

Definition at line 272 of file sys.h.

## ◆ SYS_GPA_MFPH_PA15MFP_GPIO

#define SYS_GPA_MFPH_PA15MFP_GPIO

GPA_MFPH PA15 setting for GPIO

Definition at line 268 of file sys.h.

## ◆ SYS_GPA_MFPH_PA15MFP_I2C0_SCL

#define SYS_GPA_MFPH_PA15MFP_I2C0_SCL

GPA_MFPH PA15 setting for I2C0_SCL

Definition at line 271 of file sys.h.

## ◆ SYS_GPA_MFPH_PA15MFP_SC3_PWR

#define SYS_GPA_MFPH_PA15MFP_SC3_PWR

GPA_MFPH PA15 setting for SC3_PWR

Definition at line 269 of file sys.h.

## ◆ SYS_GPA_MFPH_PA15MFP_UART2_RTS

#define SYS_GPA_MFPH_PA15MFP_UART2_RTS

GPA_MFPH PA15 setting for UART2_RTS

Definition at line 270 of file sys.h.

## ◆ SYS_GPA_MFPH_PA8MFP_EBI_A18

#define SYS_GPA_MFPH_PA8MFP_EBI_A18

GPA_MFPH PA8 setting for EBI_A18

Definition at line 210 of file sys.h.

## ◆ SYS_GPA_MFPH_PA8MFP_EPWM0_4

#define SYS_GPA_MFPH_PA8MFP_EPWM0_4

GPA_MFPH PA8 setting for EPWM0_CH4

Definition at line 209 of file sys.h.

## ◆ SYS_GPA_MFPH_PA8MFP_EPWM0_CH4

#define SYS_GPA_MFPH_PA8MFP_EPWM0_CH4

GPA_MFPH PA8 setting for EPWM0_CH4

Definition at line 208 of file sys.h.

## ◆ SYS_GPA_MFPH_PA8MFP_GPIO

#define SYS_GPA_MFPH_PA8MFP_GPIO

GPA_MFPH PA8 setting for GPIO

Definition at line 203 of file sys.h.

## ◆ SYS_GPA_MFPH_PA8MFP_PWM1_2

#define SYS_GPA_MFPH_PA8MFP_PWM1_2

GPA_MFPH PA8 setting for PWM1 CH2

Definition at line 207 of file sys.h.

## ◆ SYS_GPA_MFPH_PA8MFP_PWM1_CH2

#define SYS_GPA_MFPH_PA8MFP_PWM1_CH2

GPA_MFPH PA8 setting for PWM1 CH2

Definition at line 206 of file sys.h.

## ◆ SYS_GPA_MFPH_PA8MFP_SC0_RST

#define SYS_GPA_MFPH_PA8MFP_SC0_RST

GPA_MFPH PA8 setting for SC0_RST

Definition at line 204 of file sys.h.

## ◆ SYS_GPA_MFPH_PA8MFP_SPI3_CLK

#define SYS_GPA_MFPH_PA8MFP_SPI3_CLK

GPA_MFPH PA8 setting for SPI3_CLK

Definition at line 205 of file sys.h.

## ◆ SYS_GPA_MFPH_PA9MFP_EBI_A19

#define SYS_GPA_MFPH_PA9MFP_EBI_A19

GPA_MFPH PA9 setting for EBI_A19

Definition at line 220 of file sys.h.

## ◆ SYS_GPA_MFPH_PA9MFP_EPWM0_3

#define SYS_GPA_MFPH_PA9MFP_EPWM0_3

GPA_MFPH PA9 setting for EPWM0 CH3

Definition at line 219 of file sys.h.

## ◆ SYS_GPA_MFPH_PA9MFP_EPWM0_CH3

#define SYS_GPA_MFPH_PA9MFP_EPWM0_CH3

GPA_MFPH PA9 setting for EPWM0 CH3

Definition at line 218 of file sys.h.

## ◆ SYS_GPA_MFPH_PA9MFP_GPIO

#define SYS_GPA_MFPH_PA9MFP_GPIO

GPA_MFPH PA9 setting for GPIO

Definition at line 213 of file sys.h.

## ◆ SYS_GPA_MFPH_PA9MFP_PWM1_1

#define SYS_GPA_MFPH_PA9MFP_PWM1_1

GPA_MFPH PA9 setting for PWM1 CH1

Definition at line 217 of file sys.h.

## ◆ SYS_GPA_MFPH_PA9MFP_PWM1_CH1

#define SYS_GPA_MFPH_PA9MFP_PWM1_CH1

GPA_MFPH PA9 setting for PWM1 CH1

Definition at line 216 of file sys.h.

## ◆ SYS_GPA_MFPH_PA9MFP_SC0_PWR

#define SYS_GPA_MFPH_PA9MFP_SC0_PWR

GPA_MFPH PA9 setting for SC0_PWR

Definition at line 214 of file sys.h.

## ◆ SYS_GPA_MFPH_PA9MFP_SPI3_MISO0

#define SYS_GPA_MFPH_PA9MFP_SPI3_MISO0

GPA_MFPH PA9 setting for SPI3_MISO0

Definition at line 215 of file sys.h.

## ◆ SYS_GPA_MFPL_PA0MFP_CAN1_RXD

#define SYS_GPA_MFPL_PA0MFP_CAN1_RXD

GPA_MFPL PA0 setting for CAN1_RXD

Definition at line 134 of file sys.h.

## ◆ SYS_GPA_MFPL_PA0MFP_GPIO

#define SYS_GPA_MFPL_PA0MFP_GPIO

GPA_MFPL PA0 setting for GPIO

Definition at line 131 of file sys.h.

## ◆ SYS_GPA_MFPL_PA0MFP_INT0

#define SYS_GPA_MFPL_PA0MFP_INT0

GPA_MFPL PA0 setting for INT0

Definition at line 135 of file sys.h.

## ◆ SYS_GPA_MFPL_PA0MFP_SC0_CD

#define SYS_GPA_MFPL_PA0MFP_SC0_CD

GPA_MFPL PA0 setting for SC0_CD

Definition at line 133 of file sys.h.

## ◆ SYS_GPA_MFPL_PA0MFP_TAMPER0

#define SYS_GPA_MFPL_PA0MFP_TAMPER0

GPA_MFPL PA0 setting for TAMPER0

Definition at line 132 of file sys.h.

## ◆ SYS_GPA_MFPL_PA1MFP_CAN1_TXD

#define SYS_GPA_MFPL_PA1MFP_CAN1_TXD

GPA_MFPL PA1 setting for CAN1_TXD

Definition at line 141 of file sys.h.

## ◆ SYS_GPA_MFPL_PA1MFP_EBI_A22

#define SYS_GPA_MFPL_PA1MFP_EBI_A22

GPA_MFPL PA1 setting for EBI_A22

Definition at line 142 of file sys.h.

## ◆ SYS_GPA_MFPL_PA1MFP_GPIO

#define SYS_GPA_MFPL_PA1MFP_GPIO

GPA_MFPL PA1 setting for GPIO

Definition at line 138 of file sys.h.

## ◆ SYS_GPA_MFPL_PA1MFP_SC5_CD

#define SYS_GPA_MFPL_PA1MFP_SC5_CD

GPA_MFPL PA1 setting for SC5_CD

Definition at line 140 of file sys.h.

## ◆ SYS_GPA_MFPL_PA1MFP_TAMPER1

#define SYS_GPA_MFPL_PA1MFP_TAMPER1

GPA_MFPL PA1 setting for TAMPER1

Definition at line 139 of file sys.h.

## ◆ SYS_GPA_MFPL_PA2MFP_BRAKE11

#define SYS_GPA_MFPL_PA2MFP_BRAKE11

GPA_MFPL PA2 setting for BRAKE11

Definition at line 149 of file sys.h.

## ◆ SYS_GPA_MFPL_PA2MFP_CAP_SFIELD

#define SYS_GPA_MFPL_PA2MFP_CAP_SFIELD

GPA_MFPL PA2 setting for CAP_SFIELD

Definition at line 150 of file sys.h.

## ◆ SYS_GPA_MFPL_PA2MFP_EBI_A12

#define SYS_GPA_MFPL_PA2MFP_EBI_A12

GPA_MFPL PA2 setting for EBI_A12

Definition at line 151 of file sys.h.

## ◆ SYS_GPA_MFPL_PA2MFP_GPIO

#define SYS_GPA_MFPL_PA2MFP_GPIO

GPA_MFPL PA2 setting for GPIO

Definition at line 145 of file sys.h.

## ◆ SYS_GPA_MFPL_PA2MFP_I2S0_MCLK

#define SYS_GPA_MFPL_PA2MFP_I2S0_MCLK

GPA_MFPL PA2 setting for I2S0_MCLK

Definition at line 148 of file sys.h.

## ◆ SYS_GPA_MFPL_PA2MFP_SC2_DAT

#define SYS_GPA_MFPL_PA2MFP_SC2_DAT

GPA_MFPL PA2 setting for SC2_DAT

Definition at line 146 of file sys.h.

## ◆ SYS_GPA_MFPL_PA2MFP_SPI3_MISO0

#define SYS_GPA_MFPL_PA2MFP_SPI3_MISO0

GPA_MFPL PA2 setting for SPI3_MISO0

Definition at line 147 of file sys.h.

## ◆ SYS_GPA_MFPL_PA3MFP_BRAKE10

#define SYS_GPA_MFPL_PA3MFP_BRAKE10

GPA_MFPL PA3 setting for BRAKE10

Definition at line 158 of file sys.h.

## ◆ SYS_GPA_MFPL_PA3MFP_EBI_A13

#define SYS_GPA_MFPL_PA3MFP_EBI_A13

GPA_MFPL PA3 setting for EBI_A13

Definition at line 159 of file sys.h.

## ◆ SYS_GPA_MFPL_PA3MFP_GPIO

#define SYS_GPA_MFPL_PA3MFP_GPIO

GPA_MFPL PA3 setting for GPIO

Definition at line 154 of file sys.h.

## ◆ SYS_GPA_MFPL_PA3MFP_I2S0_DO

#define SYS_GPA_MFPL_PA3MFP_I2S0_DO

GPA_MFPL PA3 setting for I2S0_D0

Definition at line 157 of file sys.h.

## ◆ SYS_GPA_MFPL_PA3MFP_SC2_CLK

#define SYS_GPA_MFPL_PA3MFP_SC2_CLK

GPA_MFPL PA3 setting for SC2_CLK

Definition at line 155 of file sys.h.

## ◆ SYS_GPA_MFPL_PA3MFP_SPI3_MOSI0

#define SYS_GPA_MFPL_PA3MFP_SPI3_MOSI0

GPA_MFPL PA3 setting for SPI3_MOSI0

Definition at line 156 of file sys.h.

## ◆ SYS_GPA_MFPL_PA4MFP_EBI_A14

#define SYS_GPA_MFPL_PA4MFP_EBI_A14

GPA_MFPL PA4 setting for EBI_A14

Definition at line 167 of file sys.h.

## ◆ SYS_GPA_MFPL_PA4MFP_ECAP1_IC2

#define SYS_GPA_MFPL_PA4MFP_ECAP1_IC2

GPA_MFPL PA4 setting for ECAP1_IC2

Definition at line 168 of file sys.h.

## ◆ SYS_GPA_MFPL_PA4MFP_GPIO

#define SYS_GPA_MFPL_PA4MFP_GPIO

GPA_MFPL PA4 setting for GPIO

Definition at line 162 of file sys.h.

## ◆ SYS_GPA_MFPL_PA4MFP_I2S0_DI

#define SYS_GPA_MFPL_PA4MFP_I2S0_DI

GPA_MFPL PA4 setting for I2S0_DI

Definition at line 165 of file sys.h.

## ◆ SYS_GPA_MFPL_PA4MFP_QEI1_Z

#define SYS_GPA_MFPL_PA4MFP_QEI1_Z

GPA_MFPL PA4 setting for QEI1_Z

Definition at line 166 of file sys.h.

## ◆ SYS_GPA_MFPL_PA4MFP_SC2_PWR

#define SYS_GPA_MFPL_PA4MFP_SC2_PWR

GPA_MFPL PA4 setting for SC2_PWR

Definition at line 163 of file sys.h.

## ◆ SYS_GPA_MFPL_PA4MFP_SPI3_CLK

#define SYS_GPA_MFPL_PA4MFP_SPI3_CLK

GPA_MFPL PA4 setting for SPI3_CLK

Definition at line 164 of file sys.h.

## ◆ SYS_GPA_MFPL_PA5MFP_EBI_A15

#define SYS_GPA_MFPL_PA5MFP_EBI_A15

GPA_MFPL PA5 setting for EBI_A15

Definition at line 178 of file sys.h.

## ◆ SYS_GPA_MFPL_PA5MFP_ECAP1_IC1

#define SYS_GPA_MFPL_PA5MFP_ECAP1_IC1

GPA_MFPL PA5 setting for ECAP1_IC1

Definition at line 179 of file sys.h.

## ◆ SYS_GPA_MFPL_PA5MFP_GPIO

#define SYS_GPA_MFPL_PA5MFP_GPIO

GPA_MFPL PA5 setting for GPIO

Definition at line 171 of file sys.h.

## ◆ SYS_GPA_MFPL_PA5MFP_I2S0_BCLK

#define SYS_GPA_MFPL_PA5MFP_I2S0_BCLK

GPA_MFPL PA5 setting for I2S0_BCLK

Definition at line 174 of file sys.h.

## ◆ SYS_GPA_MFPL_PA5MFP_PWM0_0

#define SYS_GPA_MFPL_PA5MFP_PWM0_0

GPA_MFPL PA5 setting for PWM0 CH0

Definition at line 176 of file sys.h.

## ◆ SYS_GPA_MFPL_PA5MFP_PWM0_CH0

#define SYS_GPA_MFPL_PA5MFP_PWM0_CH0

GPA_MFPL PA5 setting for PWM0 CH0

Definition at line 175 of file sys.h.

## ◆ SYS_GPA_MFPL_PA5MFP_QEI1_B

#define SYS_GPA_MFPL_PA5MFP_QEI1_B

GPA_MFPL PA5 setting for QEI1_B

Definition at line 177 of file sys.h.

## ◆ SYS_GPA_MFPL_PA5MFP_SC2_RST

#define SYS_GPA_MFPL_PA5MFP_SC2_RST

GPA_MFPL PA5 setting for SC2_RST

Definition at line 172 of file sys.h.

## ◆ SYS_GPA_MFPL_PA5MFP_SPI3_SS0

#define SYS_GPA_MFPL_PA5MFP_SPI3_SS0

GPA_MFPL PA5 setting for SPI3_SS0

Definition at line 173 of file sys.h.

## ◆ SYS_GPA_MFPL_PA6MFP_CAN1_TXD

#define SYS_GPA_MFPL_PA6MFP_CAN1_TXD

GPA_MFPL PA6 setting for CAN1_TXD

Definition at line 188 of file sys.h.

## ◆ SYS_GPA_MFPL_PA6MFP_EBI_A16

#define SYS_GPA_MFPL_PA6MFP_EBI_A16

GPA_MFPL PA6 setting for EBI_A16

Definition at line 189 of file sys.h.

## ◆ SYS_GPA_MFPL_PA6MFP_ECAP1_IC0

#define SYS_GPA_MFPL_PA6MFP_ECAP1_IC0

GPA_MFPL PA6 setting for ECAP1_IC0

Definition at line 190 of file sys.h.

## ◆ SYS_GPA_MFPL_PA6MFP_GPIO

#define SYS_GPA_MFPL_PA6MFP_GPIO

GPA_MFPL PA6 setting for GPIO

Definition at line 182 of file sys.h.

## ◆ SYS_GPA_MFPL_PA6MFP_I2S0_LRCK

#define SYS_GPA_MFPL_PA6MFP_I2S0_LRCK

GPA_MFPL PA6 setting for I2S0_LRCK

Definition at line 184 of file sys.h.

## ◆ SYS_GPA_MFPL_PA6MFP_PWM0_1

#define SYS_GPA_MFPL_PA6MFP_PWM0_1

GPA_MFPL PA6 setting for PWM1 CH1

Definition at line 186 of file sys.h.

## ◆ SYS_GPA_MFPL_PA6MFP_PWM0_CH1

#define SYS_GPA_MFPL_PA6MFP_PWM0_CH1

GPA_MFPL PA6 setting for PWM1 CH1

Definition at line 185 of file sys.h.

## ◆ SYS_GPA_MFPL_PA6MFP_QEI1_A

#define SYS_GPA_MFPL_PA6MFP_QEI1_A

GPA_MFPL PA6 setting for QEI1_A

Definition at line 187 of file sys.h.

## ◆ SYS_GPA_MFPL_PA6MFP_SC2_CD

#define SYS_GPA_MFPL_PA6MFP_SC2_CD

GPA_MFPL PA6 setting for SC2_CD

Definition at line 183 of file sys.h.

## ◆ SYS_GPA_MFPL_PA7MFP_EBI_A17

#define SYS_GPA_MFPL_PA7MFP_EBI_A17

GPA_MFPL PA7 setting for EBI_A17

Definition at line 200 of file sys.h.

## ◆ SYS_GPA_MFPL_PA7MFP_EPWM0_5

#define SYS_GPA_MFPL_PA7MFP_EPWM0_5

GPA_MFPL PA7 setting for EPWM0 CH5

Definition at line 199 of file sys.h.

## ◆ SYS_GPA_MFPL_PA7MFP_EPWM0_CH5

#define SYS_GPA_MFPL_PA7MFP_EPWM0_CH5

GPA_MFPL PA7 setting for EPWM0 CH5

Definition at line 198 of file sys.h.

## ◆ SYS_GPA_MFPL_PA7MFP_GPIO

#define SYS_GPA_MFPL_PA7MFP_GPIO

GPA_MFPL PA7 setting for GPIO

Definition at line 193 of file sys.h.

## ◆ SYS_GPA_MFPL_PA7MFP_PWM1_3

#define SYS_GPA_MFPL_PA7MFP_PWM1_3

GPA_MFPL PA7 setting for PWM1 CH3

Definition at line 197 of file sys.h.

## ◆ SYS_GPA_MFPL_PA7MFP_PWM1_CH3

#define SYS_GPA_MFPL_PA7MFP_PWM1_CH3

GPA_MFPL PA7 setting for PWM1 CH3

Definition at line 196 of file sys.h.

## ◆ SYS_GPA_MFPL_PA7MFP_SC0_CLK

#define SYS_GPA_MFPL_PA7MFP_SC0_CLK

GPA_MFPL PA7 setting for SC0_CLK

Definition at line 194 of file sys.h.

## ◆ SYS_GPA_MFPL_PA7MFP_SPI3_SS0

#define SYS_GPA_MFPL_PA7MFP_SPI3_SS0

GPA_MFPL PA7 setting for SPI3_SS0

Definition at line 195 of file sys.h.

## ◆ SYS_GPB_MFPH_PB10MFP_EBI_AD12

#define SYS_GPB_MFPH_PB10MFP_EBI_AD12

GPB_MFPH PB10 setting for EBI_AD12

Definition at line 361 of file sys.h.

## ◆ SYS_GPB_MFPH_PB10MFP_EPWM1_4

#define SYS_GPB_MFPH_PB10MFP_EPWM1_4

GPB_MFPH PB10 setting for EPWM1_CH4

Definition at line 359 of file sys.h.

## ◆ SYS_GPB_MFPH_PB10MFP_EPWM1_CH4

#define SYS_GPB_MFPH_PB10MFP_EPWM1_CH4

GPB_MFPH PB10 setting for EPWM1_CH4

Definition at line 358 of file sys.h.

## ◆ SYS_GPB_MFPH_PB10MFP_ETM_TRACE_DATA0

#define SYS_GPB_MFPH_PB10MFP_ETM_TRACE_DATA0

GPB_MFPH PB10 setting for ETM_TRACE_DATA0

Definition at line 360 of file sys.h.

## ◆ SYS_GPB_MFPH_PB10MFP_GPIO

#define SYS_GPB_MFPH_PB10MFP_GPIO

GPB_MFPH PB10 setting for GPIO

Definition at line 356 of file sys.h.

## ◆ SYS_GPB_MFPH_PB10MFP_UART5_TXD

#define SYS_GPB_MFPH_PB10MFP_UART5_TXD

GPB_MFPH PB10 setting for UART5_TXD

Definition at line 357 of file sys.h.

## ◆ SYS_GPB_MFPH_PB11MFP_EBI_AD13

#define SYS_GPB_MFPH_PB11MFP_EBI_AD13

GPB_MFPH PB11 setting for EBI_AD13

Definition at line 369 of file sys.h.

## ◆ SYS_GPB_MFPH_PB11MFP_EPWM1_5

#define SYS_GPB_MFPH_PB11MFP_EPWM1_5

GPB_MFPH PB11 setting for EPWM1_CH5

Definition at line 367 of file sys.h.

## ◆ SYS_GPB_MFPH_PB11MFP_EPWM1_CH5

#define SYS_GPB_MFPH_PB11MFP_EPWM1_CH5

GPB_MFPH PB11 setting for EPWM1_CH5

Definition at line 366 of file sys.h.

## ◆ SYS_GPB_MFPH_PB11MFP_ETM_TRACE_CLK

#define SYS_GPB_MFPH_PB11MFP_ETM_TRACE_CLK

GPB_MFPH PB11 setting for ETM_TRACE_CLK

Definition at line 368 of file sys.h.

## ◆ SYS_GPB_MFPH_PB11MFP_GPIO

#define SYS_GPB_MFPH_PB11MFP_GPIO

GPB_MFPH PB11 setting for GPIO

Definition at line 364 of file sys.h.

## ◆ SYS_GPB_MFPH_PB11MFP_UART5_RXD

#define SYS_GPB_MFPH_PB11MFP_UART5_RXD

GPB_MFPH PB11 setting for UART5_RXD

Definition at line 365 of file sys.h.

## ◆ SYS_GPB_MFPH_PB12MFP_CAN0_RXD

#define SYS_GPB_MFPH_PB12MFP_CAN0_RXD

GPB_MFPH PB12 setting for CAN0_RXD

Definition at line 375 of file sys.h.

## ◆ SYS_GPB_MFPH_PB12MFP_EBI_AD14

#define SYS_GPB_MFPH_PB12MFP_EBI_AD14

GPB_MFPH PB12 setting for EBI_AD4

Definition at line 377 of file sys.h.

## ◆ SYS_GPB_MFPH_PB12MFP_EMAC_MII_MDC

#define SYS_GPB_MFPH_PB12MFP_EMAC_MII_MDC

GPB_MFPH PB12 setting for EMAC_MII_MDC

Definition at line 376 of file sys.h.

## ◆ SYS_GPB_MFPH_PB12MFP_GPIO

#define SYS_GPB_MFPH_PB12MFP_GPIO

GPB_MFPH PB12 setting for GPIO

Definition at line 372 of file sys.h.

## ◆ SYS_GPB_MFPH_PB12MFP_SPI2_MISO1

#define SYS_GPB_MFPH_PB12MFP_SPI2_MISO1

GPB_MFPH PB12 setting for _SPI2_MISO1

Definition at line 374 of file sys.h.

## ◆ SYS_GPB_MFPH_PB12MFP_UART4_RTS

#define SYS_GPB_MFPH_PB12MFP_UART4_RTS

GPB_MFPH PB12 setting for UART4_RTS

Definition at line 373 of file sys.h.

## ◆ SYS_GPB_MFPH_PB13MFP_CAN0_TXD

#define SYS_GPB_MFPH_PB13MFP_CAN0_TXD

GPB_MFPH PB13 setting for CAN0_TXD

Definition at line 383 of file sys.h.

## ◆ SYS_GPB_MFPH_PB13MFP_EBI_AD15

#define SYS_GPB_MFPH_PB13MFP_EBI_AD15

GPB_MFPH PB13 setting for EBI_AD15

Definition at line 385 of file sys.h.

## ◆ SYS_GPB_MFPH_PB13MFP_EMAC_MII_MDIO

#define SYS_GPB_MFPH_PB13MFP_EMAC_MII_MDIO

GPB_MFPH PB13 setting for EMAC_MII_MDIO

Definition at line 384 of file sys.h.

## ◆ SYS_GPB_MFPH_PB13MFP_GPIO

#define SYS_GPB_MFPH_PB13MFP_GPIO

GPB_MFPH PB13 setting for GPIO

Definition at line 380 of file sys.h.

## ◆ SYS_GPB_MFPH_PB13MFP_SPI2_MOSI1

#define SYS_GPB_MFPH_PB13MFP_SPI2_MOSI1

GPB_MFPH PB13 setting for SPI2_MOSI1

Definition at line 382 of file sys.h.

## ◆ SYS_GPB_MFPH_PB13MFP_UART4_CTS

#define SYS_GPB_MFPH_PB13MFP_UART4_CTS

GPB_MFPH PB13 setting for UART4_CTS

Definition at line 381 of file sys.h.

## ◆ SYS_GPB_MFPH_PB14MFP_BRAKE01

#define SYS_GPB_MFPH_PB14MFP_BRAKE01

GPB_MFPH PB14 setting for BRAKE01

Definition at line 391 of file sys.h.

## ◆ SYS_GPB_MFPH_PB14MFP_EMAC_MII_MDC

#define SYS_GPB_MFPH_PB14MFP_EMAC_MII_MDC

GPB_MFPH PB14 setting for EMAC_MII_MDC

Definition at line 392 of file sys.h.

## ◆ SYS_GPB_MFPH_PB14MFP_GPIO

#define SYS_GPB_MFPH_PB14MFP_GPIO

GPB_MFPH PB14 setting for GPIO

Definition at line 388 of file sys.h.

## ◆ SYS_GPB_MFPH_PB14MFP_I2S1_MCLK

#define SYS_GPB_MFPH_PB14MFP_I2S1_MCLK

GPB_MFPH PB14 setting for I2S1_MCLK

Definition at line 389 of file sys.h.

## ◆ SYS_GPB_MFPH_PB14MFP_SC1_RST

#define SYS_GPB_MFPH_PB14MFP_SC1_RST

GPB_MFPH PB14 setting for SC1_RST

Definition at line 390 of file sys.h.

## ◆ SYS_GPB_MFPH_PB15MFP_BRAKE00

#define SYS_GPB_MFPH_PB15MFP_BRAKE00

GPA_MFPH PB15 setting for BRAKE00

Definition at line 398 of file sys.h.

## ◆ SYS_GPB_MFPH_PB15MFP_EMAC_MII_MDIO

#define SYS_GPB_MFPH_PB15MFP_EMAC_MII_MDIO

GPA_MFPH PB15 setting for EMAC_MII_MDIO

Definition at line 399 of file sys.h.

## ◆ SYS_GPB_MFPH_PB15MFP_GPIO

#define SYS_GPB_MFPH_PB15MFP_GPIO

GPA_MFPH PB15 setting for GPIO

Definition at line 395 of file sys.h.

## ◆ SYS_GPB_MFPH_PB15MFP_I2S1_DO

#define SYS_GPB_MFPH_PB15MFP_I2S1_DO

GPA_MFPH PB15 setting for I2S1_DO

Definition at line 396 of file sys.h.

## ◆ SYS_GPB_MFPH_PB15MFP_SC1_DAT

#define SYS_GPB_MFPH_PB15MFP_SC1_DAT

GPA_MFPH PB15 setting for SC1_DAT

Definition at line 397 of file sys.h.

## ◆ SYS_GPB_MFPH_PB8MFP_EBI_AD10

#define SYS_GPB_MFPH_PB8MFP_EBI_AD10

GPB_MFPH PB8 setting for EBI_AD10

Definition at line 345 of file sys.h.

## ◆ SYS_GPB_MFPH_PB8MFP_EPWM1_2

#define SYS_GPB_MFPH_PB8MFP_EPWM1_2

GPB_MFPH PB8 setting for EPWM1_CH2

Definition at line 343 of file sys.h.

## ◆ SYS_GPB_MFPH_PB8MFP_EPWM1_CH2

#define SYS_GPB_MFPH_PB8MFP_EPWM1_CH2

GPB_MFPH PB8 setting for EPWM1_CH2

Definition at line 342 of file sys.h.

## ◆ SYS_GPB_MFPH_PB8MFP_ETM_TRACE_DATA2

#define SYS_GPB_MFPH_PB8MFP_ETM_TRACE_DATA2

GPB_MFPH PB8 setting for ETM_TRACE_DATA2

Definition at line 344 of file sys.h.

## ◆ SYS_GPB_MFPH_PB8MFP_GPIO

#define SYS_GPB_MFPH_PB8MFP_GPIO

GPB_MFPH PB8 setting for GPIO

Definition at line 340 of file sys.h.

## ◆ SYS_GPB_MFPH_PB8MFP_UART5_CTS

#define SYS_GPB_MFPH_PB8MFP_UART5_CTS

GPB_MFPH PB8 setting for UART5_CTS

Definition at line 341 of file sys.h.

## ◆ SYS_GPB_MFPH_PB9MFP_EBI_AD11

#define SYS_GPB_MFPH_PB9MFP_EBI_AD11

GPB_MFPH PB9 setting for EBI_AD11

Definition at line 353 of file sys.h.

## ◆ SYS_GPB_MFPH_PB9MFP_EPWM1_3

#define SYS_GPB_MFPH_PB9MFP_EPWM1_3

GPB_MFPH PB9 setting for EPWM1_CH3

Definition at line 351 of file sys.h.

## ◆ SYS_GPB_MFPH_PB9MFP_EPWM1_CH3

#define SYS_GPB_MFPH_PB9MFP_EPWM1_CH3

GPB_MFPH PB9 setting for EPWM1_CH3

Definition at line 350 of file sys.h.

## ◆ SYS_GPB_MFPH_PB9MFP_ETM_TRACE_DATA1

#define SYS_GPB_MFPH_PB9MFP_ETM_TRACE_DATA1

GPB_MFPH PB9 setting for ETM_TRACE_DATA1

Definition at line 352 of file sys.h.

## ◆ SYS_GPB_MFPH_PB9MFP_GPIO

#define SYS_GPB_MFPH_PB9MFP_GPIO

GPB_MFPH PB9 setting for GPIO

Definition at line 348 of file sys.h.

## ◆ SYS_GPB_MFPH_PB9MFP_UART5_RTS

#define SYS_GPB_MFPH_PB9MFP_UART5_RTS

GPB_MFPH PB9 setting for UART5_RTS

Definition at line 349 of file sys.h.

## ◆ SYS_GPB_MFPL_PB0MFP_GPIO

#define SYS_GPB_MFPL_PB0MFP_GPIO

GPB_MFPL PB0 setting for GPIO

Definition at line 276 of file sys.h.

## ◆ SYS_GPB_MFPL_PB0MFP_I2C4_SCL

#define SYS_GPB_MFPL_PB0MFP_I2C4_SCL

GPB_MFPL PB0 setting for I2C4_SCL

Definition at line 278 of file sys.h.

## ◆ SYS_GPB_MFPL_PB0MFP_INT1

#define SYS_GPB_MFPL_PB0MFP_INT1

GPB_MFPL PB0 setting for INT1

Definition at line 279 of file sys.h.

## ◆ SYS_GPB_MFPL_PB0MFP_USB0_OTG5V_ST

#define SYS_GPB_MFPL_PB0MFP_USB0_OTG5V_ST

GPB_MFPL PB0 setting for USB0_OTG5V_ST

Definition at line 277 of file sys.h.

## ◆ SYS_GPB_MFPL_PB1MFP_GPIO

#define SYS_GPB_MFPL_PB1MFP_GPIO

GPB_MFPL PB1 setting for GPIO

Definition at line 282 of file sys.h.

## ◆ SYS_GPB_MFPL_PB1MFP_I2C4_SDA

#define SYS_GPB_MFPL_PB1MFP_I2C4_SDA

GPB_MFPL PB1 setting for I2C4_SDA

Definition at line 284 of file sys.h.

## ◆ SYS_GPB_MFPL_PB1MFP_TM1_CNT_OUT

#define SYS_GPB_MFPL_PB1MFP_TM1_CNT_OUT

GPB_MFPL PB1 setting for TM1_CNT_OUT

Definition at line 285 of file sys.h.

## ◆ SYS_GPB_MFPL_PB1MFP_USB0_OTG5V_EN

#define SYS_GPB_MFPL_PB1MFP_USB0_OTG5V_EN

GPB_MFPL PB1 setting for USB0_OTG5V_EN

Definition at line 283 of file sys.h.

## ◆ SYS_GPB_MFPL_PB2MFP_EBI_AD4

#define SYS_GPB_MFPL_PB2MFP_EBI_AD4

GPB_MFPL PB2 setting for EBI_AD4

Definition at line 292 of file sys.h.

## ◆ SYS_GPB_MFPL_PB2MFP_GPIO

#define SYS_GPB_MFPL_PB2MFP_GPIO

GPB_MFPL PB2 setting for GPIO

Definition at line 288 of file sys.h.

## ◆ SYS_GPB_MFPL_PB2MFP_SPI2_SS0

#define SYS_GPB_MFPL_PB2MFP_SPI2_SS0

GPB_MFPL PB2 setting for SPI2_SS0

Definition at line 290 of file sys.h.

## ◆ SYS_GPB_MFPL_PB2MFP_UART1_RXD

#define SYS_GPB_MFPL_PB2MFP_UART1_RXD

GPB_MFPL PB2 setting for UART1_RXD

Definition at line 289 of file sys.h.

## ◆ SYS_GPB_MFPL_PB2MFP_USB1_D_N

#define SYS_GPB_MFPL_PB2MFP_USB1_D_N

GPB_MFPL PB2 setting for USB1_D_N

Definition at line 291 of file sys.h.

## ◆ SYS_GPB_MFPL_PB3MFP_EBI_AD5

#define SYS_GPB_MFPL_PB3MFP_EBI_AD5

GPB_MFPL PB3 setting for EBI_AD5

Definition at line 299 of file sys.h.

## ◆ SYS_GPB_MFPL_PB3MFP_GPIO

#define SYS_GPB_MFPL_PB3MFP_GPIO

GPB_MFPL PB3 setting for GPIO

Definition at line 295 of file sys.h.

## ◆ SYS_GPB_MFPL_PB3MFP_SPI2_CLK

#define SYS_GPB_MFPL_PB3MFP_SPI2_CLK

GPB_MFPL PB3 setting for SPI2_CLK

Definition at line 297 of file sys.h.

## ◆ SYS_GPB_MFPL_PB3MFP_UART1_TXD

#define SYS_GPB_MFPL_PB3MFP_UART1_TXD

GPB_MFPL PB3 setting for UART1_TXD

Definition at line 296 of file sys.h.

## ◆ SYS_GPB_MFPL_PB3MFP_USB1_D_P

#define SYS_GPB_MFPL_PB3MFP_USB1_D_P

GPB_MFPL PB3 setting for USB1_D_P

Definition at line 298 of file sys.h.

## ◆ SYS_GPB_MFPL_PB4MFP_EBI_AD6

#define SYS_GPB_MFPL_PB4MFP_EBI_AD6

GPB_MFPL PB4 setting for EBI_AD6

Definition at line 307 of file sys.h.

## ◆ SYS_GPB_MFPL_PB4MFP_GPIO

#define SYS_GPB_MFPL_PB4MFP_GPIO

GPB_MFPL PB4 setting for GPIO

Definition at line 302 of file sys.h.

## ◆ SYS_GPB_MFPL_PB4MFP_SPI2_MISO0

#define SYS_GPB_MFPL_PB4MFP_SPI2_MISO0

GPB_MFPL PB4 setting for SPI2_MISO0

Definition at line 304 of file sys.h.

## ◆ SYS_GPB_MFPL_PB4MFP_TM0_CNT_OUT

#define SYS_GPB_MFPL_PB4MFP_TM0_CNT_OUT

GPB_MFPL PB4 setting for TM0_CNT_OUT

Definition at line 306 of file sys.h.

## ◆ SYS_GPB_MFPL_PB4MFP_UART1_RTS

#define SYS_GPB_MFPL_PB4MFP_UART1_RTS

GPB_MFPL PB4 setting for UART1_RTS

Definition at line 303 of file sys.h.

## ◆ SYS_GPB_MFPL_PB4MFP_UART4_RXD

#define SYS_GPB_MFPL_PB4MFP_UART4_RXD

GPB_MFPL PB4 setting for UART4_RXD

Definition at line 305 of file sys.h.

## ◆ SYS_GPB_MFPL_PB5MFP_EBI_AD7

#define SYS_GPB_MFPL_PB5MFP_EBI_AD7

GPB_MFPL PB5 setting for EBI_AD7

Definition at line 314 of file sys.h.

## ◆ SYS_GPB_MFPL_PB5MFP_GPIO

#define SYS_GPB_MFPL_PB5MFP_GPIO

GPB_MFPL PB5 setting for GPIO

Definition at line 310 of file sys.h.

## ◆ SYS_GPB_MFPL_PB5MFP_SPI2_MOSI0

#define SYS_GPB_MFPL_PB5MFP_SPI2_MOSI0

GPB_MFPL PB5 setting for SPI2_MOSI0

Definition at line 312 of file sys.h.

## ◆ SYS_GPB_MFPL_PB5MFP_UART1_CTS

#define SYS_GPB_MFPL_PB5MFP_UART1_CTS

GPB_MFPL PB5 setting for UART1_CTS

Definition at line 311 of file sys.h.

## ◆ SYS_GPB_MFPL_PB5MFP_UART4_TXD

#define SYS_GPB_MFPL_PB5MFP_UART4_TXD

GPB_MFPL PB5 setting for UART4_TXD

Definition at line 313 of file sys.h.

## ◆ SYS_GPB_MFPL_PB6MFP_BRAKE01

#define SYS_GPB_MFPL_PB6MFP_BRAKE01

GPB_MFPL PB6 setting for BRAKE01

Definition at line 319 of file sys.h.

## ◆ SYS_GPB_MFPL_PB6MFP_EBI_AD8

#define SYS_GPB_MFPL_PB6MFP_EBI_AD8

GPB_MFPL PB6 setting for EBI_AD8

Definition at line 325 of file sys.h.

## ◆ SYS_GPB_MFPL_PB6MFP_EPWM1_0

#define SYS_GPB_MFPL_PB6MFP_EPWM1_0

GPB_MFPL PB6 setting for EPWM1_CH0

Definition at line 324 of file sys.h.

## ◆ SYS_GPB_MFPL_PB6MFP_EPWM1_CH0

#define SYS_GPB_MFPL_PB6MFP_EPWM1_CH0

GPB_MFPL PB6 setting for EPWM1_CH0

Definition at line 323 of file sys.h.

## ◆ SYS_GPB_MFPL_PB6MFP_GPIO

#define SYS_GPB_MFPL_PB6MFP_GPIO

GPB_MFPL PB6 setting for GPIO

Definition at line 317 of file sys.h.

## ◆ SYS_GPB_MFPL_PB6MFP_I2C2_SCL

#define SYS_GPB_MFPL_PB6MFP_I2C2_SCL

GPB_MFPL PB6 setting for I2C2_SCL

Definition at line 318 of file sys.h.

## ◆ SYS_GPB_MFPL_PB6MFP_PWM1_4

#define SYS_GPB_MFPL_PB6MFP_PWM1_4

GPB_MFPL PB6 setting for PWM1_CH4

Definition at line 322 of file sys.h.

## ◆ SYS_GPB_MFPL_PB6MFP_PWM1_CH4

#define SYS_GPB_MFPL_PB6MFP_PWM1_CH4

GPB_MFPL PB6 setting for PWM1_CH4

Definition at line 321 of file sys.h.

## ◆ SYS_GPB_MFPL_PB6MFP_UART4_RTS

#define SYS_GPB_MFPL_PB6MFP_UART4_RTS

GPB_MFPL PB6 setting for UART4_RTS

Definition at line 320 of file sys.h.

## ◆ SYS_GPB_MFPL_PB7MFP_BRAKE00

#define SYS_GPB_MFPL_PB7MFP_BRAKE00

GPB_MFPL PB7 setting for BRAKE00

Definition at line 330 of file sys.h.

## ◆ SYS_GPB_MFPL_PB7MFP_EBI_AD9

#define SYS_GPB_MFPL_PB7MFP_EBI_AD9

GPB_MFPL PB7 setting for EBI_AD9

Definition at line 337 of file sys.h.

## ◆ SYS_GPB_MFPL_PB7MFP_EPWM1_1

#define SYS_GPB_MFPL_PB7MFP_EPWM1_1

GPB_MFPL PB7 setting for EPWM1_CH1

Definition at line 335 of file sys.h.

## ◆ SYS_GPB_MFPL_PB7MFP_EPWM1_CH1

#define SYS_GPB_MFPL_PB7MFP_EPWM1_CH1

GPB_MFPL PB7 setting for EPWM1_CH1

Definition at line 334 of file sys.h.

## ◆ SYS_GPB_MFPL_PB7MFP_ETM_TRACE_DATA3

#define SYS_GPB_MFPL_PB7MFP_ETM_TRACE_DATA3

GPB_MFPL PB7 setting for ETM_TRACE_DATA3

Definition at line 336 of file sys.h.

## ◆ SYS_GPB_MFPL_PB7MFP_GPIO

#define SYS_GPB_MFPL_PB7MFP_GPIO

GPB_MFPL PB7 setting for GPIO

Definition at line 328 of file sys.h.

## ◆ SYS_GPB_MFPL_PB7MFP_I2C2_SDA

#define SYS_GPB_MFPL_PB7MFP_I2C2_SDA

GPB_MFPL PB7 setting for I2C2_SDA

Definition at line 329 of file sys.h.

## ◆ SYS_GPB_MFPL_PB7MFP_PWM1_5

#define SYS_GPB_MFPL_PB7MFP_PWM1_5

GPB_MFPL PB7 setting for PWM1_CH5

Definition at line 333 of file sys.h.

## ◆ SYS_GPB_MFPL_PB7MFP_PWM1_CH5

#define SYS_GPB_MFPL_PB7MFP_PWM1_CH5

GPB_MFPL PB7 setting for PWM1_CH5

Definition at line 332 of file sys.h.

## ◆ SYS_GPB_MFPL_PB7MFP_UART4_CTS

#define SYS_GPB_MFPL_PB7MFP_UART4_CTS

GPB_MFPL PB7 setting for UART4_CTS

Definition at line 331 of file sys.h.

## ◆ SYS_GPC_MFPH_PC10MFP_EBI_A23

#define SYS_GPC_MFPH_PC10MFP_EBI_A23

GPC_MFPH PC10 setting for EBI_A23

Definition at line 498 of file sys.h.

## ◆ SYS_GPC_MFPH_PC10MFP_EBI_AD2

#define SYS_GPC_MFPH_PC10MFP_EBI_AD2

GPC_MFPH PC10 setting for EBI_AD2

Definition at line 499 of file sys.h.

## ◆ SYS_GPC_MFPH_PC10MFP_GPIO

#define SYS_GPC_MFPH_PC10MFP_GPIO

GPC_MFPH PC10 setting for GPIO

Definition at line 493 of file sys.h.

## ◆ SYS_GPC_MFPH_PC10MFP_PWM0_2

#define SYS_GPC_MFPH_PC10MFP_PWM0_2

GPC_MFPH PC10 setting for PWM0_CH2

Definition at line 497 of file sys.h.

## ◆ SYS_GPC_MFPH_PC10MFP_PWM0_CH2

#define SYS_GPC_MFPH_PC10MFP_PWM0_CH2

GPC_MFPH PC10 setting for PWM0_CH2

Definition at line 496 of file sys.h.

## ◆ SYS_GPC_MFPH_PC10MFP_SC3_CD

#define SYS_GPC_MFPH_PC10MFP_SC3_CD

GPC_MFPH PC10 setting for SC3_CD

Definition at line 494 of file sys.h.

## ◆ SYS_GPC_MFPH_PC10MFP_UART2_RXD

#define SYS_GPC_MFPH_PC10MFP_UART2_RXD

GPC_MFPH PC10 setting for UART2_RXD

Definition at line 495 of file sys.h.

## ◆ SYS_GPC_MFPH_PC11MFP_EBI_A24

#define SYS_GPC_MFPH_PC11MFP_EBI_A24

GPC_MFPH PC11 setting for EBI_A24

Definition at line 506 of file sys.h.

## ◆ SYS_GPC_MFPH_PC11MFP_EBI_AD3

#define SYS_GPC_MFPH_PC11MFP_EBI_AD3

GPC_MFPH PC11 setting for EBI_AD3

Definition at line 507 of file sys.h.

## ◆ SYS_GPC_MFPH_PC11MFP_GPIO

#define SYS_GPC_MFPH_PC11MFP_GPIO

GPC_MFPH PC11 setting for GPIO

Definition at line 502 of file sys.h.

## ◆ SYS_GPC_MFPH_PC11MFP_PWM0_3

#define SYS_GPC_MFPH_PC11MFP_PWM0_3

GPC_MFPH PC11 setting for PWM0_CH3

Definition at line 505 of file sys.h.

## ◆ SYS_GPC_MFPH_PC11MFP_PWM0_CH3

#define SYS_GPC_MFPH_PC11MFP_PWM0_CH3

GPC_MFPH PC11 setting for PWM0_CH3

Definition at line 504 of file sys.h.

## ◆ SYS_GPC_MFPH_PC11MFP_UART2_TXD

#define SYS_GPC_MFPH_PC11MFP_UART2_TXD

GPC_MFPH PC11 setting for UART2_TXD

Definition at line 503 of file sys.h.

## ◆ SYS_GPC_MFPH_PC12MFP_CAP_DATA7

#define SYS_GPC_MFPH_PC12MFP_CAP_DATA7

GPC_MFPH PC12 setting for CAP_DATA7

Definition at line 514 of file sys.h.

## ◆ SYS_GPC_MFPH_PC12MFP_EBI_A0

#define SYS_GPC_MFPH_PC12MFP_EBI_A0

GPC_MFPH PC12 setting for MFP_EBI_A0

Definition at line 516 of file sys.h.

## ◆ SYS_GPC_MFPH_PC12MFP_ETM_TRACE_DATA3

#define SYS_GPC_MFPH_PC12MFP_ETM_TRACE_DATA3

GPC_MFPH PC12 setting for ETM_TRACE_DATA3

Definition at line 515 of file sys.h.

## ◆ SYS_GPC_MFPH_PC12MFP_GPIO

#define SYS_GPC_MFPH_PC12MFP_GPIO

GPC_MFPH PC12 setting for GPIO

Definition at line 510 of file sys.h.

## ◆ SYS_GPC_MFPH_PC12MFP_SC4_CD

#define SYS_GPC_MFPH_PC12MFP_SC4_CD

GPC_MFPH PC12 setting for SC4_CD

Definition at line 512 of file sys.h.

## ◆ SYS_GPC_MFPH_PC12MFP_SD1_CDn

#define SYS_GPC_MFPH_PC12MFP_SD1_CDn

GPC_MFPH PC12 setting for SD1_CDn

Definition at line 513 of file sys.h.

## ◆ SYS_GPC_MFPH_PC12MFP_SPI1_SS0

#define SYS_GPC_MFPH_PC12MFP_SPI1_SS0

GPC_MFPH PC12 setting for SPI1_SS0

Definition at line 511 of file sys.h.

## ◆ SYS_GPC_MFPH_PC13MFP_CAP_DATA6

#define SYS_GPC_MFPH_PC13MFP_CAP_DATA6

GPC_MFPH PC13 setting for CAP_DATA6

Definition at line 523 of file sys.h.

## ◆ SYS_GPC_MFPH_PC13MFP_EBI_A1

#define SYS_GPC_MFPH_PC13MFP_EBI_A1

GPC_MFPH PC13 setting for EBI_A1

Definition at line 525 of file sys.h.

## ◆ SYS_GPC_MFPH_PC13MFP_ETM_TRACE_DATA2

#define SYS_GPC_MFPH_PC13MFP_ETM_TRACE_DATA2

GPC_MFPH PC13 setting for ETM_TRACE_DATA2

Definition at line 524 of file sys.h.

## ◆ SYS_GPC_MFPH_PC13MFP_GPIO

#define SYS_GPC_MFPH_PC13MFP_GPIO

GPC_MFPH PC13 setting for GPIO

Definition at line 519 of file sys.h.

## ◆ SYS_GPC_MFPH_PC13MFP_SC4_RST

#define SYS_GPC_MFPH_PC13MFP_SC4_RST

GPC_MFPH PC13 setting for SC4_RST

Definition at line 521 of file sys.h.

## ◆ SYS_GPC_MFPH_PC13MFP_SD1_CMD

#define SYS_GPC_MFPH_PC13MFP_SD1_CMD

GPC_MFPH PC13 setting for SD1_CMD

Definition at line 522 of file sys.h.

## ◆ SYS_GPC_MFPH_PC13MFP_SPI1_MOSI1

#define SYS_GPC_MFPH_PC13MFP_SPI1_MOSI1

GPC_MFPH PC13 setting for SPI1_MOSI1

Definition at line 520 of file sys.h.

## ◆ SYS_GPC_MFPH_PC14MFP_CAP_DATA5

#define SYS_GPC_MFPH_PC14MFP_CAP_DATA5

GPC_MFPH PC14 setting for CAP_DATA5

Definition at line 533 of file sys.h.

## ◆ SYS_GPC_MFPH_PC14MFP_EBI_A2

#define SYS_GPC_MFPH_PC14MFP_EBI_A2

GPC_MFPH PC14 setting for EBI_A2

Definition at line 535 of file sys.h.

## ◆ SYS_GPC_MFPH_PC14MFP_ETM_TRACE_DATA1

#define SYS_GPC_MFPH_PC14MFP_ETM_TRACE_DATA1

GPC_MFPH PC14 setting for ETM_TRACE_DATA1

Definition at line 534 of file sys.h.

## ◆ SYS_GPC_MFPH_PC14MFP_GPIO

#define SYS_GPC_MFPH_PC14MFP_GPIO

GPC_MFPH PC14 setting for GPIO

Definition at line 528 of file sys.h.

## ◆ SYS_GPC_MFPH_PC14MFP_SC4_PWR

#define SYS_GPC_MFPH_PC14MFP_SC4_PWR

GPC_MFPH PC14 setting for SC4_PWR

Definition at line 530 of file sys.h.

## ◆ SYS_GPC_MFPH_PC14MFP_SD1_CLK

#define SYS_GPC_MFPH_PC14MFP_SD1_CLK

GPC_MFPH PC14 setting for SD1_CLK

Definition at line 532 of file sys.h.

## ◆ SYS_GPC_MFPH_PC14MFP_SPI1_MISO1

#define SYS_GPC_MFPH_PC14MFP_SPI1_MISO1

GPC_MFPH PC14 setting for SPI1_MISO1

Definition at line 529 of file sys.h.

## ◆ SYS_GPC_MFPH_PC14MFP_TM3_EXT

#define SYS_GPC_MFPH_PC14MFP_TM3_EXT

GPC_MFPH PC14 setting for TM3_EXT

Definition at line 531 of file sys.h.

## ◆ SYS_GPC_MFPH_PC15MFP_CAP_DATA4

#define SYS_GPC_MFPH_PC15MFP_CAP_DATA4

GPC_MFPH PC15 setting for CAP_DATA4

Definition at line 542 of file sys.h.

## ◆ SYS_GPC_MFPH_PC15MFP_EBI_A3

#define SYS_GPC_MFPH_PC15MFP_EBI_A3

GPC_MFPH PC15 setting for EBI_A3

Definition at line 544 of file sys.h.

## ◆ SYS_GPC_MFPH_PC15MFP_ETM_TRACE_DATA0

#define SYS_GPC_MFPH_PC15MFP_ETM_TRACE_DATA0

GPC_MFPH PC15 setting for ETM_TRACE_DATA0

Definition at line 543 of file sys.h.

## ◆ SYS_GPC_MFPH_PC15MFP_GPIO

#define SYS_GPC_MFPH_PC15MFP_GPIO

GPC_MFPH PC15 setting for GPIO

Definition at line 538 of file sys.h.

## ◆ SYS_GPC_MFPH_PC15MFP_SC4_DAT

#define SYS_GPC_MFPH_PC15MFP_SC4_DAT

GPC_MFPH PC15 setting for SC4_DAT

Definition at line 540 of file sys.h.

## ◆ SYS_GPC_MFPH_PC15MFP_SD1_DAT3

#define SYS_GPC_MFPH_PC15MFP_SD1_DAT3

GPC_MFPH PC15 setting for SD1_DAT3

Definition at line 541 of file sys.h.

## ◆ SYS_GPC_MFPH_PC15MFP_SPI1_MOSI0

#define SYS_GPC_MFPH_PC15MFP_SPI1_MOSI0

GPC_MFPH PC15 setting for SPI1_MOSI0

Definition at line 539 of file sys.h.

## ◆ SYS_GPC_MFPH_PC8MFP_EMAC_MII_TXEN

#define SYS_GPC_MFPH_PC8MFP_EMAC_MII_TXEN

GPC_MFPH PC8 setting for EMAC_MII_TXEN

Definition at line 479 of file sys.h.

## ◆ SYS_GPC_MFPH_PC8MFP_GPIO

#define SYS_GPC_MFPH_PC8MFP_GPIO

GPC_MFPH PC8 setting for GPIO

Definition at line 476 of file sys.h.

## ◆ SYS_GPC_MFPH_PC8MFP_SPI0_CLK

#define SYS_GPC_MFPH_PC8MFP_SPI0_CLK

GPC_MFPH PC8 setting for SPI0_CLK

Definition at line 478 of file sys.h.

## ◆ SYS_GPC_MFPH_PC8MFP_TM0_EXT

#define SYS_GPC_MFPH_PC8MFP_TM0_EXT

GPC_MFPH PC8 setting for TM0_EXT

Definition at line 477 of file sys.h.

## ◆ SYS_GPC_MFPH_PC9MFP_CAP_DATA1

#define SYS_GPC_MFPH_PC9MFP_CAP_DATA1

GPC_MFPH PC9 setting for CAP_DATA1

Definition at line 487 of file sys.h.

## ◆ SYS_GPC_MFPH_PC9MFP_EBI_A22

#define SYS_GPC_MFPH_PC9MFP_EBI_A22

GPC_MFPH PC9 setting for EBI_A22

Definition at line 489 of file sys.h.

## ◆ SYS_GPC_MFPH_PC9MFP_EBI_A6

#define SYS_GPC_MFPH_PC9MFP_EBI_A6

GPC_MFPH PC9 setting for EBI_A6

Definition at line 491 of file sys.h.

## ◆ SYS_GPC_MFPH_PC9MFP_GPIO

#define SYS_GPC_MFPH_PC9MFP_GPIO

GPC_MFPH PC9 setting for GPIO

Definition at line 482 of file sys.h.

## ◆ SYS_GPC_MFPH_PC9MFP_I2C0_SDA

#define SYS_GPC_MFPH_PC9MFP_I2C0_SDA

GPC_MFPH PC9 setting for I2C0_SDA

Definition at line 486 of file sys.h.

## ◆ SYS_GPC_MFPH_PC9MFP_I2C3_SCL

#define SYS_GPC_MFPH_PC9MFP_I2C3_SCL

GPC_MFPH PC9 setting for I2C3_SCL

Definition at line 488 of file sys.h.

## ◆ SYS_GPC_MFPH_PC9MFP_SC3_RST

#define SYS_GPC_MFPH_PC9MFP_SC3_RST

GPC_MFPH PC9 setting for SC3_RST

Definition at line 485 of file sys.h.

## ◆ SYS_GPC_MFPH_PC9MFP_SD1_DAT0

#define SYS_GPC_MFPH_PC9MFP_SD1_DAT0

GPC_MFPH PC9 setting for SD1_DAT0

Definition at line 490 of file sys.h.

## ◆ SYS_GPC_MFPH_PC9MFP_STADC

#define SYS_GPC_MFPH_PC9MFP_STADC

GPC_MFPH PC9 setting for STADC

Definition at line 483 of file sys.h.

## ◆ SYS_GPC_MFPH_PC9MFP_UART2_CTS

#define SYS_GPC_MFPH_PC9MFP_UART2_CTS

GPC_MFPH PC9 setting for UART2_CTS

Definition at line 484 of file sys.h.

## ◆ SYS_GPC_MFPL_PC0MFP_EBI_MCLK

#define SYS_GPC_MFPL_PC0MFP_EBI_MCLK

GPC_MFPL PC0 setting for EBI_MCLK

Definition at line 408 of file sys.h.

## ◆ SYS_GPC_MFPL_PC0MFP_EMAC_REFCLK

#define SYS_GPC_MFPL_PC0MFP_EMAC_REFCLK

GPC_MFPL PC0 setting for EMAC_REFCLK

Definition at line 407 of file sys.h.

## ◆ SYS_GPC_MFPL_PC0MFP_GPIO

#define SYS_GPC_MFPL_PC0MFP_GPIO

GPC_MFPL PC0 setting for GPIO

Definition at line 403 of file sys.h.

## ◆ SYS_GPC_MFPL_PC0MFP_I2S1_DI

#define SYS_GPC_MFPL_PC0MFP_I2S1_DI

GPC_MFPL PC0 setting for I2S1_D1

Definition at line 404 of file sys.h.

## ◆ SYS_GPC_MFPL_PC0MFP_INT2

#define SYS_GPC_MFPL_PC0MFP_INT2

GPC_MFPL PC0 setting for INT2

Definition at line 409 of file sys.h.

## ◆ SYS_GPC_MFPL_PC0MFP_SC1_DAT

#define SYS_GPC_MFPL_PC0MFP_SC1_DAT

GPC_MFPL PC0 setting for SC1_DAT

Definition at line 405 of file sys.h.

## ◆ SYS_GPC_MFPL_PC0MFP_UART4_RXD

#define SYS_GPC_MFPL_PC0MFP_UART4_RXD

GPC_MFPL PC0 setting for UART4_RXD

Definition at line 406 of file sys.h.

## ◆ SYS_GPC_MFPL_PC1MFP_EBI_AD13

#define SYS_GPC_MFPL_PC1MFP_EBI_AD13

GPC_MFPL PC1 setting for EBI_AD13

Definition at line 419 of file sys.h.

## ◆ SYS_GPC_MFPL_PC1MFP_EMAC_MII_RXERR

#define SYS_GPC_MFPL_PC1MFP_EMAC_MII_RXERR

GPC_MFPL PC1 setting for EMAC_MII_RXERR

Definition at line 418 of file sys.h.

## ◆ SYS_GPC_MFPL_PC1MFP_GPIO

#define SYS_GPC_MFPL_PC1MFP_GPIO

GPC_MFPL PC1 setting for GPIO

Definition at line 413 of file sys.h.

## ◆ SYS_GPC_MFPL_PC1MFP_I2S1_BCLK

#define SYS_GPC_MFPL_PC1MFP_I2S1_BCLK

GPC_MFPL PC1 setting for I2S1_BCLK

Definition at line 414 of file sys.h.

## ◆ SYS_GPC_MFPL_PC1MFP_SC1_CLK

#define SYS_GPC_MFPL_PC1MFP_SC1_CLK

GPC_MFPL PC1 setting for SC1_CLK

Definition at line 415 of file sys.h.

## ◆ SYS_GPC_MFPL_PC1MFP_TM3_CNT_OUT

#define SYS_GPC_MFPL_PC1MFP_TM3_CNT_OUT

GPC_MFPL PC1 setting for TM3_CNT_OUT

Definition at line 417 of file sys.h.

## ◆ SYS_GPC_MFPL_PC1MFP_UART4_TXD

#define SYS_GPC_MFPL_PC1MFP_UART4_TXD

GPC_MFPL PC1 setting for UART4_TXD

Definition at line 416 of file sys.h.

## ◆ SYS_GPC_MFPL_PC2MFP_EBI_AD12

#define SYS_GPC_MFPL_PC2MFP_EBI_AD12

GPC_MFPL PC2 setting for EBI_AD12

Definition at line 428 of file sys.h.

## ◆ SYS_GPC_MFPL_PC2MFP_EMAC_MII_RXDV

#define SYS_GPC_MFPL_PC2MFP_EMAC_MII_RXDV

GPC_MFPL PC2 setting for EMAC_MII_RXDV

Definition at line 427 of file sys.h.

## ◆ SYS_GPC_MFPL_PC2MFP_GPIO

#define SYS_GPC_MFPL_PC2MFP_GPIO

GPC_MFPL PC2 setting for GPIO

Definition at line 422 of file sys.h.

## ◆ SYS_GPC_MFPL_PC2MFP_I2S1_LRCK

#define SYS_GPC_MFPL_PC2MFP_I2S1_LRCK

GPC_MFPL PC2 setting for I2S1_LRCK

Definition at line 423 of file sys.h.

## ◆ SYS_GPC_MFPL_PC2MFP_SC1_PWR

#define SYS_GPC_MFPL_PC2MFP_SC1_PWR

GPC_MFPL PC2 setting for SC1_PWR

Definition at line 424 of file sys.h.

## ◆ SYS_GPC_MFPL_PC2MFP_SPI0_SS0

#define SYS_GPC_MFPL_PC2MFP_SPI0_SS0

GPC_MFPL PC2 setting for SPI0_SS0

Definition at line 426 of file sys.h.

## ◆ SYS_GPC_MFPL_PC2MFP_UART4_RTS

#define SYS_GPC_MFPL_PC2MFP_UART4_RTS

GPC_MFPL PC2 setting for UART4_RTS

Definition at line 425 of file sys.h.

## ◆ SYS_GPC_MFPL_PC3MFP_EBI_AD11

#define SYS_GPC_MFPL_PC3MFP_EBI_AD11

GPC_MFPL PC3 setting for EBI_AD11

Definition at line 438 of file sys.h.

## ◆ SYS_GPC_MFPL_PC3MFP_ECAP0_IC2

#define SYS_GPC_MFPL_PC3MFP_ECAP0_IC2

GPC_MFPL PC3 setting for ECAP0_IC2

Definition at line 439 of file sys.h.

## ◆ SYS_GPC_MFPL_PC3MFP_EMAC_MII_RXD1

#define SYS_GPC_MFPL_PC3MFP_EMAC_MII_RXD1

GPC_MFPL PC3 setting for EMAC_MII_RXD1

Definition at line 437 of file sys.h.

## ◆ SYS_GPC_MFPL_PC3MFP_GPIO

#define SYS_GPC_MFPL_PC3MFP_GPIO

GPC_MFPL PC3 setting for GPIO

Definition at line 431 of file sys.h.

## ◆ SYS_GPC_MFPL_PC3MFP_I2S1_MCLK

#define SYS_GPC_MFPL_PC3MFP_I2S1_MCLK

GPC_MFPL PC3 setting for I2S1_MCLK

Definition at line 432 of file sys.h.

## ◆ SYS_GPC_MFPL_PC3MFP_QEI0_Z

#define SYS_GPC_MFPL_PC3MFP_QEI0_Z

GPC_MFPL PC3 setting for QEI0_Z

Definition at line 436 of file sys.h.

## ◆ SYS_GPC_MFPL_PC3MFP_SC1_CD

#define SYS_GPC_MFPL_PC3MFP_SC1_CD

GPC_MFPL PC3 setting for SC1_CD

Definition at line 433 of file sys.h.

## ◆ SYS_GPC_MFPL_PC3MFP_SPI0_MISO1

#define SYS_GPC_MFPL_PC3MFP_SPI0_MISO1

GPC_MFPL PC3 setting for SPI0_MISO1

Definition at line 435 of file sys.h.

## ◆ SYS_GPC_MFPL_PC3MFP_UART4_CTS

#define SYS_GPC_MFPL_PC3MFP_UART4_CTS

GPC_MFPL PC3 setting for UART4_CTS

Definition at line 434 of file sys.h.

## ◆ SYS_GPC_MFPL_PC4MFP_EBI_AD10

#define SYS_GPC_MFPL_PC4MFP_EBI_AD10

GPC_MFPL PC4 setting for EBI_AD10

Definition at line 448 of file sys.h.

## ◆ SYS_GPC_MFPL_PC4MFP_ECAP0_IC1

#define SYS_GPC_MFPL_PC4MFP_ECAP0_IC1

GPC_MFPL PC4 setting for ECAP0_IC1

Definition at line 449 of file sys.h.

## ◆ SYS_GPC_MFPL_PC4MFP_EMAC_MII_RXD0

#define SYS_GPC_MFPL_PC4MFP_EMAC_MII_RXD0

GPC_MFPL PC4 setting for EMAC_MII_RXD0

Definition at line 447 of file sys.h.

## ◆ SYS_GPC_MFPL_PC4MFP_GPIO

#define SYS_GPC_MFPL_PC4MFP_GPIO

GPC_MFPL PC4 setting for GPIO

Definition at line 442 of file sys.h.

## ◆ SYS_GPC_MFPL_PC4MFP_I2S1_DO

#define SYS_GPC_MFPL_PC4MFP_I2S1_DO

GPC_MFPL PC4 setting for I2S1_DO

Definition at line 443 of file sys.h.

## ◆ SYS_GPC_MFPL_PC4MFP_QEI0_B

#define SYS_GPC_MFPL_PC4MFP_QEI0_B

GPC_MFPL PC4 setting for QEI0_B

Definition at line 446 of file sys.h.

## ◆ SYS_GPC_MFPL_PC4MFP_SC1_RST

#define SYS_GPC_MFPL_PC4MFP_SC1_RST

GPC_MFPL PC4 setting for SC1_RST

Definition at line 444 of file sys.h.

## ◆ SYS_GPC_MFPL_PC4MFP_SPI0_MOSI1

#define SYS_GPC_MFPL_PC4MFP_SPI0_MOSI1

GPC_MFPL PC4 setting for SPI0_MOSI1

Definition at line 445 of file sys.h.

## ◆ SYS_GPC_MFPL_PC5MFP_CLK_O

#define SYS_GPC_MFPL_PC5MFP_CLK_O

GPC_MFPL PC5 setting for CLK_O

Definition at line 453 of file sys.h.

## ◆ SYS_GPC_MFPL_PC5MFP_CLKO

#define SYS_GPC_MFPL_PC5MFP_CLKO

GPC_MFPL PC5 setting for CLK_O

Definition at line 454 of file sys.h.

## ◆ SYS_GPC_MFPL_PC5MFP_EBI_MCLK

#define SYS_GPC_MFPL_PC5MFP_EBI_MCLK

GPC_MFPL PC5 setting for EBI_MCLK

Definition at line 457 of file sys.h.

## ◆ SYS_GPC_MFPL_PC5MFP_ECAP0_IC0

#define SYS_GPC_MFPL_PC5MFP_ECAP0_IC0

GPC_MFPL PC5 setting for ECAP0_IC0

Definition at line 458 of file sys.h.

## ◆ SYS_GPC_MFPL_PC5MFP_EMAC_MII_RXCLK

#define SYS_GPC_MFPL_PC5MFP_EMAC_MII_RXCLK

GPC_MFPL PC5 setting for EMAC_MII_RXCLK

Definition at line 456 of file sys.h.

## ◆ SYS_GPC_MFPL_PC5MFP_GPIO

#define SYS_GPC_MFPL_PC5MFP_GPIO

GPC_MFPL PC5 setting for GPIO

Definition at line 452 of file sys.h.

## ◆ SYS_GPC_MFPL_PC5MFP_QEI0_A

#define SYS_GPC_MFPL_PC5MFP_QEI0_A

GPC_MFPL PC5 setting for QEI0_A

Definition at line 455 of file sys.h.

## ◆ SYS_GPC_MFPL_PC6MFP_EBI_AD9

#define SYS_GPC_MFPL_PC6MFP_EBI_AD9

GPC_MFPL PC6 setting for EBI_AD9

Definition at line 466 of file sys.h.

## ◆ SYS_GPC_MFPL_PC6MFP_EMAC_MII_TXD0

#define SYS_GPC_MFPL_PC6MFP_EMAC_MII_TXD0

GPC_MFPL PC6 setting for EMAC_MII_TXD0

Definition at line 465 of file sys.h.

## ◆ SYS_GPC_MFPL_PC6MFP_GPIO

#define SYS_GPC_MFPL_PC6MFP_GPIO

GPC_MFPL PC6 setting for GPIO

Definition at line 461 of file sys.h.

## ◆ SYS_GPC_MFPL_PC6MFP_SPI0_MISO0

#define SYS_GPC_MFPL_PC6MFP_SPI0_MISO0

GPC_MFPL PC6 setting for SPI0_MISO0

Definition at line 463 of file sys.h.

## ◆ SYS_GPC_MFPL_PC6MFP_TM2_CNT_OUT

#define SYS_GPC_MFPL_PC6MFP_TM2_CNT_OUT

GPC_MFPL PC6 setting for TM2_CNT_OUT

Definition at line 464 of file sys.h.

## ◆ SYS_GPC_MFPL_PC6MFP_TM2_EXT

#define SYS_GPC_MFPL_PC6MFP_TM2_EXT

GPC_MFPL PC6 setting for TM2_EXT

Definition at line 462 of file sys.h.

## ◆ SYS_GPC_MFPL_PC7MFP_EBI_AD8

#define SYS_GPC_MFPL_PC7MFP_EBI_AD8

GPC_MFPL PC7 setting for EBI_AD8

Definition at line 473 of file sys.h.

## ◆ SYS_GPC_MFPL_PC7MFP_EMAC_MII_TXD1

#define SYS_GPC_MFPL_PC7MFP_EMAC_MII_TXD1

GPC_MFPL PC7 setting for EMAC_MII_TXD1

Definition at line 472 of file sys.h.

## ◆ SYS_GPC_MFPL_PC7MFP_GPIO

#define SYS_GPC_MFPL_PC7MFP_GPIO

GPC_MFPL PC7 setting for GPIO

Definition at line 469 of file sys.h.

## ◆ SYS_GPC_MFPL_PC7MFP_SPI0_MOSI0

#define SYS_GPC_MFPL_PC7MFP_SPI0_MOSI0

GPC_MFPL PC7 setting for SPI0_MOSI0

Definition at line 471 of file sys.h.

## ◆ SYS_GPC_MFPL_PC7MFP_TM1_EXT

#define SYS_GPC_MFPL_PC7MFP_TM1_EXT

GPC_MFPL PC7 setting for TM1_EXT

Definition at line 470 of file sys.h.

## ◆ SYS_GPD_MFPH_PD10MFP_GPIO

#define SYS_GPD_MFPH_PD10MFP_GPIO

GPD_MFPH PD10 setting for GPIO

Definition at line 626 of file sys.h.

## ◆ SYS_GPD_MFPH_PD10MFP_I2C4_SCL

#define SYS_GPD_MFPH_PD10MFP_I2C4_SCL

GPD_MFPH PD10 setting for I2C4_SCL

Definition at line 628 of file sys.h.

## ◆ SYS_GPD_MFPH_PD10MFP_SC3_DAT

#define SYS_GPD_MFPH_PD10MFP_SC3_DAT

GPD_MFPH PD10 setting for SC3_DAT

Definition at line 627 of file sys.h.

## ◆ SYS_GPD_MFPH_PD11MFP_GPIO

#define SYS_GPD_MFPH_PD11MFP_GPIO

GPD_MFPH PD11 setting for GPIO

Definition at line 631 of file sys.h.

## ◆ SYS_GPD_MFPH_PD11MFP_SC3_RST

#define SYS_GPD_MFPH_PD11MFP_SC3_RST

GPD_MFPH PD11 setting for SC3_RST

Definition at line 632 of file sys.h.

## ◆ SYS_GPD_MFPH_PD11MFP_TM3_CNT_OUT

#define SYS_GPD_MFPH_PD11MFP_TM3_CNT_OUT

GPD_MFPH PD11 setting for TM3_CNT_OUT

Definition at line 633 of file sys.h.

## ◆ SYS_GPD_MFPH_PD12MFP_GPIO

#define SYS_GPD_MFPH_PD12MFP_GPIO

GPD_MFPH PD12 setting for GPIO

Definition at line 636 of file sys.h.

## ◆ SYS_GPD_MFPH_PD12MFP_I2C4_SDA

#define SYS_GPD_MFPH_PD12MFP_I2C4_SDA

GPD_MFPH PD12 setting for I2C4_SDA

Definition at line 638 of file sys.h.

## ◆ SYS_GPD_MFPH_PD12MFP_SC3_CLK

#define SYS_GPD_MFPH_PD12MFP_SC3_CLK

GPD_MFPH PD12 setting for SC3_CLK

Definition at line 637 of file sys.h.

## ◆ SYS_GPD_MFPH_PD13MFP_ECAP0_IC2

#define SYS_GPD_MFPH_PD13MFP_ECAP0_IC2

GPD_MFPH PD13 setting for ECAP0_IC2

Definition at line 644 of file sys.h.

## ◆ SYS_GPD_MFPH_PD13MFP_GPIO

#define SYS_GPD_MFPH_PD13MFP_GPIO

GPD_MFPH PD13 setting for GPIO

Definition at line 641 of file sys.h.

## ◆ SYS_GPD_MFPH_PD13MFP_SPI1_SS0

#define SYS_GPD_MFPH_PD13MFP_SPI1_SS0

GPD_MFPH PD13 setting for SPI1_SS0

Definition at line 642 of file sys.h.

## ◆ SYS_GPD_MFPH_PD13MFP_UART5_CTS

#define SYS_GPD_MFPH_PD13MFP_UART5_CTS

GPD_MFPH PD13 setting for UART5_CTS

Definition at line 643 of file sys.h.

## ◆ SYS_GPD_MFPH_PD14MFP_ECAP0_IC1

#define SYS_GPD_MFPH_PD14MFP_ECAP0_IC1

GPD_MFPH PD14 setting for ECAP0_IC1

Definition at line 650 of file sys.h.

## ◆ SYS_GPD_MFPH_PD14MFP_GPIO

#define SYS_GPD_MFPH_PD14MFP_GPIO

GPD_MFPH PD14 setting for GPIO

Definition at line 647 of file sys.h.

## ◆ SYS_GPD_MFPH_PD14MFP_SPI1_CLK

#define SYS_GPD_MFPH_PD14MFP_SPI1_CLK

GPD_MFPH PD14 setting for SPI1_CLK

Definition at line 648 of file sys.h.

## ◆ SYS_GPD_MFPH_PD14MFP_UART5_RTS

#define SYS_GPD_MFPH_PD14MFP_UART5_RTS

GPD_MFPH PD14 setting for UART5_RTS

Definition at line 649 of file sys.h.

## ◆ SYS_GPD_MFPH_PD15MFP_ECAP0_IC0

#define SYS_GPD_MFPH_PD15MFP_ECAP0_IC0

GPD_MFPH PD15 setting for ECAP0_IC0

Definition at line 656 of file sys.h.

## ◆ SYS_GPD_MFPH_PD15MFP_GPIO

#define SYS_GPD_MFPH_PD15MFP_GPIO

GPD_MFPH PD15 setting for GPIO

Definition at line 653 of file sys.h.

## ◆ SYS_GPD_MFPH_PD15MFP_SPI1_MISO0

#define SYS_GPD_MFPH_PD15MFP_SPI1_MISO0

GPD_MFPH PD15 setting for SPI1_MISO0

Definition at line 654 of file sys.h.

## ◆ SYS_GPD_MFPH_PD15MFP_UART5_TXD

#define SYS_GPD_MFPH_PD15MFP_UART5_TXD

GPD_MFPH PD15 setting for UART5_TXD

Definition at line 655 of file sys.h.

## ◆ SYS_GPD_MFPH_PD8MFP_GPIO

#define SYS_GPD_MFPH_PD8MFP_GPIO

GPD_MFPH PD8 setting for GPIO

Definition at line 616 of file sys.h.

## ◆ SYS_GPD_MFPH_PD8MFP_I2C0_SCL

#define SYS_GPD_MFPH_PD8MFP_I2C0_SCL

GPD_MFPH PD8 setting for I2C0_SCL

Definition at line 618 of file sys.h.

## ◆ SYS_GPD_MFPH_PD8MFP_SPI3_MISO1

#define SYS_GPD_MFPH_PD8MFP_SPI3_MISO1

GPD_MFPH PD8 setting for SPI3_MISO1

Definition at line 617 of file sys.h.

## ◆ SYS_GPD_MFPH_PD9MFP_GPIO

#define SYS_GPD_MFPH_PD9MFP_GPIO

GPD_MFPH PD9 setting for GPIO

Definition at line 621 of file sys.h.

## ◆ SYS_GPD_MFPH_PD9MFP_I2C0_SDA

#define SYS_GPD_MFPH_PD9MFP_I2C0_SDA

GPD_MFPH PD9 setting for I2C0_SDA

Definition at line 623 of file sys.h.

## ◆ SYS_GPD_MFPH_PD9MFP_SPI3_MOSI1

#define SYS_GPD_MFPH_PD9MFP_SPI3_MOSI1

GPD_MFPH PD9 setting for SPI3_MOSI1

Definition at line 622 of file sys.h.

## ◆ SYS_GPD_MFPL_PD0MFP_CAP_DATA3

#define SYS_GPD_MFPL_PD0MFP_CAP_DATA3

GPD_MFPL PD0 setting for CAP_DATA3

Definition at line 551 of file sys.h.

## ◆ SYS_GPD_MFPL_PD0MFP_EBI_A4

#define SYS_GPD_MFPL_PD0MFP_EBI_A4

GPD_MFPL PD0 setting for EBI_A4

Definition at line 553 of file sys.h.

## ◆ SYS_GPD_MFPL_PD0MFP_ETM_TRACE_CLK

#define SYS_GPD_MFPL_PD0MFP_ETM_TRACE_CLK

GPD_MFPL PD0 setting for ETM_TRACE_CLK

Definition at line 552 of file sys.h.

## ◆ SYS_GPD_MFPL_PD0MFP_GPIO

#define SYS_GPD_MFPL_PD0MFP_GPIO

GPD_MFPL PD0 setting for GPIO

Definition at line 547 of file sys.h.

## ◆ SYS_GPD_MFPL_PD0MFP_INT3

#define SYS_GPD_MFPL_PD0MFP_INT3

GPD_MFPL PD0 setting for INT3

Definition at line 554 of file sys.h.

## ◆ SYS_GPD_MFPL_PD0MFP_SC4_CLK

#define SYS_GPD_MFPL_PD0MFP_SC4_CLK

GPD_MFPL PD0 setting for SC4_CLK

Definition at line 549 of file sys.h.

## ◆ SYS_GPD_MFPL_PD0MFP_SD1_DAT2

#define SYS_GPD_MFPL_PD0MFP_SD1_DAT2

GPD_MFPL PD0 setting for SD1_DAT2

Definition at line 550 of file sys.h.

## ◆ SYS_GPD_MFPL_PD0MFP_SPI1_MISO0

#define SYS_GPD_MFPL_PD0MFP_SPI1_MISO0

GPD_MFPL PD0 setting for SPI1_MISO0

Definition at line 548 of file sys.h.

## ◆ SYS_GPD_MFPL_PD1MFP_CAP_DATA2

#define SYS_GPD_MFPL_PD1MFP_CAP_DATA2

GPD_MFPL PD1 setting for CAP_DATA2

Definition at line 561 of file sys.h.

## ◆ SYS_GPD_MFPL_PD1MFP_EBI_A5

#define SYS_GPD_MFPL_PD1MFP_EBI_A5

GPD_MFPL PD1 setting for EBI_A5

Definition at line 562 of file sys.h.

## ◆ SYS_GPD_MFPL_PD1MFP_GPIO

#define SYS_GPD_MFPL_PD1MFP_GPIO

GPD_MFPL PD1 setting for GPIO

Definition at line 557 of file sys.h.

## ◆ SYS_GPD_MFPL_PD1MFP_SD1_DAT1

#define SYS_GPD_MFPL_PD1MFP_SD1_DAT1

GPD_MFPL PD1 setting for SD1_DAT1

Definition at line 560 of file sys.h.

## ◆ SYS_GPD_MFPL_PD1MFP_SPI1_CLK

#define SYS_GPD_MFPL_PD1MFP_SPI1_CLK

GPD_MFPL PD1 setting for SPI1_CLK

Definition at line 558 of file sys.h.

## ◆ SYS_GPD_MFPL_PD1MFP_TM0_CNT_OUT

#define SYS_GPD_MFPL_PD1MFP_TM0_CNT_OUT

GPD_MFPL PD1 setting for TM0_CNT_OUT

Definition at line 559 of file sys.h.

## ◆ SYS_GPD_MFPL_PD2MFP_CAP_DATA1

#define SYS_GPD_MFPL_PD2MFP_CAP_DATA1

GPD_MFPL PD2 setting for CAP_DATA1

Definition at line 569 of file sys.h.

## ◆ SYS_GPD_MFPL_PD2MFP_EBI_A6

#define SYS_GPD_MFPL_PD2MFP_EBI_A6

GPD_MFPL PD2 setting for EBI_A6

Definition at line 570 of file sys.h.

## ◆ SYS_GPD_MFPL_PD2MFP_GPIO

#define SYS_GPD_MFPL_PD2MFP_GPIO

GPD_MFPL PD2 setting for GPIO

Definition at line 565 of file sys.h.

## ◆ SYS_GPD_MFPL_PD2MFP_I2C3_SCL

#define SYS_GPD_MFPL_PD2MFP_I2C3_SCL

GPD_MFPL PD2 setting for I2C3_SCL

Definition at line 567 of file sys.h.

## ◆ SYS_GPD_MFPL_PD2MFP_SD1_DAT0

#define SYS_GPD_MFPL_PD2MFP_SD1_DAT0

GPD_MFPL PD2 setting for SD1_DAT0

Definition at line 568 of file sys.h.

## ◆ SYS_GPD_MFPL_PD2MFP_STADC

#define SYS_GPD_MFPL_PD2MFP_STADC

GPD_MFPL PD2 setting for STADC

Definition at line 566 of file sys.h.

## ◆ SYS_GPD_MFPL_PD3MFP_ACMP2_O

#define SYS_GPD_MFPL_PD3MFP_ACMP2_O

GPD_MFPL PD3 setting for ACMP2_O

Definition at line 576 of file sys.h.

## ◆ SYS_GPD_MFPL_PD3MFP_CAP_DATA0

#define SYS_GPD_MFPL_PD3MFP_CAP_DATA0

GPD_MFPL PD3 setting for CAP_DATA0

Definition at line 578 of file sys.h.

## ◆ SYS_GPD_MFPL_PD3MFP_EBI_A7

#define SYS_GPD_MFPL_PD3MFP_EBI_A7

GPD_MFPL PD3 setting for EBI_A7

Definition at line 580 of file sys.h.

## ◆ SYS_GPD_MFPL_PD3MFP_GPIO

#define SYS_GPD_MFPL_PD3MFP_GPIO

GPD_MFPL PD3 setting for GPIO

Definition at line 573 of file sys.h.

## ◆ SYS_GPD_MFPL_PD3MFP_I2C3_SDA

#define SYS_GPD_MFPL_PD3MFP_I2C3_SDA

GPD_MFPL PD3 setting for I2C3_SDA

Definition at line 575 of file sys.h.

## ◆ SYS_GPD_MFPL_PD3MFP_JTAG_TDO

#define SYS_GPD_MFPL_PD3MFP_JTAG_TDO

GPD_MFPL PD3 setting for JTAG_TDO

Definition at line 579 of file sys.h.

## ◆ SYS_GPD_MFPL_PD3MFP_SC5_CLK

#define SYS_GPD_MFPL_PD3MFP_SC5_CLK

GPD_MFPL PD3 setting for SC5_CLK

Definition at line 574 of file sys.h.

## ◆ SYS_GPD_MFPL_PD3MFP_SD0_CDn

#define SYS_GPD_MFPL_PD3MFP_SD0_CDn

GPD_MFPL PD3 setting for SD0_CDn

Definition at line 577 of file sys.h.

## ◆ SYS_GPD_MFPL_PD4MFP_ACMP1_O

#define SYS_GPD_MFPL_PD4MFP_ACMP1_O

GPD_MFPL PD4 setting for ACMP1_O

Definition at line 586 of file sys.h.

## ◆ SYS_GPD_MFPL_PD4MFP_CAP_SCLK

#define SYS_GPD_MFPL_PD4MFP_CAP_SCLK

GPD_MFPL PD4 setting for CAP_SCLK

Definition at line 587 of file sys.h.

## ◆ SYS_GPD_MFPL_PD4MFP_EBI_A8

#define SYS_GPD_MFPL_PD4MFP_EBI_A8

GPD_MFPL PD4 setting for EBI_A8

Definition at line 589 of file sys.h.

## ◆ SYS_GPD_MFPL_PD4MFP_GPIO

#define SYS_GPD_MFPL_PD4MFP_GPIO

GPD_MFPL PD4 setting for GPIO

Definition at line 583 of file sys.h.

## ◆ SYS_GPD_MFPL_PD4MFP_JTAG_TDI

#define SYS_GPD_MFPL_PD4MFP_JTAG_TDI

GPD_MFPL PD4 setting for JTAG_TDI

Definition at line 588 of file sys.h.

## ◆ SYS_GPD_MFPL_PD4MFP_SC5_CD

#define SYS_GPD_MFPL_PD4MFP_SC5_CD

GPD_MFPL PD4 setting for SC5_CD

Definition at line 584 of file sys.h.

## ◆ SYS_GPD_MFPL_PD4MFP_UART3_RXD

#define SYS_GPD_MFPL_PD4MFP_UART3_RXD

GPD_MFPL PD4 setting for UART3_RXD

Definition at line 585 of file sys.h.

## ◆ SYS_GPD_MFPL_PD5MFP_CAP_VSYNC

#define SYS_GPD_MFPL_PD5MFP_CAP_VSYNC

GPD_MFPL PD5 setting for CAP_VSYNC

Definition at line 595 of file sys.h.

## ◆ SYS_GPD_MFPL_PD5MFP_EBI_A9

#define SYS_GPD_MFPL_PD5MFP_EBI_A9

GPD_MFPL PD5 setting for EBI_A9

Definition at line 597 of file sys.h.

## ◆ SYS_GPD_MFPL_PD5MFP_GPIO

#define SYS_GPD_MFPL_PD5MFP_GPIO

GPD_MFPL PD5 setting for GPIO

Definition at line 592 of file sys.h.

## ◆ SYS_GPD_MFPL_PD5MFP_JTAG_nTRST

#define SYS_GPD_MFPL_PD5MFP_JTAG_nTRST

GPD_MFPL PD5 setting for JTAG_nTRST

Definition at line 596 of file sys.h.

## ◆ SYS_GPD_MFPL_PD5MFP_SC5_RST

#define SYS_GPD_MFPL_PD5MFP_SC5_RST

GPD_MFPL PD5 setting for SC5_RST

Definition at line 593 of file sys.h.

## ◆ SYS_GPD_MFPL_PD5MFP_UART3_TXD

#define SYS_GPD_MFPL_PD5MFP_UART3_TXD

GPD_MFPL PD5 setting for UART3_TXD

Definition at line 594 of file sys.h.

## ◆ SYS_GPD_MFPL_PD6MFP_CAP_HSYNC

#define SYS_GPD_MFPL_PD6MFP_CAP_HSYNC

GPD_MFPL PD6 setting for CAP_HSYNC

Definition at line 604 of file sys.h.

## ◆ SYS_GPD_MFPL_PD6MFP_EBI_A10

#define SYS_GPD_MFPL_PD6MFP_EBI_A10

GPD_MFPL PD6 setting for EBI_A10

Definition at line 605 of file sys.h.

## ◆ SYS_GPD_MFPL_PD6MFP_GPIO

#define SYS_GPD_MFPL_PD6MFP_GPIO

GPD_MFPL PD6 setting for GPIO

Definition at line 600 of file sys.h.

## ◆ SYS_GPD_MFPL_PD6MFP_SC5_PWR

#define SYS_GPD_MFPL_PD6MFP_SC5_PWR

GPD_MFPL PD6 setting for SC5_PWR

Definition at line 601 of file sys.h.

## ◆ SYS_GPD_MFPL_PD6MFP_SD0_CMD

#define SYS_GPD_MFPL_PD6MFP_SD0_CMD

GPD_MFPL PD6 setting for SD0_CMD

Definition at line 603 of file sys.h.

## ◆ SYS_GPD_MFPL_PD6MFP_UART3_RTS

#define SYS_GPD_MFPL_PD6MFP_UART3_RTS

GPD_MFPL PD6 setting for UART3_RTS

Definition at line 602 of file sys.h.

## ◆ SYS_GPD_MFPL_PD7MFP_CAP_PIXCLK

#define SYS_GPD_MFPL_PD7MFP_CAP_PIXCLK

GPD_MFPL PD7 setting for CAP_PIXCLK

Definition at line 612 of file sys.h.

## ◆ SYS_GPD_MFPL_PD7MFP_EBI_A11

#define SYS_GPD_MFPL_PD7MFP_EBI_A11

GPD_MFPL PD7 setting for EBI_A11

Definition at line 613 of file sys.h.

## ◆ SYS_GPD_MFPL_PD7MFP_GPIO

#define SYS_GPD_MFPL_PD7MFP_GPIO

GPD_MFPL PD7 setting for GPIO

Definition at line 608 of file sys.h.

## ◆ SYS_GPD_MFPL_PD7MFP_SC5_DAT

#define SYS_GPD_MFPL_PD7MFP_SC5_DAT

GPD_MFPL PD7 setting for SC5_DAT

Definition at line 609 of file sys.h.

## ◆ SYS_GPD_MFPL_PD7MFP_SD0_CLK

#define SYS_GPD_MFPL_PD7MFP_SD0_CLK

GPD_MFPL PD7 setting for SD0_CLK

Definition at line 611 of file sys.h.

## ◆ SYS_GPD_MFPL_PD7MFP_UART3_CTS

#define SYS_GPD_MFPL_PD7MFP_UART3_CTS

GPD_MFPL PD7 setting for UART3_CTS

Definition at line 610 of file sys.h.

## ◆ SYS_GPE_MFPH_PE10MFP_ACMP1_P1

#define SYS_GPE_MFPH_PE10MFP_ACMP1_P1

GPE_MFPH PE10 setting for ACMP1_P1

Definition at line 730 of file sys.h.

## ◆ SYS_GPE_MFPH_PE10MFP_ADC0_10

#define SYS_GPE_MFPH_PE10MFP_ADC0_10

GPE_MFPH PE10 setting for ADC0_10

Definition at line 728 of file sys.h.

## ◆ SYS_GPE_MFPH_PE10MFP_ADC1_2

#define SYS_GPE_MFPH_PE10MFP_ADC1_2

GPE_MFPH PE10 setting for ADC1_2

Definition at line 729 of file sys.h.

## ◆ SYS_GPE_MFPH_PE10MFP_EBI_nWRL

#define SYS_GPE_MFPH_PE10MFP_EBI_nWRL

GPE_MFPH PE10 setting for EBI_nWRL

Definition at line 733 of file sys.h.

## ◆ SYS_GPE_MFPH_PE10MFP_GPIO

#define SYS_GPE_MFPH_PE10MFP_GPIO

GPE_MFPH PE10 setting for GPIO

Definition at line 727 of file sys.h.

## ◆ SYS_GPE_MFPH_PE10MFP_SD0_DAT1

#define SYS_GPE_MFPH_PE10MFP_SD0_DAT1

GPE_MFPH PE10 setting for SD0_DAT1

Definition at line 732 of file sys.h.

## ◆ SYS_GPE_MFPH_PE10MFP_SPI0_MISO1

#define SYS_GPE_MFPH_PE10MFP_SPI0_MISO1

GPE_MFPH PE10 setting for SPI0_MISO1

Definition at line 731 of file sys.h.

## ◆ SYS_GPE_MFPH_PE11MFP_ACMP1_P2

#define SYS_GPE_MFPH_PE11MFP_ACMP1_P2

GPE_MFPH PE11 setting for ACMP1_P2

Definition at line 739 of file sys.h.

## ◆ SYS_GPE_MFPH_PE11MFP_ACMP2_P3

#define SYS_GPE_MFPH_PE11MFP_ACMP2_P3

GPE_MFPH PE11 setting for ACMP2_P3

Definition at line 742 of file sys.h.

## ◆ SYS_GPE_MFPH_PE11MFP_ADC0_11

#define SYS_GPE_MFPH_PE11MFP_ADC0_11

GPE_MFPH PE11 setting for ADC0_11

Definition at line 737 of file sys.h.

## ◆ SYS_GPE_MFPH_PE11MFP_ADC1_3

#define SYS_GPE_MFPH_PE11MFP_ADC1_3

GPE_MFPH PE11 setting for ADC1_3

Definition at line 738 of file sys.h.

## ◆ SYS_GPE_MFPH_PE11MFP_EBI_nCS0

#define SYS_GPE_MFPH_PE11MFP_EBI_nCS0

GPE_MFPH PE11 setting for EBI_nCS0

Definition at line 743 of file sys.h.

## ◆ SYS_GPE_MFPH_PE11MFP_GPIO

#define SYS_GPE_MFPH_PE11MFP_GPIO

GPE_MFPH PE11 setting for GPIO

Definition at line 736 of file sys.h.

## ◆ SYS_GPE_MFPH_PE11MFP_SD0_DAT0

#define SYS_GPE_MFPH_PE11MFP_SD0_DAT0

GPE_MFPH PE11 setting for SD0_DAT0

Definition at line 741 of file sys.h.

## ◆ SYS_GPE_MFPH_PE11MFP_SPI0_MOSI1

#define SYS_GPE_MFPH_PE11MFP_SPI0_MOSI1

GPE_MFPH PE11 setting for SPI0_MOSI1

Definition at line 740 of file sys.h.

## ◆ SYS_GPE_MFPH_PE12MFP_ACMP1_P3

#define SYS_GPE_MFPH_PE12MFP_ACMP1_P3

GPE_MFPH PE12 setting for ACMP1_P3

Definition at line 748 of file sys.h.

## ◆ SYS_GPE_MFPH_PE12MFP_ACMP2_P2

#define SYS_GPE_MFPH_PE12MFP_ACMP2_P2

GPE_MFPH PE12 setting for ACMP2_P2

Definition at line 749 of file sys.h.

## ◆ SYS_GPE_MFPH_PE12MFP_ADC1_4

#define SYS_GPE_MFPH_PE12MFP_ADC1_4

GPE_MFPH PE12 setting for ADC1_4

Definition at line 747 of file sys.h.

## ◆ SYS_GPE_MFPH_PE12MFP_EBI_nCS1

#define SYS_GPE_MFPH_PE12MFP_EBI_nCS1

GPE_MFPH PE12 setting for EBI_nCS1

Definition at line 750 of file sys.h.

## ◆ SYS_GPE_MFPH_PE12MFP_GPIO

#define SYS_GPE_MFPH_PE12MFP_GPIO

GPE_MFPH PE12 setting for GPIO

Definition at line 746 of file sys.h.

## ◆ SYS_GPE_MFPH_PE13MFP_ACMP2_P1

#define SYS_GPE_MFPH_PE13MFP_ACMP2_P1

GPE_MFPH PE13 setting for ACMP2_P1

Definition at line 754 of file sys.h.

## ◆ SYS_GPE_MFPH_PE13MFP_ADC1_5

#define SYS_GPE_MFPH_PE13MFP_ADC1_5

GPE_MFPH PE13 setting for ADC1_5

Definition at line 753 of file sys.h.

## ◆ SYS_GPE_MFPH_PE13MFP_EBI_nCS2

#define SYS_GPE_MFPH_PE13MFP_EBI_nCS2

GPE_MFPH PE13 setting for EBI_nCS2

Definition at line 755 of file sys.h.

## ◆ SYS_GPE_MFPH_PE13MFP_GPIO

#define SYS_GPE_MFPH_PE13MFP_GPIO

GPE_MFPH PE13 setting for GPIO

Definition at line 752 of file sys.h.

## ◆ SYS_GPE_MFPH_PE14MFP_ACMP2_P0

#define SYS_GPE_MFPH_PE14MFP_ACMP2_P0

GPE_MFPH PE14 setting for ACMP2_P0

Definition at line 760 of file sys.h.

## ◆ SYS_GPE_MFPH_PE14MFP_ADC1_6

#define SYS_GPE_MFPH_PE14MFP_ADC1_6

GPE_MFPH PE14 setting for ADC1_6

Definition at line 759 of file sys.h.

## ◆ SYS_GPE_MFPH_PE14MFP_EBI_nCS3

#define SYS_GPE_MFPH_PE14MFP_EBI_nCS3

GPE_MFPH PE14 setting for EBI_nCS3

Definition at line 761 of file sys.h.

## ◆ SYS_GPE_MFPH_PE14MFP_GPIO

#define SYS_GPE_MFPH_PE14MFP_GPIO

GPE_MFPH PE14 setting for GPIO

Definition at line 758 of file sys.h.

## ◆ SYS_GPE_MFPH_PE15MFP_ACMP2_N

#define SYS_GPE_MFPH_PE15MFP_ACMP2_N

GPE_MFPH PE15 setting for ACMP2_N

Definition at line 766 of file sys.h.

## ◆ SYS_GPE_MFPH_PE15MFP_ADC1_7

#define SYS_GPE_MFPH_PE15MFP_ADC1_7

GPE_MFPH PE15 setting for ADC1_7

Definition at line 765 of file sys.h.

## ◆ SYS_GPE_MFPH_PE15MFP_GPIO

#define SYS_GPE_MFPH_PE15MFP_GPIO

GPE_MFPH PE15 setting for GPIO

Definition at line 764 of file sys.h.

## ◆ SYS_GPE_MFPH_PE8MFP_ACMP1_N

#define SYS_GPE_MFPH_PE8MFP_ACMP1_N

GPE_MFPH PE8 setting for ACMP1_N

Definition at line 713 of file sys.h.

## ◆ SYS_GPE_MFPH_PE8MFP_ADC0_8

#define SYS_GPE_MFPH_PE8MFP_ADC0_8

GPE_MFPH PE8 setting for ADC0_8

Definition at line 711 of file sys.h.

## ◆ SYS_GPE_MFPH_PE8MFP_ADC1_0

#define SYS_GPE_MFPH_PE8MFP_ADC1_0

GPE_MFPH PE8 setting for ADC1_0

Definition at line 712 of file sys.h.

## ◆ SYS_GPE_MFPH_PE8MFP_EBI_ALE

#define SYS_GPE_MFPH_PE8MFP_EBI_ALE

GPE_MFPH PE8 setting for EBI_ALE

Definition at line 716 of file sys.h.

## ◆ SYS_GPE_MFPH_PE8MFP_GPIO

#define SYS_GPE_MFPH_PE8MFP_GPIO

GPE_MFPH PE8 setting for GPIO

Definition at line 710 of file sys.h.

## ◆ SYS_GPE_MFPH_PE8MFP_SD0_DAT3

#define SYS_GPE_MFPH_PE8MFP_SD0_DAT3

GPE_MFPH PE8 setting for SD0_DAT3

Definition at line 715 of file sys.h.

## ◆ SYS_GPE_MFPH_PE8MFP_TM1_CNT_OUT

#define SYS_GPE_MFPH_PE8MFP_TM1_CNT_OUT

GPE_MFPH PE8 setting for TM1_CNT_OUT

Definition at line 714 of file sys.h.

## ◆ SYS_GPE_MFPH_PE9MFP_ACMP1_P0

#define SYS_GPE_MFPH_PE9MFP_ACMP1_P0

GPE_MFPH PE9 setting for ACMP1_P0

Definition at line 722 of file sys.h.

## ◆ SYS_GPE_MFPH_PE9MFP_ADC0_9

#define SYS_GPE_MFPH_PE9MFP_ADC0_9

GPE_MFPH PE9 setting for ADC0_9

Definition at line 720 of file sys.h.

## ◆ SYS_GPE_MFPH_PE9MFP_ADC1_1

#define SYS_GPE_MFPH_PE9MFP_ADC1_1

GPE_MFPH PE9 setting for ADC1_1

Definition at line 721 of file sys.h.

## ◆ SYS_GPE_MFPH_PE9MFP_EBI_nWRH

#define SYS_GPE_MFPH_PE9MFP_EBI_nWRH

GPE_MFPH PE9 setting for EBI_nWRH

Definition at line 724 of file sys.h.

## ◆ SYS_GPE_MFPH_PE9MFP_GPIO

#define SYS_GPE_MFPH_PE9MFP_GPIO

GPE_MFPH PE9 setting for GPIO

Definition at line 719 of file sys.h.

## ◆ SYS_GPE_MFPH_PE9MFP_SD0_DAT2

#define SYS_GPE_MFPH_PE9MFP_SD0_DAT2

GPE_MFPH PE9 setting for SD0_DAT2

Definition at line 723 of file sys.h.

## ◆ SYS_GPE_MFPL_PE0MFP_ADC0_0

#define SYS_GPE_MFPL_PE0MFP_ADC0_0

GPE_MFPL PE0 setting for ADC0_0

Definition at line 660 of file sys.h.

## ◆ SYS_GPE_MFPL_PE0MFP_GPIO

#define SYS_GPE_MFPL_PE0MFP_GPIO

GPE_MFPL PE0 setting for GPIO

Definition at line 659 of file sys.h.

## ◆ SYS_GPE_MFPL_PE0MFP_INT4

#define SYS_GPE_MFPL_PE0MFP_INT4

GPE_MFPL PE0 setting for INT4

Definition at line 661 of file sys.h.

## ◆ SYS_GPE_MFPL_PE1MFP_ADC0_1

#define SYS_GPE_MFPL_PE1MFP_ADC0_1

GPE_MFPL PE1 setting for ADC0_1

Definition at line 665 of file sys.h.

## ◆ SYS_GPE_MFPL_PE1MFP_GPIO

#define SYS_GPE_MFPL_PE1MFP_GPIO

GPE_MFPL PE1 setting for GPIO

Definition at line 664 of file sys.h.

## ◆ SYS_GPE_MFPL_PE1MFP_TM2_CNT_OUT

#define SYS_GPE_MFPL_PE1MFP_TM2_CNT_OUT

GPE_MFPL PE1 setting for TM2_CNT_OUT

Definition at line 666 of file sys.h.

## ◆ SYS_GPE_MFPL_PE2MFP_ACMP0_O

#define SYS_GPE_MFPL_PE2MFP_ACMP0_O

GPE_MFPL PE2 setting for ACMP0_O

Definition at line 671 of file sys.h.

## ◆ SYS_GPE_MFPL_PE2MFP_ADC0_2

#define SYS_GPE_MFPL_PE2MFP_ADC0_2

GPE_MFPL PE2 setting for ADC0_2

Definition at line 670 of file sys.h.

## ◆ SYS_GPE_MFPL_PE2MFP_GPIO

#define SYS_GPE_MFPL_PE2MFP_GPIO

GPE_MFPL PE2 setting for GPIO

Definition at line 669 of file sys.h.

## ◆ SYS_GPE_MFPL_PE2MFP_SPI0_MISO0

#define SYS_GPE_MFPL_PE2MFP_SPI0_MISO0

GPE_MFPL PE2 setting for SPI0_MISO0

Definition at line 672 of file sys.h.

## ◆ SYS_GPE_MFPL_PE3MFP_ACMP0_P3

#define SYS_GPE_MFPL_PE3MFP_ACMP0_P3

GPE_MFPL PE3 setting for ACMP0_P3

Definition at line 677 of file sys.h.

## ◆ SYS_GPE_MFPL_PE3MFP_ADC0_3

#define SYS_GPE_MFPL_PE3MFP_ADC0_3

GPE_MFPL PE3 setting for ADC0_3

Definition at line 676 of file sys.h.

## ◆ SYS_GPE_MFPL_PE3MFP_GPIO

#define SYS_GPE_MFPL_PE3MFP_GPIO

GPE_MFPL PE3 setting for GPIO

Definition at line 675 of file sys.h.

## ◆ SYS_GPE_MFPL_PE3MFP_SPI0_MOSI0

#define SYS_GPE_MFPL_PE3MFP_SPI0_MOSI0

GPE_MFPL PE3 setting for SPI0_MOSI0

Definition at line 678 of file sys.h.

## ◆ SYS_GPE_MFPL_PE4MFP_ACMP0_P2

#define SYS_GPE_MFPL_PE4MFP_ACMP0_P2

GPE_MFPL PE4 setting for ACMP0_P2

Definition at line 683 of file sys.h.

## ◆ SYS_GPE_MFPL_PE4MFP_ADC0_4

#define SYS_GPE_MFPL_PE4MFP_ADC0_4

GPE_MFPL PE4 setting for ADC0_4

Definition at line 682 of file sys.h.

## ◆ SYS_GPE_MFPL_PE4MFP_GPIO

#define SYS_GPE_MFPL_PE4MFP_GPIO

GPE_MFPL PE4 setting for GPIO

Definition at line 681 of file sys.h.

## ◆ SYS_GPE_MFPL_PE4MFP_SPI0_SS0

#define SYS_GPE_MFPL_PE4MFP_SPI0_SS0

GPE_MFPL PE4 setting for SPI0_SS0

Definition at line 684 of file sys.h.

## ◆ SYS_GPE_MFPL_PE5MFP_ACMP0_P1

#define SYS_GPE_MFPL_PE5MFP_ACMP0_P1

GPE_MFPL PE5 setting for ACMP0_P1

Definition at line 689 of file sys.h.

## ◆ SYS_GPE_MFPL_PE5MFP_ADC0_5

#define SYS_GPE_MFPL_PE5MFP_ADC0_5

GPE_MFPL PE5 setting for ADC0_5

Definition at line 688 of file sys.h.

## ◆ SYS_GPE_MFPL_PE5MFP_GPIO

#define SYS_GPE_MFPL_PE5MFP_GPIO

GPE_MFPL PE5 setting for GPIO

Definition at line 687 of file sys.h.

## ◆ SYS_GPE_MFPL_PE5MFP_SD0_CDn

#define SYS_GPE_MFPL_PE5MFP_SD0_CDn

GPE_MFPL PE5 setting for SD0_CDn

Definition at line 691 of file sys.h.

## ◆ SYS_GPE_MFPL_PE5MFP_SPI0_CLK

#define SYS_GPE_MFPL_PE5MFP_SPI0_CLK

GPE_MFPL PE5 setting for SPI0_CLK

Definition at line 690 of file sys.h.

## ◆ SYS_GPE_MFPL_PE6MFP_ACMP0_P0

#define SYS_GPE_MFPL_PE6MFP_ACMP0_P0

GPE_MFPL PE6 setting for ACMP0_P0

Definition at line 696 of file sys.h.

## ◆ SYS_GPE_MFPL_PE6MFP_ADC0_6

#define SYS_GPE_MFPL_PE6MFP_ADC0_6

GPE_MFPL PE6 setting for ADC0_6

Definition at line 695 of file sys.h.

## ◆ SYS_GPE_MFPL_PE6MFP_EBI_nWR

#define SYS_GPE_MFPL_PE6MFP_EBI_nWR

GPE_MFPL PE6 setting for EBI_nWR

Definition at line 699 of file sys.h.

## ◆ SYS_GPE_MFPL_PE6MFP_GPIO

#define SYS_GPE_MFPL_PE6MFP_GPIO

GPE_MFPL PE6 setting for GPIO

Definition at line 694 of file sys.h.

## ◆ SYS_GPE_MFPL_PE6MFP_SD0_CMD

#define SYS_GPE_MFPL_PE6MFP_SD0_CMD

GPE_MFPL PE6 setting for SD0_CMD

Definition at line 698 of file sys.h.

## ◆ SYS_GPE_MFPL_PE6MFP_SPI0_MISO0

#define SYS_GPE_MFPL_PE6MFP_SPI0_MISO0

GPE_MFPL PE6 setting for SPI0_MISO0

Definition at line 697 of file sys.h.

## ◆ SYS_GPE_MFPL_PE7MFP_ACMP0_N

#define SYS_GPE_MFPL_PE7MFP_ACMP0_N

GPE_MFPL PE7 setting for ACMP0_N

Definition at line 704 of file sys.h.

## ◆ SYS_GPE_MFPL_PE7MFP_ADC0_7

#define SYS_GPE_MFPL_PE7MFP_ADC0_7

GPE_MFPL PE7 setting for ADC0_7

Definition at line 703 of file sys.h.

## ◆ SYS_GPE_MFPL_PE7MFP_EBI_nRD

#define SYS_GPE_MFPL_PE7MFP_EBI_nRD

GPE_MFPL PE7 setting for _EBI_nRD

Definition at line 707 of file sys.h.

## ◆ SYS_GPE_MFPL_PE7MFP_GPIO

#define SYS_GPE_MFPL_PE7MFP_GPIO

GPE_MFPL PE7 setting for GPIO

Definition at line 702 of file sys.h.

## ◆ SYS_GPE_MFPL_PE7MFP_SD0_CLK

#define SYS_GPE_MFPL_PE7MFP_SD0_CLK

GPE_MFPL PE7 setting for SD0_CLK

Definition at line 706 of file sys.h.

## ◆ SYS_GPE_MFPL_PE7MFP_SPI0_MOSI0

#define SYS_GPE_MFPL_PE7MFP_SPI0_MOSI0

GPE_MFPL PE7 setting for SPI0_MOSI0

Definition at line 705 of file sys.h.

## ◆ SYS_GPF_MFPH_PF10MFP_GPIO

#define SYS_GPF_MFPH_PF10MFP_GPIO

GPF_MFPH PF10 setting for GPIO

Definition at line 828 of file sys.h.

## ◆ SYS_GPF_MFPH_PF10MFP_OPA0_IN_N

#define SYS_GPF_MFPH_PF10MFP_OPA0_IN_N

GPF_MFPH PF10 setting for OPA0_IN_N

Definition at line 829 of file sys.h.

## ◆ SYS_GPF_MFPH_PF10MFP_OPA0_N

#define SYS_GPF_MFPH_PF10MFP_OPA0_N

GPF_MFPH PF10 setting for OPA0_IN_N

Definition at line 830 of file sys.h.

## ◆ SYS_GPF_MFPH_PF10MFP_PWM0_1

#define SYS_GPF_MFPH_PF10MFP_PWM0_1

GPF_MFPH PF10 setting for PWM0_CH1

Definition at line 832 of file sys.h.

## ◆ SYS_GPF_MFPH_PF10MFP_PWM0_CH1

#define SYS_GPF_MFPH_PF10MFP_PWM0_CH1

GPF_MFPH PF10 setting for PWM0_CH1

Definition at line 831 of file sys.h.

## ◆ SYS_GPF_MFPH_PF11MFP_GPIO

#define SYS_GPF_MFPH_PF11MFP_GPIO

GPF_MFPH PF11 setting for GPIO

Definition at line 835 of file sys.h.

## ◆ SYS_GPF_MFPH_PF11MFP_OPA0_O

#define SYS_GPF_MFPH_PF11MFP_OPA0_O

GPF_MFPH PF11 setting for OPA0_O

Definition at line 836 of file sys.h.

## ◆ SYS_GPF_MFPH_PF11MFP_UART1_RTS

#define SYS_GPF_MFPH_PF11MFP_UART1_RTS

GPF_MFPH PF11 setting for UART1_RTS

Definition at line 837 of file sys.h.

## ◆ SYS_GPF_MFPH_PF12MFP_GPIO

#define SYS_GPF_MFPH_PF12MFP_GPIO

GPF_MFPH PF12 setting for GPIO

Definition at line 840 of file sys.h.

## ◆ SYS_GPF_MFPH_PF12MFP_OPA1_IN_P

#define SYS_GPF_MFPH_PF12MFP_OPA1_IN_P

GPF_MFPH PF12 setting for OPA1_IN_P

Definition at line 841 of file sys.h.

## ◆ SYS_GPF_MFPH_PF12MFP_OPA1_P

#define SYS_GPF_MFPH_PF12MFP_OPA1_P

GPF_MFPH PF12 setting for OPA1_IN_P

Definition at line 842 of file sys.h.

## ◆ SYS_GPF_MFPH_PF12MFP_UART1_CTS

#define SYS_GPF_MFPH_PF12MFP_UART1_CTS

GPF_MFPH PF12 setting for UART1_CTS

Definition at line 843 of file sys.h.

## ◆ SYS_GPF_MFPH_PF13MFP_GPIO

#define SYS_GPF_MFPH_PF13MFP_GPIO

GPF_MFPH PF13 setting for GPIO

Definition at line 845 of file sys.h.

## ◆ SYS_GPF_MFPH_PF13MFP_OPA1_IN_N

#define SYS_GPF_MFPH_PF13MFP_OPA1_IN_N

GPF_MFPH PF13 setting for OPA1_IN_N

Definition at line 846 of file sys.h.

## ◆ SYS_GPF_MFPH_PF13MFP_OPA1_N

#define SYS_GPF_MFPH_PF13MFP_OPA1_N

GPF_MFPH PF13 setting for OPA1_IN_N

Definition at line 847 of file sys.h.

## ◆ SYS_GPF_MFPH_PF13MFP_UART1_TXD

#define SYS_GPF_MFPH_PF13MFP_UART1_TXD

GPF_MFPH PF13 setting for UART1_TXD

Definition at line 848 of file sys.h.

## ◆ SYS_GPF_MFPH_PF14MFP_GPIO

#define SYS_GPF_MFPH_PF14MFP_GPIO

GPF_MFPH PF14 setting for GPIO

Definition at line 851 of file sys.h.

## ◆ SYS_GPF_MFPH_PF14MFP_OPA1_O

#define SYS_GPF_MFPH_PF14MFP_OPA1_O

GPF_MFPH PF14 setting for OPA1_O

Definition at line 852 of file sys.h.

## ◆ SYS_GPF_MFPH_PF14MFP_UART1_RXD

#define SYS_GPF_MFPH_PF14MFP_UART1_RXD

GPF_MFPH PF14 setting for UART1_RXD

Definition at line 853 of file sys.h.

## ◆ SYS_GPF_MFPH_PF15MFP_GPIO

#define SYS_GPF_MFPH_PF15MFP_GPIO

GPF_MFPH PF15 setting for GPIO

Definition at line 856 of file sys.h.

## ◆ SYS_GPF_MFPH_PF15MFP_UART0_RTS

#define SYS_GPF_MFPH_PF15MFP_UART0_RTS

GPF_MFPH PF15 setting for UART0_RTS

Definition at line 857 of file sys.h.

## ◆ SYS_GPF_MFPH_PF8MFP_EMAC_MII_TXD2

#define SYS_GPF_MFPH_PF8MFP_EMAC_MII_TXD2

GPF_MFPH PF8 setting for EMAC_MII_TXD2

Definition at line 818 of file sys.h.

## ◆ SYS_GPF_MFPH_PF8MFP_GPIO

#define SYS_GPF_MFPH_PF8MFP_GPIO

GPF_MFPH PF8 setting for GPIO

Definition at line 815 of file sys.h.

## ◆ SYS_GPF_MFPH_PF8MFP_SD0_CLK

#define SYS_GPF_MFPH_PF8MFP_SD0_CLK

GPF_MFPH PF8 setting for SD0_CLK

Definition at line 817 of file sys.h.

## ◆ SYS_GPF_MFPH_PF8MFP_UART2_RTS

#define SYS_GPF_MFPH_PF8MFP_UART2_RTS

GPF_MFPH PF8 setting for UART2_RTS

Definition at line 816 of file sys.h.

## ◆ SYS_GPF_MFPH_PF9MFP_GPIO

#define SYS_GPF_MFPH_PF9MFP_GPIO

GPF_MFPH PF9 setting for GPIO

Definition at line 821 of file sys.h.

## ◆ SYS_GPF_MFPH_PF9MFP_OPA0_IN_P

#define SYS_GPF_MFPH_PF9MFP_OPA0_IN_P

GPF_MFPH PF9 setting for OPA0_IN_P

Definition at line 822 of file sys.h.

## ◆ SYS_GPF_MFPH_PF9MFP_OPA0_P

#define SYS_GPF_MFPH_PF9MFP_OPA0_P

GPF_MFPH PF9 setting for OPA0_IN_P

Definition at line 823 of file sys.h.

## ◆ SYS_GPF_MFPH_PF9MFP_PWM0_0

#define SYS_GPF_MFPH_PF9MFP_PWM0_0

GPF_MFPH PF9 setting for PWM0_CH0

Definition at line 825 of file sys.h.

## ◆ SYS_GPF_MFPH_PF9MFP_PWM0_CH0

#define SYS_GPF_MFPH_PF9MFP_PWM0_CH0

GPF_MFPH PF9 setting for PWM0_CH0

Definition at line 824 of file sys.h.

## ◆ SYS_GPF_MFPL_PF0MFP_GPIO

#define SYS_GPF_MFPL_PF0MFP_GPIO

GPF_MFPL PF0 setting for GPIO

Definition at line 769 of file sys.h.

## ◆ SYS_GPF_MFPL_PF0MFP_INT5

#define SYS_GPF_MFPL_PF0MFP_INT5

GPF_MFPL PF0 setting for INT5

Definition at line 772 of file sys.h.

## ◆ SYS_GPF_MFPL_PF0MFP_SPI1_MOSI0

#define SYS_GPF_MFPL_PF0MFP_SPI1_MOSI0

GPF_MFPL PF0 setting for SPI1_MOSI0

Definition at line 770 of file sys.h.

## ◆ SYS_GPF_MFPL_PF0MFP_UART5_RXD

#define SYS_GPF_MFPL_PF0MFP_UART5_RXD

GPF_MFPL PF0 setting for UART5_RXD

Definition at line 771 of file sys.h.

## ◆ SYS_GPF_MFPL_PF1MFP_GPIO

#define SYS_GPF_MFPL_PF1MFP_GPIO

GPF_MFPL PF1 setting for GPIO

Definition at line 775 of file sys.h.

## ◆ SYS_GPF_MFPL_PF1MFP_SPI2_MOSI1

#define SYS_GPF_MFPL_PF1MFP_SPI2_MOSI1

GPF_MFPL PF1 setting for SPI2_MOSI1

Definition at line 776 of file sys.h.

## ◆ SYS_GPF_MFPL_PF2MFP_EMAC_MII_RXD3

#define SYS_GPF_MFPL_PF2MFP_EMAC_MII_RXD3

GPF_MFPL PF2 setting for EMAC_MII_RXD3

Definition at line 782 of file sys.h.

## ◆ SYS_GPF_MFPL_PF2MFP_GPIO

#define SYS_GPF_MFPL_PF2MFP_GPIO

GPF_MFPL PF2 setting for GPIO

Definition at line 779 of file sys.h.

## ◆ SYS_GPF_MFPL_PF2MFP_SD0_DAT3

#define SYS_GPF_MFPL_PF2MFP_SD0_DAT3

GPF_MFPL PF2 setting for SD0_DAT3

Definition at line 781 of file sys.h.

## ◆ SYS_GPF_MFPL_PF2MFP_SPI3_SS0

#define SYS_GPF_MFPL_PF2MFP_SPI3_SS0

GPF_MFPL PF2 setting for SPI3_SS0

Definition at line 780 of file sys.h.

## ◆ SYS_GPF_MFPL_PF3MFP_EMAC_MII_RXD2

#define SYS_GPF_MFPL_PF3MFP_EMAC_MII_RXD2

GPF_MFPL PF3 setting for EMAC_MII_RXD2

Definition at line 788 of file sys.h.

## ◆ SYS_GPF_MFPL_PF3MFP_GPIO

#define SYS_GPF_MFPL_PF3MFP_GPIO

GPF_MFPL PF3 setting for GPIO

Definition at line 785 of file sys.h.

## ◆ SYS_GPF_MFPL_PF3MFP_SD0_DAT2

#define SYS_GPF_MFPL_PF3MFP_SD0_DAT2

GPF_MFPL PF3 setting for SD0_DAT2

Definition at line 787 of file sys.h.

## ◆ SYS_GPF_MFPL_PF3MFP_SPI3_CLK

#define SYS_GPF_MFPL_PF3MFP_SPI3_CLK

GPF_MFPL PF3 setting for SPI3_CLK

Definition at line 786 of file sys.h.

## ◆ SYS_GPF_MFPL_PF4MFP_EMAC_MII_COL0

#define SYS_GPF_MFPL_PF4MFP_EMAC_MII_COL0

GPF_MFPL PF4 setting for EMAC_MII_COL0

Definition at line 794 of file sys.h.

## ◆ SYS_GPF_MFPL_PF4MFP_GPIO

#define SYS_GPF_MFPL_PF4MFP_GPIO

GPF_MFPL PF4 setting for GPIO

Definition at line 791 of file sys.h.

## ◆ SYS_GPF_MFPL_PF4MFP_SD0_DAT1

#define SYS_GPF_MFPL_PF4MFP_SD0_DAT1

GPF_MFPL PF4 setting for SD0_DAT1

Definition at line 793 of file sys.h.

## ◆ SYS_GPF_MFPL_PF4MFP_SPI3_MISO0

#define SYS_GPF_MFPL_PF4MFP_SPI3_MISO0

GPF_MFPL PF4 setting for SPI3_MISO0

Definition at line 792 of file sys.h.

## ◆ SYS_GPF_MFPL_PF5MFP_EMAC_MII_CRS

#define SYS_GPF_MFPL_PF5MFP_EMAC_MII_CRS

GPF_MFPL PF5 setting for EMAC_MII_CRS

Definition at line 800 of file sys.h.

## ◆ SYS_GPF_MFPL_PF5MFP_GPIO

#define SYS_GPF_MFPL_PF5MFP_GPIO

GPF_MFPL PF5 setting for GPIO

Definition at line 797 of file sys.h.

## ◆ SYS_GPF_MFPL_PF5MFP_SD0_DAT0

#define SYS_GPF_MFPL_PF5MFP_SD0_DAT0

GPF_MFPL PF5 setting for SD0_DAT0

Definition at line 799 of file sys.h.

## ◆ SYS_GPF_MFPL_PF5MFP_SPI3_MOSI0

#define SYS_GPF_MFPL_PF5MFP_SPI3_MOSI0

GPF_MFPL PF5 setting for SPI3_MOSI0

Definition at line 798 of file sys.h.

## ◆ SYS_GPF_MFPL_PF6MFP_EMAC_MII_TXCLK

#define SYS_GPF_MFPL_PF6MFP_EMAC_MII_TXCLK

GPF_MFPL PF6 setting for EMAC_MII_TXCLK

Definition at line 806 of file sys.h.

## ◆ SYS_GPF_MFPL_PF6MFP_GPIO

#define SYS_GPF_MFPL_PF6MFP_GPIO

GPF_MFPL PF6 setting for GPIO

Definition at line 803 of file sys.h.

## ◆ SYS_GPF_MFPL_PF6MFP_SD0_CDn

#define SYS_GPF_MFPL_PF6MFP_SD0_CDn

GPF_MFPL PF6 setting for SD0_CDn

Definition at line 805 of file sys.h.

## ◆ SYS_GPF_MFPL_PF6MFP_UART2_RXD

#define SYS_GPF_MFPL_PF6MFP_UART2_RXD

GPF_MFPL PF6 setting for UART2_RXD

Definition at line 804 of file sys.h.

## ◆ SYS_GPF_MFPL_PF7MFP_EMAC_MII_TXD3

#define SYS_GPF_MFPL_PF7MFP_EMAC_MII_TXD3

GPF_MFPL PF7 setting for EMAC_MII_TXD3

Definition at line 812 of file sys.h.

## ◆ SYS_GPF_MFPL_PF7MFP_GPIO

#define SYS_GPF_MFPL_PF7MFP_GPIO

GPF_MFPL PF7 setting for GPIO

Definition at line 809 of file sys.h.

## ◆ SYS_GPF_MFPL_PF7MFP_SD0_CMD

#define SYS_GPF_MFPL_PF7MFP_SD0_CMD

GPF_MFPL PF7 setting for SD0_CMD

Definition at line 811 of file sys.h.

## ◆ SYS_GPF_MFPL_PF7MFP_UART2_TXD

#define SYS_GPF_MFPL_PF7MFP_UART2_TXD

GPF_MFPL PF7 setting for UART2_TXD

Definition at line 810 of file sys.h.

## ◆ SYS_GPG_MFPH_PG10MFP_GPIO

#define SYS_GPG_MFPH_PG10MFP_GPIO

GPG_MFPH PG10 setting for GPIO

Definition at line 915 of file sys.h.

## ◆ SYS_GPG_MFPH_PG10MFP_ICE_CLK

#define SYS_GPG_MFPH_PG10MFP_ICE_CLK

GPG_MFPH PG10 setting for ICE_CLK

Definition at line 916 of file sys.h.

## ◆ SYS_GPG_MFPH_PG10MFP_JTAG_TCLK

#define SYS_GPG_MFPH_PG10MFP_JTAG_TCLK

GPG_MFPH PG10 setting for JTAG_TCLK

Definition at line 917 of file sys.h.

## ◆ SYS_GPG_MFPH_PG11MFP_GPIO

#define SYS_GPG_MFPH_PG11MFP_GPIO

GPG_MFPH PG11 setting for GPIO

Definition at line 920 of file sys.h.

## ◆ SYS_GPG_MFPH_PG11MFP_ICE_DAT

#define SYS_GPG_MFPH_PG11MFP_ICE_DAT

GPG_MFPH PG11 setting for ICE_DAT

Definition at line 921 of file sys.h.

## ◆ SYS_GPG_MFPH_PG11MFP_JTAG_TMS

#define SYS_GPG_MFPH_PG11MFP_JTAG_TMS

GPG_MFPH PG11 setting for JTAG_TMS

Definition at line 922 of file sys.h.

## ◆ SYS_GPG_MFPH_PG12MFP_GPIO

#define SYS_GPG_MFPH_PG12MFP_GPIO

GPG_MFPH PG12 setting for GPIO

Definition at line 925 of file sys.h.

## ◆ SYS_GPG_MFPH_PG12MFP_XT1_OUT

#define SYS_GPG_MFPH_PG12MFP_XT1_OUT

GPG_MFPH PG12 setting for XT1_OUT

Definition at line 926 of file sys.h.

## ◆ SYS_GPG_MFPH_PG13MFP_GPIO

#define SYS_GPG_MFPH_PG13MFP_GPIO

GPG_MFPH PG13 setting for GPIO

Definition at line 929 of file sys.h.

## ◆ SYS_GPG_MFPH_PG13MFP_XT1_IN

#define SYS_GPG_MFPH_PG13MFP_XT1_IN

GPG_MFPH PG13 setting for XT1_IN

Definition at line 930 of file sys.h.

## ◆ SYS_GPG_MFPH_PG14MFP_GPIO

#define SYS_GPG_MFPH_PG14MFP_GPIO

GPG_MFPH PG14 setting for GPIO

Definition at line 933 of file sys.h.

## ◆ SYS_GPG_MFPH_PG14MFP_I2C1_SDA

#define SYS_GPG_MFPH_PG14MFP_I2C1_SDA

GPG_MFPH PG14 setting for I2C1_SDA

Definition at line 935 of file sys.h.

## ◆ SYS_GPG_MFPH_PG14MFP_X32K_OUT

#define SYS_GPG_MFPH_PG14MFP_X32K_OUT

GPG_MFPH PG14 setting for X32K_OUT

Definition at line 934 of file sys.h.

## ◆ SYS_GPG_MFPH_PG15MFP_GPIO

#define SYS_GPG_MFPH_PG15MFP_GPIO

GPG_MFPH PG15 setting for GPIO

Definition at line 938 of file sys.h.

## ◆ SYS_GPG_MFPH_PG15MFP_I2C1_SCL

#define SYS_GPG_MFPH_PG15MFP_I2C1_SCL

GPG_MFPH PG15 setting for I2C1_SCL

Definition at line 940 of file sys.h.

## ◆ SYS_GPG_MFPH_PG15MFP_X32K_IN

#define SYS_GPG_MFPH_PG15MFP_X32K_IN

GPG_MFPH PG15 setting for X32K_IN

Definition at line 939 of file sys.h.

## ◆ SYS_GPG_MFPH_PG8MFP_GPIO

#define SYS_GPG_MFPH_PG8MFP_GPIO

GPG_MFPH PG8 setting for GPIO

Definition at line 901 of file sys.h.

## ◆ SYS_GPG_MFPH_PG8MFP_I2S1_DO

#define SYS_GPG_MFPH_PG8MFP_I2S1_DO

GPG_MFPH PG8 setting for I2S1_DO

Definition at line 903 of file sys.h.

## ◆ SYS_GPG_MFPH_PG8MFP_SC3_DAT

#define SYS_GPG_MFPH_PG8MFP_SC3_DAT

GPG_MFPH PG8 setting for SC3_DAT

Definition at line 905 of file sys.h.

## ◆ SYS_GPG_MFPH_PG8MFP_SPI2_MOSI0

#define SYS_GPG_MFPH_PG8MFP_SPI2_MOSI0

GPG_MFPH PG8 setting for SPI2_MOSI0

Definition at line 902 of file sys.h.

## ◆ SYS_GPG_MFPH_PG8MFP_UART4_RTS

#define SYS_GPG_MFPH_PG8MFP_UART4_RTS

GPG_MFPH PG8 setting for UART4_RTS

Definition at line 904 of file sys.h.

## ◆ SYS_GPG_MFPH_PG9MFP_GPIO

#define SYS_GPG_MFPH_PG9MFP_GPIO

GPG_MFPH PG9 setting for GPIO

Definition at line 908 of file sys.h.

## ◆ SYS_GPG_MFPH_PG9MFP_I2S1_DI

#define SYS_GPG_MFPH_PG9MFP_I2S1_DI

GPG_MFPH PG9 setting for I2S1_DI

Definition at line 910 of file sys.h.

## ◆ SYS_GPG_MFPH_PG9MFP_SC3_CLK

#define SYS_GPG_MFPH_PG9MFP_SC3_CLK

GPG_MFPH PG9 setting for SC3_CLK

Definition at line 912 of file sys.h.

## ◆ SYS_GPG_MFPH_PG9MFP_SPI2_CLK

#define SYS_GPG_MFPH_PG9MFP_SPI2_CLK

GPG_MFPH PG9 setting for SPI2_CLK

Definition at line 909 of file sys.h.

## ◆ SYS_GPG_MFPH_PG9MFP_UART4_CTS

#define SYS_GPG_MFPH_PG9MFP_UART4_CTS

GPG_MFPH PG9 setting for UART4_CTS

Definition at line 911 of file sys.h.

## ◆ SYS_GPG_MFPL_PG0MFP_GPIO

#define SYS_GPG_MFPL_PG0MFP_GPIO

GPG_MFPL PG0 setting for GPIO

Definition at line 861 of file sys.h.

## ◆ SYS_GPG_MFPL_PG0MFP_INT6

#define SYS_GPG_MFPL_PG0MFP_INT6

GPG_MFPL PG0 setting for INT6

Definition at line 863 of file sys.h.

## ◆ SYS_GPG_MFPL_PG0MFP_UART0_CTS

#define SYS_GPG_MFPL_PG0MFP_UART0_CTS

GPG_MFPL PG0 setting for UART0_CTS

Definition at line 862 of file sys.h.

## ◆ SYS_GPG_MFPL_PG1MFP_GPIO

#define SYS_GPG_MFPL_PG1MFP_GPIO

GPG_MFPL PG1 setting for GPIO

Definition at line 866 of file sys.h.

## ◆ SYS_GPG_MFPL_PG1MFP_UART0_RXD

#define SYS_GPG_MFPL_PG1MFP_UART0_RXD

GPG_MFPL PG1 setting for UART0_RXD

Definition at line 867 of file sys.h.

## ◆ SYS_GPG_MFPL_PG2MFP_GPIO

#define SYS_GPG_MFPL_PG2MFP_GPIO

GPG_MFPL PG2 setting for GPIO

Definition at line 870 of file sys.h.

## ◆ SYS_GPG_MFPL_PG2MFP_UART0_TXD

#define SYS_GPG_MFPL_PG2MFP_UART0_TXD

GPG_MFPL PG2 setting for UART0_TXD

Definition at line 871 of file sys.h.

## ◆ SYS_GPG_MFPL_PG3MFP_GPIO

#define SYS_GPG_MFPL_PG3MFP_GPIO

GPG_MFPL PG3 setting for GPIO

Definition at line 874 of file sys.h.

## ◆ SYS_GPG_MFPL_PG3MFP_I2S1_DO

#define SYS_GPG_MFPL_PG3MFP_I2S1_DO

GPG_MFPL PG3 setting for I2S1_DO

Definition at line 876 of file sys.h.

## ◆ SYS_GPG_MFPL_PG3MFP_PS2_CLK

#define SYS_GPG_MFPL_PG3MFP_PS2_CLK

GPG_MFPL PG3 setting for PS2_CLK

Definition at line 875 of file sys.h.

## ◆ SYS_GPG_MFPL_PG3MFP_SC1_RST

#define SYS_GPG_MFPL_PG3MFP_SC1_RST

GPG_MFPL PG3 setting for SC1_RST

Definition at line 877 of file sys.h.

## ◆ SYS_GPG_MFPL_PG4MFP_GPIO

#define SYS_GPG_MFPL_PG4MFP_GPIO

GPG_MFPL PG4 setting for GPIO

Definition at line 879 of file sys.h.

## ◆ SYS_GPG_MFPL_PG4MFP_I2S1_DI

#define SYS_GPG_MFPL_PG4MFP_I2S1_DI

GPG_MFPL PG4 setting for I2S1_DI

Definition at line 881 of file sys.h.

## ◆ SYS_GPG_MFPL_PG4MFP_PS2_DAT

#define SYS_GPG_MFPL_PG4MFP_PS2_DAT

GPG_MFPL PG4 setting for PS2_DAT

Definition at line 880 of file sys.h.

## ◆ SYS_GPG_MFPL_PG4MFP_SC1_PWR

#define SYS_GPG_MFPL_PG4MFP_SC1_PWR

GPG_MFPL PG4 setting for SC1_PWR

Definition at line 882 of file sys.h.

## ◆ SYS_GPG_MFPL_PG5MFP_GPIO

#define SYS_GPG_MFPL_PG5MFP_GPIO

GPG_MFPL PG5 setting for GPIO

Definition at line 885 of file sys.h.

## ◆ SYS_GPG_MFPL_PG5MFP_I2S1_BCLK

#define SYS_GPG_MFPL_PG5MFP_I2S1_BCLK

GPG_MFPL PG5 setting for I2S1_BCLK

Definition at line 886 of file sys.h.

## ◆ SYS_GPG_MFPL_PG5MFP_SC1_DAT

#define SYS_GPG_MFPL_PG5MFP_SC1_DAT

GPG_MFPL PG5 setting for SC1_DAT

Definition at line 887 of file sys.h.

## ◆ SYS_GPG_MFPL_PG6MFP_GPIO

#define SYS_GPG_MFPL_PG6MFP_GPIO

GPG_MFPL PG6 setting for GPIO

Definition at line 889 of file sys.h.

## ◆ SYS_GPG_MFPL_PG6MFP_I2S1_LRCK

#define SYS_GPG_MFPL_PG6MFP_I2S1_LRCK

GPG_MFPL PG6 setting for I2S1_LRCK

Definition at line 890 of file sys.h.

## ◆ SYS_GPG_MFPL_PG6MFP_SC1_CLK

#define SYS_GPG_MFPL_PG6MFP_SC1_CLK

GPG_MFPL PG6 setting for SC1_CLK

Definition at line 891 of file sys.h.

## ◆ SYS_GPG_MFPL_PG7MFP_GPIO

#define SYS_GPG_MFPL_PG7MFP_GPIO

GPG_MFPL PG7 setting for GPIO

Definition at line 894 of file sys.h.

## ◆ SYS_GPG_MFPL_PG7MFP_I2S1_MCLK

#define SYS_GPG_MFPL_PG7MFP_I2S1_MCLK

GPG_MFPL PG7 setting for I2S1_MCLK

Definition at line 896 of file sys.h.

## ◆ SYS_GPG_MFPL_PG7MFP_SC1_CD

#define SYS_GPG_MFPL_PG7MFP_SC1_CD

GPG_MFPL PG7 setting for SC1_CD

Definition at line 897 of file sys.h.

## ◆ SYS_GPG_MFPL_PG7MFP_SC3_RST

#define SYS_GPG_MFPL_PG7MFP_SC3_RST

GPG_MFPL PG7 setting for SC3_RST

Definition at line 898 of file sys.h.

## ◆ SYS_GPG_MFPL_PG7MFP_SPI2_MISO0

#define SYS_GPG_MFPL_PG7MFP_SPI2_MISO0

GPG_MFPL PG7 setting for SPI2_MISO0

Definition at line 895 of file sys.h.

## ◆ SYS_GPH_MFPH_PH10MFP_GPIO

#define SYS_GPH_MFPH_PH10MFP_GPIO

GPH_MFPH PH10 setting for GPIO

Definition at line 989 of file sys.h.

## ◆ SYS_GPH_MFPH_PH10MFP_SPI2_MOSI1

#define SYS_GPH_MFPH_PH10MFP_SPI2_MOSI1

GPH_MFPH PH10 setting for SPI2_MOSI1

Definition at line 990 of file sys.h.

## ◆ SYS_GPH_MFPH_PH11MFP_GPIO

#define SYS_GPH_MFPH_PH11MFP_GPIO

GPH_MFPH PH11 setting for GPIO

Definition at line 993 of file sys.h.

## ◆ SYS_GPH_MFPH_PH11MFP_UART3_RXD

#define SYS_GPH_MFPH_PH11MFP_UART3_RXD

GPH_MFPH PH11 setting for UART3_RXD

Definition at line 994 of file sys.h.

## ◆ SYS_GPH_MFPH_PH12MFP_GPIO

#define SYS_GPH_MFPH_PH12MFP_GPIO

GPH_MFPH PH12 setting for GPIO

Definition at line 997 of file sys.h.

## ◆ SYS_GPH_MFPH_PH12MFP_UART3_TXD

#define SYS_GPH_MFPH_PH12MFP_UART3_TXD

GPH_MFPH PH12 setting for UART3_TXD

Definition at line 998 of file sys.h.

## ◆ SYS_GPH_MFPH_PH13MFP_GPIO

#define SYS_GPH_MFPH_PH13MFP_GPIO

GPH_MFPH PH13 setting for GPIO

Definition at line 1001 of file sys.h.

## ◆ SYS_GPH_MFPH_PH13MFP_UART3_RTS

#define SYS_GPH_MFPH_PH13MFP_UART3_RTS

GPH_MFPH PH13 setting for UART3_RTS

Definition at line 1002 of file sys.h.

## ◆ SYS_GPH_MFPH_PH14MFP_GPIO

#define SYS_GPH_MFPH_PH14MFP_GPIO

GPH_MFPH PH14 setting for GPIO

Definition at line 1005 of file sys.h.

## ◆ SYS_GPH_MFPH_PH14MFP_UART3_CTS

#define SYS_GPH_MFPH_PH14MFP_UART3_CTS

GPH_MFPH PH14 setting for UART3_CTS

Definition at line 1006 of file sys.h.

## ◆ SYS_GPH_MFPH_PH15MFP_GPIO

#define SYS_GPH_MFPH_PH15MFP_GPIO

GPH_MFPH PH15 setting for GPIO

Definition at line 1009 of file sys.h.

## ◆ SYS_GPH_MFPH_PH15MFP_SC5_CLK

#define SYS_GPH_MFPH_PH15MFP_SC5_CLK

GPH_MFPH PH15 setting for SC5_CLK

Definition at line 1010 of file sys.h.

## ◆ SYS_GPH_MFPH_PH8MFP_GPIO

#define SYS_GPH_MFPH_PH8MFP_GPIO

GPH_MFPH PH8 setting for GPIO

Definition at line 981 of file sys.h.

## ◆ SYS_GPH_MFPH_PH8MFP_SPI2_MOSI0

#define SYS_GPH_MFPH_PH8MFP_SPI2_MOSI0

GPH_MFPH PH8 setting for SPI2_MOSI0

Definition at line 982 of file sys.h.

## ◆ SYS_GPH_MFPH_PH9MFP_GPIO

#define SYS_GPH_MFPH_PH9MFP_GPIO

GPH_MFPH PH9 setting for GPIO

Definition at line 985 of file sys.h.

## ◆ SYS_GPH_MFPH_PH9MFP_SPI2_MISO1

#define SYS_GPH_MFPH_PH9MFP_SPI2_MISO1

GPH_MFPH PH9 setting for SPI2_MISO1

Definition at line 986 of file sys.h.

## ◆ SYS_GPH_MFPL_PH0MFP_CAN1_RXD

#define SYS_GPH_MFPL_PH0MFP_CAN1_RXD

GPH_MFPL PH0 setting for CAN1_RXD

Definition at line 947 of file sys.h.

## ◆ SYS_GPH_MFPL_PH0MFP_GPIO

#define SYS_GPH_MFPL_PH0MFP_GPIO

GPH_MFPL PH0 setting for GPIO

Definition at line 944 of file sys.h.

## ◆ SYS_GPH_MFPL_PH0MFP_I2C1_SCL

#define SYS_GPH_MFPL_PH0MFP_I2C1_SCL

GPH_MFPL PH0 setting for I2C1_SCL

Definition at line 945 of file sys.h.

## ◆ SYS_GPH_MFPL_PH0MFP_INT7

#define SYS_GPH_MFPL_PH0MFP_INT7

GPH_MFPL PH0 setting for INT7

Definition at line 948 of file sys.h.

## ◆ SYS_GPH_MFPL_PH0MFP_UART4_RXD

#define SYS_GPH_MFPL_PH0MFP_UART4_RXD

GPH_MFPL PH0 setting for UART4_RXD

Definition at line 946 of file sys.h.

## ◆ SYS_GPH_MFPL_PH1MFP_CAN1_TXD

#define SYS_GPH_MFPL_PH1MFP_CAN1_TXD

GPH_MFPL PH1 setting for CAN1_TXD

Definition at line 954 of file sys.h.

## ◆ SYS_GPH_MFPL_PH1MFP_GPIO

#define SYS_GPH_MFPL_PH1MFP_GPIO

GPH_MFPL PH1 setting for GPIO

Definition at line 951 of file sys.h.

## ◆ SYS_GPH_MFPL_PH1MFP_I2C1_SDA

#define SYS_GPH_MFPL_PH1MFP_I2C1_SDA

GPH_MFPL PH1 setting for I2C1_SDA

Definition at line 953 of file sys.h.

## ◆ SYS_GPH_MFPL_PH1MFP_UART4_TXD

#define SYS_GPH_MFPL_PH1MFP_UART4_TXD

GPH_MFPL PH1 setting for UART4_TXD

Definition at line 952 of file sys.h.

## ◆ SYS_GPH_MFPL_PH2MFP_GPIO

#define SYS_GPH_MFPL_PH2MFP_GPIO

GPH_MFPL PH2 setting for GPIO

Definition at line 957 of file sys.h.

## ◆ SYS_GPH_MFPL_PH2MFP_UART2_CTS

#define SYS_GPH_MFPL_PH2MFP_UART2_CTS

GPH_MFPL PH2 setting for UART2_CTS

Definition at line 958 of file sys.h.

## ◆ SYS_GPH_MFPL_PH3MFP_GPIO

#define SYS_GPH_MFPL_PH3MFP_GPIO

GPH_MFPL PH3 setting for GPIO

Definition at line 961 of file sys.h.

## ◆ SYS_GPH_MFPL_PH3MFP_I2C3_SCL

#define SYS_GPH_MFPL_PH3MFP_I2C3_SCL

GPH_MFPL PH3 setting for I2C3_SCL

Definition at line 962 of file sys.h.

## ◆ SYS_GPH_MFPL_PH4MFP_GPIO

#define SYS_GPH_MFPL_PH4MFP_GPIO

GPH_MFPL PH4 setting for GPIO

Definition at line 965 of file sys.h.

## ◆ SYS_GPH_MFPL_PH4MFP_I2C3_SDA

#define SYS_GPH_MFPL_PH4MFP_I2C3_SDA

GPH_MFPL PH4 setting for I2C3_SDA

Definition at line 966 of file sys.h.

## ◆ SYS_GPH_MFPL_PH5MFP_GPIO

#define SYS_GPH_MFPL_PH5MFP_GPIO

GPH_MFPL PH5 setting for GPIO

Definition at line 969 of file sys.h.

## ◆ SYS_GPH_MFPL_PH5MFP_SPI2_SS0

#define SYS_GPH_MFPL_PH5MFP_SPI2_SS0

GPH_MFPL PH5 setting for SPI2_SS0

Definition at line 970 of file sys.h.

## ◆ SYS_GPH_MFPL_PH6MFP_GPIO

#define SYS_GPH_MFPL_PH6MFP_GPIO

GPH_MFPL PH6 setting for GPIO

Definition at line 973 of file sys.h.

## ◆ SYS_GPH_MFPL_PH6MFP_SPI2_CLK

#define SYS_GPH_MFPL_PH6MFP_SPI2_CLK

GPH_MFPL PH6 setting for SPI2_CLK

Definition at line 974 of file sys.h.

## ◆ SYS_GPH_MFPL_PH7MFP_GPIO

#define SYS_GPH_MFPL_PH7MFP_GPIO

GPH_MFPL PH7 setting for GPIO

Definition at line 977 of file sys.h.

## ◆ SYS_GPH_MFPL_PH7MFP_SPI2_MISO0

#define SYS_GPH_MFPL_PH7MFP_SPI2_MISO0

GPH_MFPL PH7 setting for SPI2_MISO0

Definition at line 978 of file sys.h.

## ◆ SYS_GPI_MFPH_PI10MFP_GPIO

#define SYS_GPI_MFPH_PI10MFP_GPIO

GPI_MFPH PI10 setting for GPIO

Definition at line 1055 of file sys.h.

## ◆ SYS_GPI_MFPH_PI11MFP_GPIO

#define SYS_GPI_MFPH_PI11MFP_GPIO

GPI_MFPH PI11 setting for GPIO

Definition at line 1058 of file sys.h.

## ◆ SYS_GPI_MFPH_PI11MFP_I2C4_SCL

#define SYS_GPI_MFPH_PI11MFP_I2C4_SCL

GPI_MFPH PI11 setting for I2C4_SCL

Definition at line 1061 of file sys.h.

## ◆ SYS_GPI_MFPH_PI11MFP_I2S1_BCLK

#define SYS_GPI_MFPH_PI11MFP_I2S1_BCLK

GPI_MFPH PI11 setting for I2S1_BCLK

Definition at line 1060 of file sys.h.

## ◆ SYS_GPI_MFPH_PI11MFP_SC3_PWR

#define SYS_GPI_MFPH_PI11MFP_SC3_PWR

GPI_MFPH PI11 setting for SC3_PWR

Definition at line 1062 of file sys.h.

## ◆ SYS_GPI_MFPH_PI11MFP_SPI2_SS0

#define SYS_GPI_MFPH_PI11MFP_SPI2_SS0

GPI_MFPH PI11 setting for SPI2_SS0

Definition at line 1059 of file sys.h.

## ◆ SYS_GPI_MFPH_PI12MFP_GPIO

#define SYS_GPI_MFPH_PI12MFP_GPIO

GPI_MFPH PI12 setting for GPIO

Definition at line 1065 of file sys.h.

## ◆ SYS_GPI_MFPH_PI12MFP_I2C4_SDA

#define SYS_GPI_MFPH_PI12MFP_I2C4_SDA

GPI_MFPH PI12 setting for I2C4_SDA

Definition at line 1068 of file sys.h.

## ◆ SYS_GPI_MFPH_PI12MFP_I2S1_LRCK

#define SYS_GPI_MFPH_PI12MFP_I2S1_LRCK

GPI_MFPH PI12 setting for I2S1_LRCK

Definition at line 1067 of file sys.h.

## ◆ SYS_GPI_MFPH_PI12MFP_SC3_CD

#define SYS_GPI_MFPH_PI12MFP_SC3_CD

GPI_MFPH PI12 setting for SC3_CD

Definition at line 1069 of file sys.h.

## ◆ SYS_GPI_MFPH_PI12MFP_SPI2_MISO1

#define SYS_GPI_MFPH_PI12MFP_SPI2_MISO1

GPI_MFPH PI12 setting for SPI2_MISO1

Definition at line 1066 of file sys.h.

## ◆ SYS_GPI_MFPH_PI13MFP_GPIO

#define SYS_GPI_MFPH_PI13MFP_GPIO

GPI_MFPH PI13 setting for GPIO

Definition at line 1072 of file sys.h.

## ◆ SYS_GPI_MFPH_PI14MFP_GPIO

#define SYS_GPI_MFPH_PI14MFP_GPIO

GPI_MFPH PI14 setting for GPIO

Definition at line 1075 of file sys.h.

## ◆ SYS_GPI_MFPH_PI15MFP_GPIO

#define SYS_GPI_MFPH_PI15MFP_GPIO

GPI_MFPH PI15 setting for GPIO

Definition at line 1078 of file sys.h.

## ◆ SYS_GPI_MFPH_PI8MFP_GPIO

#define SYS_GPI_MFPH_PI8MFP_GPIO

GPI_MFPH PI8 setting for GPIO

Definition at line 1046 of file sys.h.

## ◆ SYS_GPI_MFPH_PI8MFP_I2C2_SDA

#define SYS_GPI_MFPH_PI8MFP_I2C2_SDA

GPI_MFPH PI8 setting for I2C2_SDA

Definition at line 1047 of file sys.h.

## ◆ SYS_GPI_MFPH_PI8MFP_SPI3_MOSI1

#define SYS_GPI_MFPH_PI8MFP_SPI3_MOSI1

GPI_MFPH PI8 setting for SPI3_MOSI1

Definition at line 1048 of file sys.h.

## ◆ SYS_GPI_MFPH_PI9MFP_GPIO

#define SYS_GPI_MFPH_PI9MFP_GPIO

GPI_MFPH PI9 setting for GPIO

Definition at line 1051 of file sys.h.

## ◆ SYS_GPI_MFPH_PI9MFP_I2C4_SCL

#define SYS_GPI_MFPH_PI9MFP_I2C4_SCL

GPI_MFPH PI9 setting for I2C4_SCL

Definition at line 1052 of file sys.h.

## ◆ SYS_GPI_MFPL_PI0MFP_GPIO

#define SYS_GPI_MFPL_PI0MFP_GPIO

GPI_MFPL PI0 setting for GPIO

Definition at line 1013 of file sys.h.

## ◆ SYS_GPI_MFPL_PI0MFP_SC5_RST

#define SYS_GPI_MFPL_PI0MFP_SC5_RST

GPI_MFPL PI0 setting for SC5_RST

Definition at line 1014 of file sys.h.

## ◆ SYS_GPI_MFPL_PI1MFP_GPIO

#define SYS_GPI_MFPL_PI1MFP_GPIO

GPI_MFPL PI1 setting for GPIO

Definition at line 1017 of file sys.h.

## ◆ SYS_GPI_MFPL_PI1MFP_SC5_PWR

#define SYS_GPI_MFPL_PI1MFP_SC5_PWR

GPI_MFPL PI1 setting for SC5_PWR

Definition at line 1018 of file sys.h.

## ◆ SYS_GPI_MFPL_PI2MFP_GPIO

#define SYS_GPI_MFPL_PI2MFP_GPIO

GPI_MFPL PI2 setting for GPIO

Definition at line 1021 of file sys.h.

## ◆ SYS_GPI_MFPL_PI2MFP_SC5_DAT

#define SYS_GPI_MFPL_PI2MFP_SC5_DAT

GPI_MFPL PI2 setting for SC5_DAT

Definition at line 1022 of file sys.h.

## ◆ SYS_GPI_MFPL_PI3MFP_GPIO

#define SYS_GPI_MFPL_PI3MFP_GPIO

GPI_MFPL PI3 setting for GPIO

Definition at line 1025 of file sys.h.

## ◆ SYS_GPI_MFPL_PI3MFP_SPI3_SS0

#define SYS_GPI_MFPL_PI3MFP_SPI3_SS0

GPI_MFPL PI3 setting for SPI3_SS0

Definition at line 1026 of file sys.h.

## ◆ SYS_GPI_MFPL_PI4MFP_GPIO

#define SYS_GPI_MFPL_PI4MFP_GPIO

GPI_MFPL PI4 setting for GPIO

Definition at line 1029 of file sys.h.

## ◆ SYS_GPI_MFPL_PI4MFP_SPI3_CLK

#define SYS_GPI_MFPL_PI4MFP_SPI3_CLK

GPI_MFPL PI4 setting for SPI3_CLK

Definition at line 1030 of file sys.h.

## ◆ SYS_GPI_MFPL_PI5MFP_GPIO

#define SYS_GPI_MFPL_PI5MFP_GPIO

GPI_MFPL PI5 setting for GPIO

Definition at line 1033 of file sys.h.

## ◆ SYS_GPI_MFPL_PI5MFP_SPI3_MISO0

#define SYS_GPI_MFPL_PI5MFP_SPI3_MISO0

GPI_MFPL PI5 setting for SPI3_MISO0

Definition at line 1034 of file sys.h.

## ◆ SYS_GPI_MFPL_PI6MFP_GPIO

#define SYS_GPI_MFPL_PI6MFP_GPIO

GPI_MFPL PI6 setting for GPIO

Definition at line 1037 of file sys.h.

## ◆ SYS_GPI_MFPL_PI6MFP_SPI3_MOSI0

#define SYS_GPI_MFPL_PI6MFP_SPI3_MOSI0

GPI_MFPL PI6 setting for SPI3_MOSI0

Definition at line 1038 of file sys.h.

## ◆ SYS_GPI_MFPL_PI7MFP_GPIO

#define SYS_GPI_MFPL_PI7MFP_GPIO

GPI_MFPL PI7 setting for GPIO

Definition at line 1041 of file sys.h.

## ◆ SYS_GPI_MFPL_PI7MFP_I2C2_SCL

#define SYS_GPI_MFPL_PI7MFP_I2C2_SCL

GPI_MFPL PI7 setting for I2C2_SCL

Definition at line 1042 of file sys.h.

## ◆ SYS_GPI_MFPL_PI7MFP_SPI3_MISO1

#define SYS_GPI_MFPL_PI7MFP_SPI3_MISO1

GPI_MFPL PI7 setting for SPI3_MISO1

Definition at line 1043 of file sys.h.

## ◆ SYS_USBPHY_USBROLE_ID_DEPH

#define SYS_USBPHY_USBROLE_ID_DEPH

ID dependent device

Definition at line 115 of file sys.h.

## ◆ SYS_USBPHY_USBROLE_ON_THE_GO

#define SYS_USBPHY_USBROLE_ON_THE_GO

On-The-Go device

Definition at line 116 of file sys.h.

## ◆ SYS_USBPHY_USBROLE_OTG_V33_EN

#define SYS_USBPHY_USBROLE_OTG_V33_EN

USB LDO33 Enabled

Definition at line 112 of file sys.h.

## ◆ SYS_USBPHY_USBROLE_STD_USBD

#define SYS_USBPHY_USBROLE_STD_USBD

Standard USB device

Definition at line 113 of file sys.h.

## ◆ SYS_USBPHY_USBROLE_STD_USBH

#define SYS_USBPHY_USBROLE_STD_USBH

Standard USB host

Definition at line 114 of file sys.h.

## ◆ SYS_VREFCTL_ADCMODESEL_ADC

#define SYS_VREFCTL_ADCMODESEL_ADC

ADC mode

Definition at line 106 of file sys.h.

## ◆ SYS_VREFCTL_ADCMODESEL_EADC

#define SYS_VREFCTL_ADCMODESEL_EADC

EADC mode

Definition at line 105 of file sys.h.

## ◆ SYS_VREFCTL_PWMSYNCMODE_EN

#define SYS_VREFCTL_PWMSYNCMODE_EN

PWM SYNC MODE ENABLED, PWM engine clock is same as HCLK

Definition at line 107 of file sys.h.

## ◆ SYS_VREFCTL_VREF_2_048V

#define SYS_VREFCTL_VREF_2_048V

VOUT= 2.048V

Definition at line 101 of file sys.h.

## ◆ SYS_VREFCTL_VREF_2_65V

#define SYS_VREFCTL_VREF_2_65V

VOUT= 2.56V

Definition at line 100 of file sys.h.

## ◆ SYS_VREFCTL_VREF_3_072V

#define SYS_VREFCTL_VREF_3_072V

VOUT= 3.072V

Definition at line 102 of file sys.h.

## ◆ SYS_VREFCTL_VREF_4_096V

#define SYS_VREFCTL_VREF_4_096V

VOUT= 4.096V

Definition at line 103 of file sys.h.

## ◆ SYS_VREFCTL_VREF_AVDD

#define SYS_VREFCTL_VREF_AVDD

VOUT= AVDD

Definition at line 104 of file sys.h.

## ◆ TMR0_RST

#define TMR0_RST

Reset TMR0

Definition at line 45 of file sys.h.

## ◆ TMR1_RST

#define TMR1_RST

Reset TMR1

Definition at line 46 of file sys.h.

## ◆ TMR2_RST

#define TMR2_RST

Reset TMR2

Definition at line 47 of file sys.h.

## ◆ TMR3_RST

#define TMR3_RST

Reset TMR3

Definition at line 48 of file sys.h.

## ◆ UART0_RST

#define UART0_RST

Reset UART0

Definition at line 58 of file sys.h.

## ◆ UART1_RST

#define UART1_RST

Reset UART1

Definition at line 59 of file sys.h.

## ◆ UART2_RST

#define UART2_RST

Reset UART2

Definition at line 60 of file sys.h.

## ◆ UART3_RST

#define UART3_RST

Reset UART3

Definition at line 61 of file sys.h.

## ◆ UART4_RST

#define UART4_RST

Reset UART4

Definition at line 62 of file sys.h.

## ◆ UART5_RST

#define UART5_RST

Reset UART5

Definition at line 63 of file sys.h.

## ◆ USBD_RST

#define USBD_RST

Reset USBD

Definition at line 67 of file sys.h.

## ◆ USBH_RST

#define USBH_RST

Reset USBH

Definition at line 38 of file sys.h.