| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
CLK_T Struct Reference

`#include <NUC472_442.h>`

## Data Fields
__IO uint32_t | PWRCTL
__IO uint32_t | AHBCLK
__IO uint32_t | APBCLK0
__IO uint32_t | APBCLK1
__IO uint32_t | CLKSEL0
__IO uint32_t | CLKSEL1
__IO uint32_t | CLKSEL2
__IO uint32_t | CLKSEL3
__IO uint32_t | CLKDIV0
__IO uint32_t | CLKDIV1
__IO uint32_t | CLKDIV2
__IO uint32_t | CLKDIV3
__IO uint32_t | PLLCTL
__IO uint32_t | PLL2CTL
__IO uint32_t | STATUS
__IO uint32_t | CLKOCTL
__IO uint32_t | CLKDCTL

## Detailed Description

    @addtogroup CLK System Clock Controller(CLK)
    Memory Mapped Structure for CLK Controller

Definition at line 2781 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h