| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Modules | Macros
SC Exported Constants
NUC472/NUC442 Device Driver » SC Driver
Collaboration diagram for SC Exported Constants:

## Modules
| SC Exported Functions

## Macros
#define | SC_INTERFACE_NUM
#define | SC_PIN_STATE_HIGH
#define | SC_PIN_STATE_LOW
#define | SC_PIN_STATE_IGNORE
#define | SC_CLK_ON
#define | SC_CLK_OFF
#define | SC_TMR_MODE_0
#define | SC_TMR_MODE_1
#define | SC_TMR_MODE_2
#define | SC_TMR_MODE_3
#define | SC_TMR_MODE_4
#define | SC_TMR_MODE_5
#define | SC_TMR_MODE_6
#define | SC_TMR_MODE_7
#define | SC_TMR_MODE_8
#define | SC_TMR_MODE_F

## Detailed Description

## Macro Definition Documentation

## ◆ SC_CLK_OFF

#define SC_CLK_OFF

Smartcard clock off

Definition at line 37 of file sc.h.

## ◆ SC_CLK_ON

#define SC_CLK_ON

Smartcard clock on

Definition at line 36 of file sc.h.

## ◆ SC_INTERFACE_NUM

#define SC_INTERFACE_NUM

Smartcard interface numbers

Definition at line 32 of file sc.h.

## ◆ SC_PIN_STATE_HIGH

#define SC_PIN_STATE_HIGH

Smartcard pin status high

Definition at line 33 of file sc.h.

## ◆ SC_PIN_STATE_IGNORE

#define SC_PIN_STATE_IGNORE

Ignore pin status

Definition at line 35 of file sc.h.

## ◆ SC_PIN_STATE_LOW

#define SC_PIN_STATE_LOW

Smartcard pin status low

Definition at line 34 of file sc.h.

## ◆ SC_TMR_MODE_0

#define SC_TMR_MODE_0

Timer Operation Mode 0, down count

Definition at line 39 of file sc.h.

## ◆ SC_TMR_MODE_1

#define SC_TMR_MODE_1

Timer Operation Mode 1, down count, start after detect start bit

Definition at line 40 of file sc.h.

## ◆ SC_TMR_MODE_2

#define SC_TMR_MODE_2

Timer Operation Mode 2, down count, start after receive start bit

Definition at line 41 of file sc.h.

## ◆ SC_TMR_MODE_3

#define SC_TMR_MODE_3

Timer Operation Mode 3, down count, use for activation, only timer 0 support this mode

Definition at line 42 of file sc.h.

## ◆ SC_TMR_MODE_4

#define SC_TMR_MODE_4

Timer Operation Mode 4, down count with reload after timeout

Definition at line 43 of file sc.h.

## ◆ SC_TMR_MODE_5

#define SC_TMR_MODE_5

Timer Operation Mode 5, down count, start after detect start bit, reload after timeout

Definition at line 44 of file sc.h.

## ◆ SC_TMR_MODE_6

#define SC_TMR_MODE_6

Timer Operation Mode 6, down count, start after receive start bit, reload after timeout

Definition at line 45 of file sc.h.

## ◆ SC_TMR_MODE_7

#define SC_TMR_MODE_7

Timer Operation Mode 7, down count, start and reload after detect start bit

Definition at line 46 of file sc.h.

## ◆ SC_TMR_MODE_8

#define SC_TMR_MODE_8

Timer Operation Mode 8, up count

Definition at line 47 of file sc.h.

## ◆ SC_TMR_MODE_F

#define SC_TMR_MODE_F

Timer Operation Mode 15, down count, reload after detect start bit

Definition at line 48 of file sc.h.