| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Modules | Macros
CRC Exported Constants
NUC472/NUC442 Device Driver » CRC Driver
Collaboration diagram for CRC Exported Constants:

## Modules
| CRC Exported Functions

## Macros
#define | CRC_CCITT 0x00000000UL
#define | CRC_8 0x40000000UL
#define | CRC_16 0x80000000UL
#define | CRC_32 0xC0000000UL
#define | CRC_CHECKSUM_COM 0x08000000UL
#define | CRC_CHECKSUM_RVS 0x02000000UL
#define | CRC_WDATA_COM 0x04000000UL
#define | CRC_WDATA_RVS 0x01000000UL
#define | CRC_CPU_WDATA_8 0x00000000UL
#define | CRC_CPU_WDATA_16 0x10000000UL
#define | CRC_CPU_WDATA_32 0x20000000UL

## Detailed Description

## Macro Definition Documentation

## ◆ CRC_16

#define CRC_16 0x80000000UL

CRC Polynomial Mode - CRC16

Definition at line 37 of file crc.h.

## ◆ CRC_32

#define CRC_32 0xC0000000UL

CRC Polynomial Mode - CRC32

Definition at line 38 of file crc.h.

## ◆ CRC_8

#define CRC_8 0x40000000UL

CRC Polynomial Mode - CRC8

Definition at line 36 of file crc.h.

## ◆ CRC_CCITT

#define CRC_CCITT 0x00000000UL

CRC Polynomial Mode - CCITT

Definition at line 35 of file crc.h.

## ◆ CRC_CHECKSUM_COM

#define CRC_CHECKSUM_COM 0x08000000UL

CRC Checksum Complement

Definition at line 43 of file crc.h.

## ◆ CRC_CHECKSUM_RVS

#define CRC_CHECKSUM_RVS 0x02000000UL

CRC Checksum Reverse

Definition at line 44 of file crc.h.

## ◆ CRC_CPU_WDATA_16

#define CRC_CPU_WDATA_16 0x10000000UL

CRC CPU Write Data length is 16-bit

Definition at line 52 of file crc.h.

## ◆ CRC_CPU_WDATA_32

#define CRC_CPU_WDATA_32 0x20000000UL

CRC CPU Write Data length is 32-bit

Definition at line 53 of file crc.h.

## ◆ CRC_CPU_WDATA_8

#define CRC_CPU_WDATA_8 0x00000000UL

CRC CPU Write Data length is 8-bit

Definition at line 51 of file crc.h.

## ◆ CRC_WDATA_COM

#define CRC_WDATA_COM 0x04000000UL

CRC Write Data Complement

Definition at line 45 of file crc.h.

## ◆ CRC_WDATA_RVS

#define CRC_WDATA_RVS 0x01000000UL

CRC Write Data Reverse

Definition at line 46 of file crc.h.