| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
CAN_IF_T Struct Reference

`#include <NUC472_442.h>`

## Data Fields
__IO uint32_t | CREQ
__IO uint32_t | CMASK
__IO uint32_t | MASK1
__IO uint32_t | MASK2
__IO uint32_t | ARB1
__IO uint32_t | ARB2
__IO uint32_t | MCON
__IO uint32_t | DAT_A1
__IO uint32_t | DAT_A2
__IO uint32_t | DAT_B1
__IO uint32_t | DAT_B2

## Detailed Description

    @addtogroup CAN Controller Area Network Controller(CAN)
    Memory Mapped Structure for CAN Controller

Definition at line 849 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h