| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
RTC_T Struct Reference

`#include <NUC472_442.h>`

## Data Fields
__IO uint32_t | INIT
__O uint32_t | RWEN
__IO uint32_t | FREQADJ
__IO uint32_t | TIME
__IO uint32_t | CAL
__IO uint32_t | CLKFMT
__IO uint32_t | WEEKDAY
__IO uint32_t | TALM
__IO uint32_t | CALM
__I uint32_t | LEAPYEAR
__IO uint32_t | INTEN
__IO uint32_t | INTSTS
__IO uint32_t | TICK
__IO uint32_t | SPRCTL
__IO uint32_t | SPR [24]
__IO uint32_t | TAMPCTL
__IO uint32_t | TAMPSTS
__IO uint32_t | TAMP0PCTL
__IO uint32_t | TAMP1PCTL
__IO uint32_t | LXTIPCTL
__IO uint32_t | LXTOPCTL
__IO uint32_t | TAMSK
__IO uint32_t | CAMSK

## Detailed Description

    @addtogroup RTC Real Time Clock Controller(RTC)
    Memory Mapped Structure for RTC Controller

Definition at line 20402 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h