| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

Data Fields
USBH_T Struct Reference

`#include <NUC472_442.h>`

## Data Fields
__I uint32_t | HcRevision
__IO uint32_t | HcControl
__IO uint32_t | HcCommandStatus
__IO uint32_t | HcInterruptStatus
__IO uint32_t | HcInterruptEnable
__IO uint32_t | HcInterruptDisable
__IO uint32_t | HcHCCA
__IO uint32_t | HcPeriodCurrentED
__IO uint32_t | HcControlHeadED
__IO uint32_t | HcControlCurrentED
__IO uint32_t | HcBulkHeadED
__IO uint32_t | HcBulkCurrentED
__IO uint32_t | HcDoneHead
__IO uint32_t | HcFmInterval
__I uint32_t | HcFmRemaining
__I uint32_t | HcFmNumber
__IO uint32_t | HcPeriodicStart
__IO uint32_t | HcLSThreshold
__IO uint32_t | HcRhDescriptorA
__IO uint32_t | HcRhDescriptorB
__IO uint32_t | HcRhStatus
__IO uint32_t | HcRhPortStatus [2]
__IO uint32_t | HcPhyControl
__IO uint32_t | HcMiscControl

## Detailed Description

    @addtogroup USBH USB Host Controller(USBH)
    Memory Mapped Structure for USBH Controller

Definition at line 26148 of file NUC472_442.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/NUC472_442/Include/NUC472_442.h