| NUC472_NUC442_BSP V3.04.000 The Board Support Package for NUC472/NUC442

UmasScsiGlue.h
Go to the documentation of this file.
1/* Driver for USB Mass Storage compliant devices
2 * SCSI Connecting Glue Header File
3 *
4 * $Id: scsiglue.h,v 1.4 2000/08/25 00:13:51 mdharm Exp $
5 *
6 * Current development and maintenance by:
7 * (c) 1999, 2000 Matthew Dharm (mdharm-usb@one-eyed-alien.net)
8 *
9 * This driver is based on the 'USB Mass Storage Class' document. This
10 * describes in detail the protocol used to communicate with such
11 * devices. Clearly, the designers had SCSI and ATAPI commands in
12 * mind when they created this document. The commands are all very
13 * similar to commands in the SCSI-II and ATAPI specifications.
14 *
15 * It is important to note that in a number of cases this class
16 * exhibits class-specific exemptions from the USB specification.
17 * Notably the usage of NAK, STALL and ACK differs from the norm, in
18 * that they are used to communicate wait, failed and OK on commands.
19 *
20 * Also, for certain devices, the interrupt endpoint is used to convey
21 * status of a command.
22 *
23 * Please see http://www.one-eyed-alien.net/~mdharm/linux-usb for more
24 * information about this driver.
25 *
26 * This program is free software; you can redistribute it and/or modify it
27 * under the terms of the GNU General Public License as published by the
28 * Free Software Foundation; either version 2, or (at your option) any
29 * later version.
30 *
31 * This program is distributed in the hope that it will be useful, but
32 * WITHOUT ANY WARRANTY; without even the implied warranty of
33 * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE. See the GNU
34 * General Public License for more details.
35 *
36 * You should have received a copy of the GNU General Public License along
37 * with this program; if not, write to the Free Software Foundation, Inc.,
38 * 675 Mass Ave, Cambridge, MA 02139, USA.
39 */
40
41#ifndef _SCSIGLUE_H_
42#define _SCSIGLUE_H_
43
45
46#define USB_STOR_SCSI_SENSE_HDRSZ 4
47#define USB_STOR_SCSI_SENSE_10_HDRSZ 8
48
49struct usb_stor_scsi_sense_hdr
50{
51 uint8_t *dataLength;
52 uint8_t *mediumType;
53 uint8_t *devSpecParms;
54 uint8_t *blkDescLength;
55};
56
57typedef struct usb_stor_scsi_sense_hdr Usb_Stor_Scsi_Sense_Hdr;
58
59union usb_stor_scsi_sense_hdr_u
60{
61 Usb_Stor_Scsi_Sense_Hdr hdr;
62 uint8_t *array[USB_STOR_SCSI_SENSE_HDRSZ];
63};
64
65typedef union usb_stor_scsi_sense_hdr_u Usb_Stor_Scsi_Sense_Hdr_u;
66
67struct usb_stor_scsi_sense_hdr_10
68{
69 uint8_t *dataLengthMSB;
70 uint8_t *dataLengthLSB;
71 uint8_t *mediumType;
72 uint8_t *devSpecParms;
73 uint8_t *reserved1;
74 uint8_t *reserved2;
75 uint8_t *blkDescLengthMSB;
76 uint8_t *blkDescLengthLSB;
77};
78
79typedef struct usb_stor_scsi_sense_hdr_10 Usb_Stor_Scsi_Sense_Hdr_10;
80
81union usb_stor_scsi_sense_hdr_10_u
82{
83 Usb_Stor_Scsi_Sense_Hdr_10 hdr;
84 uint8_t *array[USB_STOR_SCSI_SENSE_10_HDRSZ];
85};
86
87typedef union usb_stor_scsi_sense_hdr_10_u Usb_Stor_Scsi_Sense_Hdr_10_u;
88
89void usb_stor_scsiSenseParseBuffer( SCSI_CMD_T *, Usb_Stor_Scsi_Sense_Hdr_u *,
90 Usb_Stor_Scsi_Sense_Hdr_10_u *, int *);
91
92
93extern uint8_t usb_stor_sense_notready[18];
94extern Scsi_Host_Template usb_stor_host_template;
95extern int usb_stor_scsiSense10to6(SCSI_CMD_T*);
96extern int usb_stor_scsiSense6to10(SCSI_CMD_T*);
97
99
100#endif