| CMSIS-Core (Cortex-M) CMSIS-Core support for Cortex-M processor-based devices |

Loading...
Searching...
No Matches
Data Fields
FPU_Type Struct Reference

Structure type to access the Floating Point Unit (FPU). More...

## Data Fields
__IOM uint32_t | FPCAR
| Offset: 0x008 (R/W) Floating-Point Context Address Register.
__IOM uint32_t | FPCCR
| Offset: 0x004 (R/W) Floating-Point Context Control Register.
__IOM uint32_t | FPDSCR
| Offset: 0x00C (R/W) Floating-Point Default Status Control Register.
__IM uint32_t | MVFR0
| Offset: 0x010 (R/ ) Media and FP Feature Register 0.
__IM uint32_t | MVFR1
| Offset: 0x014 (R/ ) Media and FP Feature Register 1.

## Description

Structure type to access the Floating Point Unit (FPU).

## Field Documentation

## ◆ FPCAR

__IOM uint32_t FPU_Type::FPCAR

Offset: 0x008 (R/W) Floating-Point Context Address Register.

## ◆ FPCCR

__IOM uint32_t FPU_Type::FPCCR

Offset: 0x004 (R/W) Floating-Point Context Control Register.

## ◆ FPDSCR

__IOM uint32_t FPU_Type::FPDSCR

Offset: 0x00C (R/W) Floating-Point Default Status Control Register.

## ◆ MVFR0

__IM uint32_t FPU_Type::MVFR0

Offset: 0x010 (R/ ) Media and FP Feature Register 0.

## ◆ MVFR1

__IM uint32_t FPU_Type::MVFR1

Offset: 0x014 (R/ ) Media and FP Feature Register 1.