| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Macros
NAND Data Bus Width
NAND Interface » NAND Control Codes

Specify data bus width of the NAND interface. More...

## Macros
#define | ARM_NAND_BUS_DATA_WIDTH_8 (0x00UL)
| Bus Data Width: 8 bit (default)
#define | ARM_NAND_BUS_DATA_WIDTH_16 (0x01UL)
| Bus Data Width: 16 bit.

## Description

Specify data bus width of the NAND interface.

The defines can be used in the function ARM_NAND_Control for the parameter arg and with the ARM_NAND_BUS_DATA_WIDTH as the control code.

## Macro Definition Documentation

## ◆ ARM_NAND_BUS_DATA_WIDTH_8

#define ARM_NAND_BUS_DATA_WIDTH_8 (0x00UL)

Bus Data Width: 8 bit (default)

## ◆ ARM_NAND_BUS_DATA_WIDTH_16

#define ARM_NAND_BUS_DATA_WIDTH_16 (0x01UL)

Bus Data Width: 16 bit.