| CMSIS-Core (Cortex-M) CMSIS-Core support for Cortex-M processor-based devices |

Loading...
Searching...
No Matches
Macros
Device capabilitiy defines

Defines to configure and check device capabilities. More...

## Macros
#define | __ARMv81MML_REV
| Armv8.1-M Baseline device Core revision r0p1.
#define | __ARMv8MBL_REV
| Armv8-M Baseline device Core revision r0p1.
#define | __ARMv8MML_REV
| Armv8-M Mainline device Core revision r0p1.
#define | __CM0_REV
| Cortex-M0 Core revision r0p1.
#define | __CM0PLUS_REV
| Cortex-M0+ Core revision r0p1.
#define | __CM1_REV
| Cortex-M1 Core revision r0p1.
#define | __CM23_REV
| Cortex-M23 Core revision r0p1.
#define | __CM33_REV
| Cortex-M33 Core revision r0p1.
#define | __CM35P_REV
| Cortex-M35P Core revision r0p1.
#define | __CM3_REV
| Cortex-M3 Core revision r0p1.
#define | __CM4_REV
| Cortex-M4 Core revision r0p1.
#define | __CM55_REV
| Cortex-M55 Core revision r0p1.
#define | __CM7_REV
| Cortex-M7 Core revision r0p1.
#define | __CM85_REV
| Cortex-M85 Core revision r0p1.
#define | __DCACHE_PRESENT
| Data Cache present or not.
#define | __DSP_PRESENT
| DSP extension present or not.
#define | __DTCM_PRESENT
| Data Tightly Coupled Memory is present or not.
#define | __FPU_DP
| Double precision FPU present.
#define | __FPU_PRESENT
| FPU present or not.
#define | __ICACHE_PRESENT
| Instruction Cache present or not.
#define | __MPU_PRESENT
| MPU present or not.
#define | __NVIC_PRIO_BITS
| Number of Bits used for Priority Levels.
#define | __PMU_NUM_EVENTCNT
| PMU Event Counters.
#define | __PMU_PRESENT
| PMU present or not.
#define | __SAUREGION_PRESENT
| SAU regions present or not.
#define | __SC000_REV
| SC000 Core revision r0p1.
#define | __SC300_REV
| SC300 Core revision r0p1.
#define | __Vendor_SysTickConfig
| Set to 1 if a venor specfic SysTick configuration is used.
#define | __VTOR_PRESENT
| VTOR present or not.

## Description

Defines to configure and check device capabilities.

These defines are used by the Device Header File <Device.h> in order to enable or disable functionality provided by CMSIS-Core(M) dependent on the device capabilities.

## Macro Definition Documentation

## ◆ __ARMv81MML_REV

#define __ARMv81MML_REV

Armv8.1-M Baseline device Core revision r0p1.

([15:8] revision number, [7:0] patch number)

## ◆ __ARMv8MBL_REV

#define __ARMv8MBL_REV

Armv8-M Baseline device Core revision r0p1.

([15:8] revision number, [7:0] patch number)

## ◆ __ARMv8MML_REV

#define __ARMv8MML_REV

Armv8-M Mainline device Core revision r0p1.

([15:8] revision number, [7:0] patch number)

## ◆ __CM0_REV

#define __CM0_REV

Cortex-M0 Core revision r0p1.

([15:8] revision number, [7:0] patch number)

## ◆ __CM0PLUS_REV

#define __CM0PLUS_REV

Cortex-M0+ Core revision r0p1.

([15:8] revision number, [7:0] patch number)

## ◆ __CM1_REV

#define __CM1_REV

Cortex-M1 Core revision r0p1.

([15:8] revision number, [7:0] patch number)

## ◆ __CM23_REV

#define __CM23_REV

Cortex-M23 Core revision r0p1.

([15:8] revision number, [7:0] patch number)

## ◆ __CM33_REV

#define __CM33_REV

Cortex-M33 Core revision r0p1.

([15:8] revision number, [7:0] patch number)

## ◆ __CM35P_REV

#define __CM35P_REV

Cortex-M35P Core revision r0p1.

([15:8] revision number, [7:0] patch number)

## ◆ __CM3_REV

#define __CM3_REV

Cortex-M3 Core revision r0p1.

([15:8] revision number, [7:0] patch number)

## ◆ __CM4_REV

#define __CM4_REV

Cortex-M4 Core revision r0p1.

([15:8] revision number, [7:0] patch number)

## ◆ __CM55_REV

#define __CM55_REV

Cortex-M55 Core revision r0p1.

([15:8] revision number, [7:0] patch number)

## ◆ __CM7_REV

#define __CM7_REV

Cortex-M7 Core revision r0p1.

([15:8] revision number, [7:0] patch number)

## ◆ __CM85_REV

#define __CM85_REV

Cortex-M85 Core revision r0p1.

([15:8] revision number, [7:0] patch number)

## ◆ __DCACHE_PRESENT

#define __DCACHE_PRESENT

Data Cache present or not.

## ◆ __DSP_PRESENT

#define __DSP_PRESENT

DSP extension present or not.

## ◆ __DTCM_PRESENT

#define __DTCM_PRESENT

Data Tightly Coupled Memory is present or not.

## ◆ __FPU_DP

#define __FPU_DP

Double precision FPU present.

The combination of the defines __FPU_PRESENT and __FPU_DP determine the whether the FPU is with single or double precision as shown in the table below.

__FPU_PRESENT | __FPU_DP | Description
0 | ignored | Processor has no FPU. The value set for __FPU_DP.
1 | 0 | Processor with FPU with single precision.
1 | 1 | Processor with FPU with double precision.

## ◆ __FPU_PRESENT

#define __FPU_PRESENT

FPU present or not.

The combination of the defines __FPU_PRESENT and __FPU_DP determine the whether the FPU is with single or double precision as shown in the table below.

__FPU_PRESENT | __FPU_DP | Description
0 | ignored | Processor has no FPU. The value set for __FPU_DP.
1 | 0 | Processor with FPU with single precision.
1 | 1 | Processor with FPU with double precision.

FPU present

The

## ◆ __ICACHE_PRESENT

#define __ICACHE_PRESENT

Instruction Cache present or not.

## ◆ __MPU_PRESENT

#define __MPU_PRESENT

MPU present or not.

## ◆ __NVIC_PRIO_BITS

#define __NVIC_PRIO_BITS

Number of Bits used for Priority Levels.

## ◆ __PMU_NUM_EVENTCNT

#define __PMU_NUM_EVENTCNT

PMU Event Counters.

The number of Event counters if PMU is present (see __PMU_PRESENT)

## ◆ __PMU_PRESENT

#define __PMU_PRESENT

PMU present or not.

## ◆ __SAUREGION_PRESENT

#define __SAUREGION_PRESENT

SAU regions present or not.

## ◆ __SC000_REV

#define __SC000_REV

SC000 Core revision r0p1.

([15:8] revision number, [7:0] patch number)

## ◆ __SC300_REV

#define __SC300_REV

SC300 Core revision r0p1.

([15:8] revision number, [7:0] patch number)

## ◆ __Vendor_SysTickConfig

#define __Vendor_SysTickConfig

Set to 1 if a venor specfic SysTick configuration is used.

If this define is set to 1, then the default SysTick_Config function is excluded. In this case, the file device.h must contain a vendor specific implementation of this function.

## ◆ __VTOR_PRESENT

#define __VTOR_PRESENT

VTOR present or not.

See SCB_Type::VTOR