| CMSIS-Core (Cortex-M) CMSIS-Core support for Cortex-M processor-based devices |

Loading...
Searching...
No Matches
Macros
Define values
MPU Functions for Armv6-M/v7-M

Define values for MPU region setup. More...

## Macros
#define | ARM_MPU_ACCESS_xxx
| Values for MPU region access attributes (in RASR field)
#define | ARM_MPU_AP_xxx
| Values for MPU region access permissions (in RASR field)
#define | ARM_MPU_CACHEP_xxx
| Cache policy values for MPU region access attributes (in RASR field)
#define | ARM_MPU_REGION_SIZE_xxx
| Size values of a MPU region (in RASR field)

## Description

Define values for MPU region setup.

The following define values are used with ARM_MPU_RASR to setup the RASR value field in the MPU region.

See also
  ARM_MPU_Region_t, ARM_MPU_SetRegion, ARM_MPU_SetRegionEx.

## Macro Definition Documentation

## ◆ ARM_MPU_ACCESS_xxx

#define ARM_MPU_ACCESS_xxx

Values for MPU region access attributes (in RASR field)

The following define values are used to compose the access attributes for an MPU region:

#define | TEX | Shareable | Cacheable | Bufferable | Description
--- | --- | --- | --- | --- | ---
ARM_MPU_ACCESS_ORDERED | 000b | 1 | 0 | 0 | Strongly ordered memory
ARM_MPU_ACCESS_DEVICE(S) | 0s0b | S | 0 | S | Memory mapped peripheral device, shared (S=1) or non-shared (S=0)
ARM_MPU_ACCESS_NORMAL(O,I,S) | 1BBb | S | A | A | Normal memory, with outer/inner cache policy (O/I=ARM_MPU_CACHEP_xxx, shared (S=1) or non-share (S=0)

## ◆ ARM_MPU_AP_xxx

#define ARM_MPU_AP_xxx

Values for MPU region access permissions (in RASR field)

The following define values are used to compose the access permission for an MPU region:

#define | Value | Access permissions
--- | --- | ---
ARM_MPU_AP_NONE | 0x0U | None: any access generates a permission fault.
ARM_MPU_AP_PRIV | 0x1U | Privileged Read/Write: privileged access only; any unprivileged access generates a permission fault.
ARM_MPU_AP_URO | 0x2U | Privileged Read/Write; Unprivileged Read-only: any unprivileged write generates a permission fault.
ARM_MPU_AP_FULL | 0x3U | Privileged Read/Write. Unprivileged Read/Write: full access, permission faults are never generated.
ARM_MPU_AP_PRO | 0x5U | Privileged Read-only: any unprivileged access or privileged write generates a permission fault.
ARM_MPU_AP_RO | 0x6U | Privileged and Unprivileged Read-only: any write generates a permission fault.

## ◆ ARM_MPU_CACHEP_xxx

#define ARM_MPU_CACHEP_xxx

Cache policy values for MPU region access attributes (in RASR field)

The following define values are used to compose the cacheability flags within the access attributes for an MPU region:

#define | Value | Cacheability policy
--- | --- | ---
ARM_MPU_CACHEP_NOCACHE | 00b | Non-cacheable
ARM_MPU_CACHEP_WB_WRA | 01b | Write-back, write and read allocate
ARM_MPU_CACHEP_WT_NWA | 10b | Write-through, no write allocate
ARM_MPU_CACHEP_WB_NWA | 11b | Write-back, no write allocate

## ◆ ARM_MPU_REGION_SIZE_xxx

#define ARM_MPU_REGION_SIZE_xxx

Size values of a MPU region (in RASR field)

The following define values are used to compose the size information for an MPU region:

#define | Value | Description
--- | --- | ---
ARM_MPU_REGION_SIZE_32B | 0x04U | Region size 32 Bytes
ARM_MPU_REGION_SIZE_64B | 0x05U | Region size 64 Bytes
ARM_MPU_REGION_SIZE_128B | 0x06U | Region size 128 Bytes
ARM_MPU_REGION_SIZE_256B | 0x07U | Region size 256 Bytes
ARM_MPU_REGION_SIZE_512B | 0x08U | Region size 512 Bytes
ARM_MPU_REGION_SIZE_1KB | 0x09U | Region size 1 KByte
ARM_MPU_REGION_SIZE_2KB | 0x0AU | Region size 2 KBytes
ARM_MPU_REGION_SIZE_4KB | 0x0BU | Region size 4 KBytes
ARM_MPU_REGION_SIZE_8KB | 0x0CU | Region size 8 KBytes
ARM_MPU_REGION_SIZE_16KB | 0x0DU | Region size 16 KBytes
ARM_MPU_REGION_SIZE_32KB | 0x0EU | Region size 32 KBytes
ARM_MPU_REGION_SIZE_64KB | 0x0FU | Region size 64 KBytes
ARM_MPU_REGION_SIZE_128KB | 0x10U | Region size 128 KBytes
ARM_MPU_REGION_SIZE_256KB | 0x11U | Region size 256 KBytes
ARM_MPU_REGION_SIZE_512KB | 0x12U | Region size 512 KBytes
ARM_MPU_REGION_SIZE_1MB | 0x13U | Region size 1 MByte
ARM_MPU_REGION_SIZE_2MB | 0x14U | Region size 2 MBytes
ARM_MPU_REGION_SIZE_4MB | 0x15U | Region size 4 MBytes
ARM_MPU_REGION_SIZE_8MB | 0x16U | Region size 8 MBytes
ARM_MPU_REGION_SIZE_16MB | 0x17U | Region size 16 MBytes
ARM_MPU_REGION_SIZE_32MB | 0x18U | Region size 32 MBytes
ARM_MPU_REGION_SIZE_64MB | 0x19U | Region size 64 MBytes
ARM_MPU_REGION_SIZE_128MB | 0x1AU | Region size 128 MBytes
ARM_MPU_REGION_SIZE_256MB | 0x1BU | Region size 256 MBytes
ARM_MPU_REGION_SIZE_512MB | 0x1CU | Region size 512 MBytes
ARM_MPU_REGION_SIZE_1GB | 0x1DU | Region size 1 GByte
ARM_MPU_REGION_SIZE_2GB | 0x1EU | Region size 2 GBytes
ARM_MPU_REGION_SIZE_4GB | 0x1FU | Region size 4 GBytes