| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Macros
NAND Events
NAND Interface

The NAND driver generates call back events that are notified via the function ARM_NAND_SignalEvent. More...

## Macros
#define | ARM_NAND_EVENT_DEVICE_READY (1UL << 0)
| Device Ready: R/Bn rising edge.
#define | ARM_NAND_EVENT_DRIVER_READY (1UL << 1)
| Driver Ready.
#define | ARM_NAND_EVENT_DRIVER_DONE (1UL << 2)
| Driver operation done.

## Description

The NAND driver generates call back events that are notified via the function ARM_NAND_SignalEvent.

This section provides the event values for the ARM_NAND_SignalEvent callback function.

The following call back notification events are generated:

## Macro Definition Documentation

## ◆ ARM_NAND_EVENT_DEVICE_READY

#define ARM_NAND_EVENT_DEVICE_READY (1UL << 0)

Device Ready: R/Bn rising edge.

## ◆ ARM_NAND_EVENT_DRIVER_READY

#define ARM_NAND_EVENT_DRIVER_READY (1UL << 1)

Driver Ready.

## ◆ ARM_NAND_EVENT_DRIVER_DONE

#define ARM_NAND_EVENT_DRIVER_DONE (1UL << 2)

Driver operation done.