| CMSIS-Core (Cortex-A) CMSIS-Core support for Cortex-A processor-based devices |

Loading...
Searching...
No Matches
Macros
ref_core_ca.txt File Reference

## Macros
#define | _VAL2FLD(field, value)
| Mask and shift a bit field value for assigning the result to a peripheral register.
#define | _FLD2VAL(field, value)
| Extract from a peripheral register value the a bit field value.
#define | __CA_CMSIS_VERSION
| Contains the CMSIS version.
#define | __CA_CMSIS_VERSION_MAIN
| Contains the CMSIS major version.
#define | __CA_CMSIS_VERSION_SUB
| Contains the CMSIS minor version.
#define | __CA_REV 0x0000
| Contains the core revision for a Cortex-A class device.
#define | __CORTEX_A 0x0000
| Contains the core family for a Cortex-A class device.